ADAE* Adabas SAF Security (ADASAF) Messages

#### Search Results

Search

# ADAE* Adabas SAF Security (ADASAF) Messages

Note
Each of the messages in this section starts with the relevant database ID.

### Overview of Messages

`ADAE01 | ADAE02 | ADAE03 | ADAE04 | ADAE05 | ADAE06 | ADAE07 | ADAE08 | ADAE12 | ADAE15 | ADAE16 | ADAE17 | ADAE18`

ADAE01 | Unable to load required modules
Explanation | A required module could not be loaded. Operation terminates with an abend U0042.
Action | Check that the modules NA2PMAC and ESICFG are available.

ADAE02 | Unable to allocate required storage
Explanation | There is insufficient storage available for ADASAF to operate. Operation terminates with an abend U0042.
Action | Increase the amount of storage (above the 16-megabyte line) available to the failing job.

ADAE03 | Unable to allocate NRS storage
Explanation | ADASAF needs approximately two KB of storage below the 16-megabyte line. If the storage is not available at initialization (or after a newcopy operator command), ADASAF issues this message and operation terminates.
Action | Ensure that enough storage is available.

ADAE04 | Module module-name not loaded
Explanation | The indicated module could not be loaded during initialization or during the newcopy operator command. If the module is required (rather than optional), operation terminates.
Action | Ensure that the module is available.

ADAE05 | Invalid parameters detected
Explanation | One or more invalid parameters were specified in DDSAF. Operation terminates.
Action | Correct the invalid parameters.

ADAE06 | Allocation of user file cache failed
Explanation | ADASAF allocates a user file cache above the 16-megabyte line. If the storage is not available at initialization (or after a newcopy operator command), ADASAF issues this message and operation terminates.
Action | Ensure that enough storage is available or reduce the MAXFILES parameter (this may adversely affect performance).

ADAE07 | input-parameter
Explanation | ADASAF echoes the parameters read from DDSAF for information and auditing purposes.

ADAE08 | Invalid parameter: input-parameter
Explanation | ADASAF detected incorrect input in DDSAF. ADAE08 is issued for each invalid parameter found and is followed by ADAE05.
Action | Correct the invalid parameter.

ADAE12 | ADASAF is active in {FAIL|WARN} mode
Explanation | ADASAF has successfully initialized in the mode indicated.

ADAE15 | NEWCOPY of parameter module failed
Explanation | After a NEWCOPY operator command, ADASAF was unable to reload ESICFG. Operation terminates.
Action | This error occurs only if there is a shortage of storage or the module ESICFG was deleted from the load library after initialization. Determine which of these is the case and correct it.

ADAE16 | NEWCOPY reinitialization failed
Explanation | This message appears after a failure during NEWCOPY processing. It should be accompanied by a more detailed error message specifying the nature of the failure.
Action | Take the action recommended by the accompanying message.

ADAE17 | Not APF-authorized
Explanation | ADASAF must run APF-authorized. Operation terminates.
Action | Check that all STEPLIBs are in the APF list and that ADARUN is linked with AC(1).

ADAE18 | No security details for job job-name
Explanation | An Adabas command received from the named job had no security credentials attached to it. The command is rejected with response code 200 (ADARSP200), subcode 3.
Action | Ensure that the security exits are correctly installed in the Adabas SVC and that the source job has been configured correctly to support SAF security systems.