XTS* - Software AG Internal Transport Subsystem Messages

#### Search Results

Search

# XTS* - Software AG Internal Transport Subsystem Messages

The Software AG internal transport subsystem Messages and Codes documentation provides information for each warning and error message that you can encounter using the internal transport subsystem of Software AG products.

This documentation is organized as follows:

Warnings | Provides the message ID, message text, and a brief explanation for each warning message.
Errors | Provides the message ID, message text, and a brief explanation for each error message.
Generic TCP/IP Messages | Lists the message ID and message text for each generic TCP/IP error. For complete information on the TCP/IP error conditions, refer to your TCP/IP documentation.

Note
The internal component API returns warnings as positive values and errors as negative values.

## Warnings

### Overview of Messages

`XTS0000W | XTS0001W | XTS0003W | XTS0004W | XTS0005W | XTS0006W | XTS0007W | XTS0008W | XTS0009W | XTS0010W | XTS0011W | XTS0012W | XTS0013W | XTS0014W | XTS0015W`

XTS0000W | XTS Success
Explanation | The transport subsystem processing completed successfully.

XTS0001W | XTS No LISTEN has been issued
Explanation | A server has only XTSconnect entries and no XTSlisten. It is possible for a server to connect only to a proxy, and the warning helps applications determine if XTSlisten is missing.

XTS0003W | XTS Load message file failed
Explanation | The transport subsystem failed to load the XTS.MSG file. This file contains text for the error messages; there is an internal table also, so XTS.MSG is not mandatory.

XTS0004W | XTS Client already registered
Explanation | Multiple `XtsBindClient` calls occurred for the same client. Only the first call is considered.

XTS0005W | XTS More data
Explanation | The receive buffer defined by a transport subsystem send and wait call is not big enough to get all data received by the transport subsystem. A subsequent call has to be made to receive all data.

XTS0006W | XTS No SSL random file warning
Explanation | There is no random file defined for a transport subsystem/Secure Sockets Layer (SSL) application; a random file usage by SSL is highly recommended.

XTS0007W | XTS Notify connect
Explanation | This is a receive callback notification for an incoming connection.

XTS0008W | XTS Notify disconnect
Explanation | This is a receive callback notification for a disconnection.

XTS0009W | XTS Notify broadcast
Explanation | This is a receive callback notification for a broadcast attempt.

XTS0010W | XTS Notify unsupported
Explanation | This is a receive callback notification when protocols set by XTSlisten are not supported.

XTS0011W | XTS Notify message reference dead
Explanation | This is a receive callback notification indicating the active message references are deleted when a client disconnects.

XTS0012W | XTS Notify outbound connect
Explanation | This is a receive callback notification for an outbound connection.

XTS0013W | XTS Notify listen failure
Explanation | This is a notification to the callback routine submitted by XtsRegisterByTargetName or XtsRegisterByTargetId indicating a failure of an XTSlisten URL.

XTS0014W | XTS Notify connect failure
Explanation | This is a notification to the callback routine submitted by XtsRegisterByTargetName or XtsRegisterByTargetId indicating a failure of an XTSconnect URL.

XTS0015W | XTS Notify end broadcast
Explanation | This is a notification to the callback routine submitted by XtsRegisterByTargetName or XtsRegisterByTargetId indicating an end broadcast message was received from another node.

## Errors

### Overview of Messages

`XTS0050E | XTS0051E | XTS0052E | XTS0053E | XTS0054E | XTS0055E | XTS0056E | XTS0057E | XTS0058E | XTS0059E | XTS0060E | XTS0061E | XTS0062E | XTS0063E | XTS0064E | XTS0065E | XTS0066E | XTS0069E | XTS0070E | XTS0071E | XTS0072E | XTS0073E | XTS0074E | XTS0075E | XTS0077E | XTS0078E | XTS0079E | XTS0082E | XTS0083E | XTS0084E | XTS0085E | XTS0086E | XTS0087E | XTS0088E | XTS0089E | XTS0090E | XTS0094E | XTS0095E | XTS0096E | XTS0097E | XTS0098E | XTS0100E | XTS0101E | XTS0102E | XTS0103E | XTS0104E | XTS0105E | XTS0106E | XTS0107E | XTS0108E | XTS0109E | XTS0110E | XTS0111E | XTS0112E | XTS0113E | XTS0114E | XTS0115E | XTS0116E | XTS0117E | XTS0118E | XTS0119E | XTS0120E | XTS0121E | XTS0122E | XTS0123E | XTS0124E | XTS0126E | XTS0127E | XTS0128E | XTS0129E | XTS0130E | XTS0131E | XTS0132E | XTS0150E | XTS0151E | XTS0152E | XTS0153E | XTS0154E | XTS0155E | XTS0156E | XTS0157E | XTS0158E | XTS0159E | XTS0163E | XTS0167E | XTS0168E | XTS0169E | XTS0170E | XTS0171E | XTS0172E | XTS0173E | XTS0174E | XTS0200E | XTS0201E | XTS0203E | XTS0204E | XTS0205E | XTS0206E | XTS0207E | XTS0208E | XTS0209E | XTS0210E | XTS0211E | XTS0212E | XTS0213E | XTS0214E | XTS0215E | XTS0216E | XTS0217E | XTS0218E | XTS0219E | XTS0220E | XTS0221E | XTS0222E | XTS0223E | XTS0224E | XTS0225E | XTS0226E | XTS0227E | XTS0228E | XTS0229E | XTS0230E | XTS0231E | XTS1000E`

XTS0050E | XTS Semaphore Error
Explanation | A failure to create a semaphore occurred. Contact Software AG customer support.

XTS0051E | XTS Memory Allocation Error
Explanation | A failure to allocate memory occurred. Contact Software AG customer support.

XTS0052E | XTS Server already registered
Explanation | The transport subsystem server is already registered.

XTS0053E | XTS Incorrect URL
Explanation | A URL with a syntax error was encountered. Check the Directory Server repositories.

XTS0054E | XTS Failure Loading Protocol Handler
Explanation | A failure to load protocol handlers (for example, Xtstcp.lib) occurred. It was probably caused by a configuration problem. Contact Software AG customer support.

XTS0055E | XTS Protocol Init failed
Explanation | A protocol initialization failure occurred. Contact Software AG customer support.

XTS0056E | XTS Invalid protocol type
Explanation | The specified protocol is not supported by the transport subsystem. This is possibly and error in URL syntax.

XTS0057E | XTS Listen Failed
Explanation | A listen failed. Check the log file for protocol-specific errors. This is caused mostly by trying to listen on a port taken by another server.

XTS0058E | XTS Accept Failed
Explanation | The accept failed. Check the log file for protocol-specific errors.

XTS0059E | XTS Connect Failed
Explanation | The connect failed. Check the log file for protocol-specific errors.

XTS0060E | XTS No directory information
Explanation | No XTSaccess information is provided for the server to which the application wants to connect. Please add a target definition through the Directory Server.

XTS0061E | XTS Failure to create a thread
Explanation | A failure to create a thread occurred. Contact Software AG customer support

XTS0062E | XTS Timeout error
Explanation | A failure to connect or send data in the time set by the user occurred. To complete the connect or send, repeat the call or increase the timeout value.

XTS0063E | XTS Send Failed
Explanation | A completion code is returned to the send callback routine when send fails. Check the log file for the protocol-specific error code.

XTS0064E | XTS Invalid reference
Explanation | An invalid message reference was passed by the user.

XTS0065E | XTS Send incomplete
Explanation | A send was interrupted by a client disconnection.

XTS0066E | XTS No such server
Explanation | A nonexistent server name was passed by the user. It applies to the transport subsystem statistics and dumps calls.

XTS0069E | XTS Resolve Target failed
Explanation | The client failed to send a handshake message to the server; Error caused by the server going down or a protocol send error.

XTS0070E | XTS Resolve Target Reply failed
Explanation | The server failed to reply to the client during handshaking. This error is caused by the client going down or by a protocol send error.

XTS0071E | XTS Target cannot be resolved
Explanation | The client failed to resolve the target name. This error is caused by different names used by the server and the client but with the same address.

XTS0072E | XTS Not initialized
Explanation | The transport subsystem call was submitted before the transport subsystem was initialized. Errors were returned by XtsShutdown, XtsSendMessageByRT, and the transport subsystem statistics call.

XTS0073E | XTS Bind Client failed
Explanation | The client bind failed because of a protocol send error or because the server went down.

XTS0074E | XTS Too many user threads
Explanation | The number of user threads in existence reached the maximum (64). Stop creating new user threads or reduce their time to live (timeout).

XTS0075E | XTS Created thread failed
Explanation | The transport subsystem failed to create a new user thread. This is an SMP error, possibly because of the limitations of the number of threads that a system can support. Contact Software AG customer support.

XTS0077E | XTS Conversion failed
Explanation | The conversion between wide character and MBNS failed. Contact Software AG customer support.

XTS0078E | XTS No Target Name
Explanation | The target name is a zero pointer. Pass a valid string.

XTS0079E | XTS No Client Name
Explanation | The client name is a zero pointer. Pass a valid string.

XTS0082E | XTS Zero Length not accepted
Explanation | The length of the data to be sent is zero, Make the length a positive number.

XTS0083E | XTS Target ID Out of Range
Explanation | The target ID value is bigger than "2113929215".

XTS0084E | XTS Channel Inactive
Explanation | The server-client connection was no longer active when XtsSendByRt or XtsBindClient were called. This error is generated by a client going down during the call.

XTS0085E | XTS Disconnect message
Explanation | A client or server disconnection was detected during a transport subsystem call.

XTS0086E | XTS Hash table error
Explanation | An internal transport subsystem hash table error occurred. Contact Software AG customer support.

XTS0087E | XTS Thread key error
Explanation | An allocate/delete thread memory failure occurred. Contact Software AG customer support.

XTS0088E | XTS No CONNECT or LISTEN has been issued
Explanation | A server registration failed to submit at least one listen or connect. Check the XTSlisten or XTSconnect URL parameters.

XTS0089E | XTS Protocol not supported
Explanation | An attempt was made to use XtsBindClient over the RAW or XTSDS protocol. This feature is not supported.

XTS0090E | XTS Single Thread not supported
Explanation | This error code is returned when the transport subsystem call does not support the single thread feature. Examples include `XtsRegisterServerByName`(ID) and `XtsGiveThread`.

XTS0094E | XTS Zero pointer
Explanation | A zero pointer was passed by the user. This is an invalid value.

XTS0095E | XTS Hash table full
Explanation | An internal transport subsystem hash table error occurred. Contact Software AG customer support.

XTS0096E | XTS Send User Exit failed
Explanation | The user exit send routine failed. Check the user exit code.

XTS0097E | XTS Recv User Exit failed
Explanation | The user exit receive routine failed. Check the user exit code.

XTS0098E | XTS Load User Exit failed
Explanation | The transport subsystem failed to load the user exit library. Check the environment or the user exit routine names.

XTS0100E | XTS Shutdown in process
Explanation | This error code is returned when the transport subsystem is in shutdown mode (because XtsShutdown was called by another thread).

XTS0101E | XTS Route Timeout
Explanation | The proxy cannot deliver the message because the route timeout was insufficient. Change the route timeout.

XTS0102E | XTS Route Table overflow
Explanation | The proxy cannot deliver the message because of a route table overflow. Repeat the transport subsystem call.

XTS0103E | XTS Route TTL expired
Explanation | The proxy cannot deliver the message because the route time to live was insufficient. Change the time to live time.

XTS0104E | XTS Route failed
Explanation | The proxy cannot deliver the message because of a route failure. Repeat the transport subsystem call.

XTS0105E | XTS Null parameter
Explanation | A null parameter is encountered when a notify callback routine registration is called.

XTS0106E | XTS Connection Rejected
Explanation | The connection was rejected by the notify callback routine.

XTS0107E | XTS Replica redirected
Explanation | The connection was redirected by the callback routine.

XTS0108E | XTS timeout - connect in progress
Explanation | A timeout error occurred, but connection is in progress. Submit the call again or increase the timeout value.

XTS0109E | XTS invalid session
Explanation | An invalid session handle was used by the transport subsystem session calls.

XTS0110E | XTS invalid key
Explanation | An invalid session handle was used by the transport subsystem session calls.

XTS0111E | XTS Count converters failed
Explanation | The count of available converter names failed.

XTS0112E | XTS Convert enum failed
Explanation | The enumeration of text converter names failed.

XTS0113E | XTS Buffer too small
Explanation | The text conversion buffer is not big enough..

XTS0114E | XTS No more ports available
Explanation | No replicated server ports are available .

XTS0115E | XTS Text converter library load failed
Explanation | The load of the transport subsystem converter ending failed.

XTS0116E | XTS Text converter resolve failed
Explanation | The text converter interface function could not be resolved.

XTS0117E | XTS Name to EDDkey map failed
Explanation | The ICU converter name to Software AG ECS EDD key conversion failed..

XTS0118E | XTS XDS library loading failed
Explanation | The XDS library used by ADVDIR could not be loaded.

XTS0119E | XTS DS access time out error
Explanation | A timeout occurred accessing the Directory Server (the default timeout is one minute).

XTS0120E | XTS Failed to set ECS environment
Explanation | A failure occurred when setting the ECS environment.

XTS0121E | XTS Set UDP Port failed
Explanation | The UDP port selected by user cannot be used (because it is used by another application).

XTS0122E | XTS Sync and async send in raw mode not allowed
Explanation | Using synchronous and asynchronous calls on the same channel is not allowed.

XTS0123E | XTS Unknown received buffer
Explanation | The transport subsystem received an unknown buffer from an application.

XTS0124E | XTS Function retired
Explanation | The transport subsystem function is not supported any longer.

XTS0126E | XTS invalid duplicate server
Explanation | This error is generated when the same server is registered again with a different protocol than the one used when it was first registered.

XTS0127E | XTS Fatal error
Explanation | An internal error occurred, indicating a severe transport subsystem code problem. Contact Software AG customer support.

XTS0128E | XTS Load library failed
Explanation | The transport subsystem failed to load a library (the log file indicates which one).

XTS0129E | XTS Key not found
Explanation | The key used to retrieve transport subsystem parameters does not exist.

XTS0130E | XTS Xts.Config Key not found
Explanation | The key used by the user to retrieve transport subsystem parameters from xts.config file does not exist.

XTS0131E | XTS No directory information for XTS profile
Explanation | The profile is not defined in the Directory Server.

XTS0132E | XTS Load function failed
Explanation | A failure occurred loading a function (the name of the function and the name of the library are in the log file).

XTS0150E | XTS SSL init failed
Explanation | The transport subsystem failed to initialize the Secure Sockets Layer (SSL) library. Check the log file for the SSL error messages.

XTS0151E | XTS SSL Verify CA locations failed
Explanation | The Secure Sockets Layer (SSL) failed to load the CA certificates. Probable causes include an invalid path specification or nonexistent CA certificates.

XTS0152E | XTS SSL Certificate file not specified
Explanation | No Secure Sockets Layer (SSL) certificate was specified.

XTS0153E | XTS SSL Invalid Certificate
Explanation | The URL-specified Secure Sockets Layer (SSL) certificate has an invalid format.

XTS0154E | XTS SSL Invalid Key File
Explanation | The URL-specified Secure Sockets Layer (SSL) key file has an invalid format.

XTS0155E | XTS SSL Invalid Key
Explanation | The Secure Sockets Layer (SSL) key specified by the user is invalid.

XTS0156E | XTS SSL Connect failed
Explanation | A Secure Sockets Layer (SSL) connect failed (caused by an SSL handshaking error). Check the log file for the Secure Sockets Layer (SSL) error messages.

XTS0157E | XTS SSL Accept failed
Explanation | A Secure Sockets Layer (SSL) accept failed (caused by an SSL handshaking error). Check the log file for the SSL error messages.

XTS0158E | XTS SSL Read failed
Explanation | A Secure Sockets Layer (SSL) read failed. Check the log file for the SSL error messages.

XTS0159E | XTS SSL Write failed
Explanation | A Secure Sockets Layer (SSL) write failed. Check the log file for the SSL error messages.

XTS0163E | XTS SSL Failed loading library
Explanation | A failure to load the Secure Sockets Layer (SSL) library occurred. Check the environment.

XTS0167E | XTS SSL Illegal host name
Explanation | The peer certificate subject name and host name are different, indicating an illegal connection.

XTS0168E | XTS SSL No local certificate
Explanation | There is no local Secure Sockets Layer (SSL) certificate.

XTS0169E | XTS SSL No remote certificate
Explanation | There is no local Secure Sockets Layer (SSL) certificate.

XTS0170E | XTS SSL insufficient user memory
Explanation | There is insufficient user memory for returning the requested data.

XTS0171E | XTS SSL certificate rejected
Explanation | The certificate was rejected during verification.

XTS0172E | XTS SSL zero length message return
Explanation | The Secure Sockets Layer (SSL) write or read routines returned an invalid zero value. Contact Software AG customer support.

XTS0173E | XTS SSL want read error
Explanation | The Secure Sockets Layer (SSL) write routine returned want read error code. Contact Software AG customer support. This is a transport subsystem internal sequence error.

XTS0174E | XTS SSL want write error
Explanation | The Secure Sockets Layer (SSL) read routine returned want write error code. Contact Software AG customer support. This is a transport subsystem internal sequence error.

XTS0200E | DS Open File failed
Explanation | A failure to open a file occurred. Check if the file exists and that the path is correct.

XTS0201E | DS Incomplete Entry
Explanation | A URL syntax error occurred. Check the log file for detailed information.

XTS0203E | DS Service not provided
Explanation | An invalid Directory Service selection was made.

XTS0204E | DS Null parameter
Explanation | A Directory Service call was encountered with a null parameter.

XTS0205E | DS Incomplete Entry
Explanation | An attempt to add an incomplete URL record was made.

XTS0206E | DS Topic Not Defined
Explanation | The user tried to use a qualifier unknown to the Directory Server.

XTS0207E | DS Unknown request
Explanation | An unknown XTSDS request was encountered. Check the syntax of the Directory Server call.

XTS0208E | DS No Entries
Explanation | The Directory Server or configuration file contains no entries for the specified target.

XTS0209E | DS Delete Failed
Explanation | A Directory Service delete call failed. Check the log file for detailed information.

XTS0210E | DS Connection Failed
Explanation | Connection to the Directory Server failed.

XTS0211E | DS Bind Failed
Explanation | Deprecated message.

XTS0212E | DS Search Failed
Explanation | Retrieve URL command failed.

XTS0213E | DS Add Failed
Explanation | Addition of a new URL failed.

XTS0214E | DS Already Exists
Explanation | An attempt was made to add a record that already exists.

XTS0215E | DS Failure Loading Service Handler
Explanation | A failure occurred loading a directory service. Check the environment. Contact Software AG customer support.

XTS0216E | DS Wrong directory parameter
Explanation | Unknown directory parameter.

XTS0217E | DS not Initialized
Explanation | Directory Server was not initialized before usage.

XTS0218E | DS Invalid target Name
Explanation | The target name contains one of the following characters: "#", ".", "[", "]", "=", "\", "\", or "*". The target name is invalid.

XTS0219E | DS Incomplete request
Explanation | An incomplete XTSDS request was caused by a zero value of the target, qualifier, or user data.

XTS0220E | DS No URL entries
Explanation | The XTSDS server does not have any URL to return for the retrieve call.

XTS0221E | DS XDS error
Explanation | An XDS processing error occurred..

XTS0222E | DS Rollback is not implemented
Explanation | No Directory Service rollback was performed..

XTS0223E | DS OVO error
Explanation | An OVO error occurred during Directory Service processing.

XTS0224E | DS One time set violation
Explanation | A one-time setting function was called multiple times. A programs encoding mode cannot change once it is set.

XTS0225E | DS Encoding conflict
Explanation | The INIDIR file encoding conflicts with programs encoding.

XTS0226E | DS Create file failed
Explanation | The file creation failed during Directory Service processing..

XTS0227E | DS IO file failed
Explanation | A file I/O error occurred during Directory Service processing.

XTS0228E | DS Wrong file format`
Explanation | The INIDIR file format was not recognized.

XTS0229E | DS Send buffer bigger than maximum allowed
Explanation | An internal transport subsystem error occurred, generated when a URL is added or deleted from the Directory Server and its size exceeds 65520 bytes.

XTS0230E | DS Invalid Service
Explanation | Invalid type of service used.

XTS0231E | DS Invalid Header
Explanation | Invalid Directory Service header used for communication.

XTS1000E | XTS Unknown error = code
Explanation | This message is returned by XtsGetMessage when it cannot find text for a given error code.

## Generic TCP/IP Messages

### Overview of Messages

`XTS1001E | XTS1002E | XTS1003E | XTS1004E | XTS1005E | XTS1006E | XTS1007E | XTS1008E | XTS1009E | XTS1010E | XTS1011E | XTS1012E | XTS1013E | XTS1014E | XTS1015E | XTS1016E | XTS1017E | XTS1018E | XTS1019E | XTS1020E | XTS1021E | XTS1022E | XTS1023E | XTS1024E | XTS1025E | XTS1026E | XTS1027E | XTS1028E | XTS1029E | XTS1030E | XTS1031E | XTS1032E | XTS1033E | XTS1034E | XTS1035E | XTS1036E | XTS1037E | XTS1038E | XTS1039E | XTS1040E | XTS1041E | XTS1042E | XTS1043E | XTS1044E | XTS1045E | XTS1046E | XTS1047E | XTS1048E | XTS1049E | XTS1050E | XTS1051E | XTS1052E | XTS1053E | XTS1054E | XTS1055E | XTS1056E | XTS1057E | XTS1058E | XTS1059E | XTS1060E | XTS1061E | XTS1062E | XTS1063E | XTS1064E | XTS1065E | XTS1066E | XTS1067E | XTS1068E | XTS1069E | XTS1070E | XTS1071E | XTS1072E | XTS1073E | XTS1074E | XTS1075E | XTS1076E | XTS1077E | XTS1078E | XTS1079E | XTS1080E | XTS1081E | XTS1082E | XTS1083E | XTS1084E | XTS1085E | XTS1086E | XTS1087E | XTS1088E | XTS1089E | XTS1090E | XTS1091E | XTS1092E | XTS1093E | XTS1094E | XTS1095E | XTS1096E | XTS1097E | XTS1098E | XTS1099E | XTS1100E | XTS1101E | XTS1102E | XTS1103E | XTS1104E | XTS1105E | XTS1106E | XTS1107E | XTS1108E | XTS1109E | XTS1111E | XTS1112E | XTS1113E | XTS1114E | XTS1115E | XTS1116E | XTS1118E | XTS1119E | XTS1120E | XTS1122E | XTS1123E | XTS1124E | XTS1125E | XTS1126E | XTS1127E | XTS1128E | XTS1129E | XTS1130E | XTS1131E | XTS1132E | XTS1133E | XTS1134E | XTS1135E | XTS1136E | XTS1137E | XTS1138E | XTS1139E | XTS1140E | XTS1141E | XTS1142E | XTS1143E | XTS1144E | XTS1145E | XTS1146E | XTS1147E | XTS1148E | XTS1149E | XTS1150E | XTS1151E | XTS1152E | XTS1153E | XTS1154E | XTS1155E | XTS1156E | XTS1157E | XTS1158E | XTS1159E | XTS1160E | XTS1161E | XTS1162E | XTS1163E | XTS1164E | XTS1165E | XTS1166E | XTS1167E | XTS1168E | XTS1169E`

XTS1001E | TCP/IP Operation not permitted

XTS1002E | TCP/IP No such file or directory

XTS1003E | TCP/IP No such process

XTS1004E | TCP/IP Interrupted function call

XTS1005E | TCP/IP I/O error

XTS1006E | TCP/IP No such device or address

XTS1007E | TCP/IP Arg list too long

XTS1008E | TCP/IP Exec format error

XTS1009E | TCP/IP Bad file number

XTS1010E | TCP/IP No children

XTS1011E | TCP/IP Operation would cause deadlock

XTS1012E | TCP/IP Not enough core

XTS1013E | TCP/IP Permission denied

XTS1014E | TCP/IP Bad address

XTS1015E | TCP/IP Block device required

XTS1016E | TCP/IP Mount device busy

XTS1017E | TCP/IP File exists

XTS1018E | TCP/IP Cross-device link

XTS1019E | TCP/IP No such device

XTS1020E | TCP/IP Not a directory

XTS1021E | TCP/IP Is a directory

XTS1022E | TCP/IP Invalid argument

XTS1023E | TCP/IP File table overflow

XTS1024E | TCP/IP Too many open sockets

XTS1025E | TCP/IP Inappropriate ioctl for device

XTS1026E | TCP/IP Text file busy

XTS1027E | TCP/IP File too large

XTS1028E | TCP/IP No space left on device

XTS1029E | TCP/IP Illegal seek

XTS1030E | TCP/IP Read-only file system

XTS1031E | TCP/IP Too many links

XTS1032E | TCP/IP Broken pipe

XTS1033E | TCP/IP Argument too large

XTS1034E | TCP/IP Result too large

XTS1035E | TCP/IP Resource temporarily unavailable

XTS1036E | TCP/IP Operation now in progress

XTS1037E | TCP/IP Operation already in progress

XTS1038E | TCP/IP Socket operation on non-socket

XTS1039E | TCP/IP Destination address required

XTS1040E | TCP/IP Message too long

XTS1041E | TCP/IP Protocol wrong type for socket

XTS1042E | TCP/IP Bad protocol option

XTS1043E | TCP/IP Protocol not supported

XTS1044E | TCP/IP Socket type not supported

XTS1045E | TCP/IP Operation not supported

XTS1046E | TCP/IP Protocol Family not supported

XTS1047E | TCP/IP Address family not supported by protocol family

XTS1048E | TCP/IP Address already in use

XTS1049E | TCP/IP Cannot assign requested address

XTS1050E | TCP/IP Network is down

XTS1051E | TCP/IP Network is unreachable

XTS1052E | TCP/IP Network dropped connection on reset

XTS1053E | TCP/IP Software caused connection abort

XTS1054E | TCP/IP Connection reset by peer

XTS1055E | TCP/IP No buffer space available

XTS1056E | TCP/IP Socket is already connected

XTS1057E | TCP/IP Socket is not connected

XTS1058E | TCP/IP Cannot send after socket shutdown

XTS1059E | TCP/IP Too many references

XTS1060E | TCP/IP Connection timed out

XTS1061E | TCP/IP Connection refused

XTS1062E | TCP/IP Too many levels of symbolic links

XTS1063E | TCP/IP File name too long

XTS1064E | TCP/IP Host is down

XTS1065E | TCP/IP No route to host

XTS1066E | TCP/IP Directory not empty

XTS1067E | TCP/IP Too many processes

XTS1068E | TCP/IP Too many users

XTS1069E | TCP/IP Disc quota exceeded

XTS1070E | TCP/IP Stale NFS file handle

XTS1071E | TCP/IP Too many levels of remote in path

XTS1072E | TCP/IP Device not ready

XTS1073E | TCP/IP Write-protected media

XTS1074E | TCP/IP Unformatted media

XTS1075E | TCP/IP No connection

XTS1076E | TCP/IP Old, currently unused AIX errno

XTS1077E | TCP/IP Restart the system call

XTS1078E | TCP/IP Invalid file system control data

XTS1079E | TCP/IP Media surface error

XTS1080E | TCP/IP I/O completed, but needs relocation

XTS1081E | TCP/IP No attribute found

XTS1082E | TCP/IP Out of STREAM resources

XTS1083E | TCP/IP System call timed out

XTS1084E | TCP/IP Next message has wrong type

XTS1085E | TCP/IP Protocol error

XTS1086E | TCP/IP No message on stream read queue

XTS1087E | TCP/IP fd not associated with a stream

XTS1088E | TCP/IP Security authentication denied

XTS1089E | TCP/IP Not a trusted program

XTS1090E | TCP/IP Illegal byte sequence

XTS1091E | TCP/IP Network subsystem is unavailable

XTS1092E | TCP/IP WINSOCK.DLL version out of range

XTS1093E | TCP/IP Successful WSAStartup not yet performed

XTS1094E | TCP/IP Cross mount point (not really error)

XTS1095E | TCP/IP cannot start operation

XTS1096E | TCP/IP Cannot access a needed shared library

XTS1097E | TCP/IP operation (now) in progress

XTS1098E | TCP/IP Lib section in a.out corrupted

XTS1099E | TCP/IP Attempting to link in too many shared libraries

XTS1100E | TCP/IP Cannot exec a shared library directly

XTS1101E | TCP/IP Graceful shutdown in progress

XTS1102E | TCP/IP Streams pipe error

XTS1103E | TCP/IP Structure needs cleaning

XTS1104E | TCP/IP Not a XENIX named tip file

XTS1105E | TCP/IP No XENIX semaphores available

XTS1106E | TCP/IP Is a named type file

XTS1107E | TCP/IP Remote I/O error

XTS1108E | TCP/IP No medium found

XTS1109E | TCP/IP Wrong medium type

XTS1111E | TCP/IP Host not found

XTS1112E | TCP/IP Non-authoritative host not found

XTS1113E | TCP/IP This is a non-recoverable error

XTS1114E | TCP/IP Valid name, no data record of requested type

XTS1115E | TCP/IP Resource unavailable

XTS1116E | TCP/IP Operation canceled

XTS1118E | TCP/IP Disc quota exceeded

XTS1119E | TCP/IP Identifier removed

XTS1120E | TCP/IP Too many open files

XTS1122E | TCP/IP Multihop attempted

XTS1123E | TCP/IP No locks available

XTS1124E | TCP/IP The link has been severed

XTS1125E | TCP/IP No message of the desired type

XTS1126E | TCP/IP Function not supported

XTS1127E | TCP/IP Directory not empty

XTS1128E | TCP/IP Operation not supported

XTS1129E | TCP/IP Value too large to be stored in data

XTS1130E | TCP/IP Stale NFS file handle

XTS1131E | TCP/IP There is no more data available

XTS1132E | TCP/IP The call has been canceled

XTS1133E | TCP/IP Invalid procedure table from service provider

XTS1134E | TCP/IP Invalid service provider version number

XTS1135E | TCP/IP Unable to initialize a service provider

XTS1136E | TCP/IP System call failure

XTS1137E | TCP/IP Service not found

XTS1138E | TCP/IP Type not found

XTS1139E | TCP/IP There is no more data available

XTS1140E | TCP/IP The call has been canceled

XTS1141E | TCP/IP Refused

XTS1142E | TCP/IP Cbannel number out of range

XTS1143E | TCP/IP Level 2 not synchronized

XTS1144E | TCP/IP Level 3 halted

XTS1145E | TCP/IP Level 3 reset

XTS1146E | TCP/IP Link number out of range

XTS1147E | TCP/IP Protocol driver not attached

XTS1148E | TCP/IP No 43 CSI structure available

XTS1149E | TCP/IP Level 2 halted

XTS1150E | TCP/IP Invalid exchange

XTS1151E | TCP/IP Invalid request descriptor

XTS1152E | TCP/IP Exchange full

XTS1153E | TCP/IP No anode

XTS1154E | TCP/IP Invalid request code

XTS1155E | TCP/IP Invalid slot

XTS1156E | TCP/IP File locking deadlock error

XTS1157E | TCP/IP Bad fon file fmt

XTS1158E | TCP/IP Process died with the lock

XTS1159E | TCP/IP Lock is not recoverable

XTS1160E | TCP/IP Machine is not on the network

XTS1161E | TCP/IP Package not installed

XTS1162E | TCP/IP The object is remote

XTS1163E | TCP/IP Advertise error

XTS1164E | TCP/IP Mount error

XTS1165E | TCP/IP Communication error on send

XTS1166E | TCP/IP Locked lock was unmapped

XTS1167E | TCP/IP Name not unique on network

XTS1168E | TCP/IP FD invalid for this operation

XTS1169E | TCP/IP Remote address changed