PL6* - PRILOG6 Print Program Messages

#### Search Results

Search

# PL6* - PRILOG6 Print Program Messages

The following message groups are described:

- Messages from the Independent Components

- Messages from the System-Dependent Component

## Messages from the Independent Components

### Overview of Messages

`PL6000I | PL6001E | PL6002E | PL6003W | PL6004E | PL610I | PL611E`

PL6000I | Card read =>control-card
Explanation | The PRILOG6 input control card that was read is displayed in the message
Action | No action is required for this informational message.

PL6001E | Unrecognized input card
Explanation | One of the control cards read was not recognized by PRILOG6.
Action | Ensure that all cards either being with PRILOG6 or an asterisk (*) for a comment line.

PL6002E | Invalid parm: parameter
Explanation | The specified input parameter or value in the PRILOG6 control cards is invalid.
Action | Correct the identified parameter and rerun the program.

PL6003W | CLOGLAYOUT is x
Explanation | This informs the user as to the CLOGLAYOUT being processed. x is the CLOGLAYOUT type (usually 8, older CLOGs maybe 5).
Action | This is an information message.

PL6004E | VERBOSE parameter requires another qualifier
Explanation | The PRILOG FIELDS VERBOSE parameter requires a qualifier. This error occurs when the parameter `FIELDS=(VERBOSE)` is input, when the specification should be, for example, `FIELDS=(LIST,VERBOSE)`.
Action | Correct the identified parameter and rerun the program.

PL610I | nnnnnnnn records skipped because CLOG created with LOGCB=NO
Explanation | This message list the number of CLOG records (nnnnnnnn) that have been skipped because they do not contain ACB/ACBX data as defined by the ADARUN parameter LOGCB=NO.
Action | No action is required for this informational message.

PL611E | no records read from DDCLOGIN
Explanation | The file linked to DDCLOGIN is either empty or is of the wrong type. This may be accompanied by PL6D02 or PL6D03 messages.
Action | Check the JCL link statement DDCLOGIN and the file linked to it. Correct and rerun the job.

## Messages from the System-Dependent Component

### Overview of Messages

`PL6D01 | PL6D02 | PL6D03`

PL6D01 | DDCARD file failed to open, using defaults
Explanation | The input card file could not be opened.
Action | If the defaults are used, there are no input cards and this file is not required. The message can be ignored. The default values are CLOGLAYOUT=5 and FIELDS=(LIST). If values other than the defaults are required, ensure that the file is available and rerun the job.

PL6D02 | DDCLOGIN file failed to open - no reports
Explanation | The file containing the CLOG records did not open. No reports are printed.
Action | Ensure that the file is properly allocated and rerun the job.

PL6D03 | DDCLOGIN must be DSORG PS/VB - no Reports
Explanation | The file containing the CLOG records was of the wrong type and not opened. The file on the DDCLOGIN link name should be sequential (DSORG PS) and variable-blocked (RECFM=VB). No reports are printed.
Action | Check the attributes of the file on the DDCLOGIN link name. Reallocate and rerun the job.