ADACM* - ADATCP Messages

#### Search Results

Search

# ADACM* - ADATCP Messages

### Overview of Messages

`ADACM007E | ADACM008E | ADACM009E | ADACM010E | ADACM011I | ADACM012E | ADACM013E | ADACM014E | ADACM015E | ADACM016E | ADACM017I | ADACM018E | ADACM019E | ADACM020E | ADACM021E | ADACM022E | ADACM023E | ADACM024E | ADACM025E | ADACM026E | ADACM027E | ADACM028E | ADACM029E | ADACM030E | ADACM031E | ADACM032E | ADACM034E | ADACM035E | ADACM036E | ADACM037E | ADACM038E | ADACM039E`

ADACM007E | PARM ERROR
Explanation | One of the parameters passed within the URL was incorrect.
Action | Ensure that the URL includes valid values for all required elements: the API name (protocol), stack ID, and port number. Correct the URL and try again.

ADACM008E | INVALID VALUE IN PORT= PARAMETER
Explanation | The port that was specified in the URL was not valid.
Action | The port number can be 1-5 bytes; it cannot be zero (0) or greater than 65535.

ADACM009E | URL=url ALREADY {ACTIVE | CLOSED}
Explanation | Either the URL is already opened (ACTIVE) or already closed (CLOSED).
Action | Ensure that the URL includes valid values for all required elements: the API name (protocol), stack ID, and port number. Correct the URL and try again.

ADACM010E | URL=url NOT FOUND
Explanation | The URL itself was not found.
Action | Ensure that the URL includes valid values for all required elements: the API name (protocol), stack ID, and port number. Correct the URL and try again.

ADACM011I | URL=url HAS BEEN {CLOSED | OPENED}
Explanation | Either the URL was successfully closed or opened.
Action | None. This message is for information only.

ADACM012E | THE NETWORK IS DOWN
Explanation | ADATCP cannot be started because the network is not active.
Action | Check that the stack specified in the URL is active. If it is, contact your systems administrator.

ADACM013E | NO BUFFER SPACE IS AVAILABLE
Explanation | No buffer space is available to ADATCP to allocate its control blocks.
Action | Ensure that sufficient storage is available on the system.

ADACM014E | THE LINK HAS BEEN SEVERED
Explanation | An error caused TCP/IP or ADATCP to terminate.
Action | This message is issued along with another message that explains the reason for the termination. Refer to the other message.

ADACM015E | TCP/IP IS NOT INSTALLED OR ACTIVE
Explanation | The TCP/IP stack specified in the URL is not installed or not active.
Action | Check that the specified URL is the one intended. If so, either install the specified stack or start it.

ADACM016E | THE SOCKET DESCRIPTOR TABLE IS FULL
Explanation | The maximum number of socket descriptors has been reached: no more sockets can be created.
Action | Increase the maximum number of sockets that can be created.

ADACM017I | TCP/IP HAS TERMINATED
Explanation | Unless this message is accompanied by an error message, TCP/IP has terminated normally.
Action | If an error message accompanies this message, refer to that message. Otherwise, this message is for information only.

ADACM018E | THE API CANNOT LOCATE THE TCP/IP SPECIFIED
Explanation | The stack specified in the URL is not valid: TCP/IP cannot initialize.
Action | Ensure that the stack is available on the system and that it is active.

ADACM019E | THE TCP/IP NAME SPECIFIED IS NOT VALID
Explanation | The TCP/IP name specified in the URL is not valid.
Action | Check that the URL contains the correct stack name. If so, ensure that the stack is available on the system and that it is active.

ADACM020E | TCP/IP FAILED TO LOAD
Explanation | The TCP/IP stack specified in the URL cannot be initialized.
Action | Ensure that the TCP/IP stack specified is correct and that it is active. If it is correct and active, contact the systems administrator.

ADACM021E | UNABLE TO ALLOCATE STORAGE FOR SOCKETCB
Explanation | ADATCP is unable to allocate the necessary storage.
Action | Ensure that adequate storage is available on the system.

ADACM022E | INVALID OPERATING SYSTEM FOR API=HPS
Explanation | The operating system specified in the URL is incorrect.
Action | The only operating systems currently supported are OES and HPS.

ADACM023E | UNABLE TO INITIALIZE TCP/IP INTERFACE
Explanation | The TCP/IP stack specified in either the URL or the protocol that was used is invalid.
Action | Check that the URL or protocol contains the correct stack name. If so, ensure that the stack is available on the system and that it is active.

ADACM024E | UNABLE TO GET A SOCKET
Explanation | The system is unable to create a new socket. This may be caused by an incorrect stack. If an error number accompanies this message, it will inform you if the problem is inadequate system resources (ENOBUFS) or access denied (EACCES).
Action | Ensure that the correct stack is being used. If the problem is inadequate system resources, contact your systems administrator. Contact your security administrator for system access problems.

ADACM025E | UNABLE TO BIND SOCKET TO LOCAL SYSTEM
Explanation | ADATCP was unable to bind the socket to the local system. Another application may be using the port specified in the URL.
Action | Use the TSO NETSTAT command to check current use of the specified port. If something else is using the port, terminate ADATCP and change the port in the URL.

ADACM026E | UNABLE TO ACCEPT CONNECTIONS
Explanation | ADATCP is unable to accept connections from client applications. This may indicate a shortage of buffer space or that the maximum number of socket descriptors have already been created/opened.
Action | Ensure that adequate buffer space is available to the system. If necessary, increase the maximum number of sockets available to the system.

ADACM027E | UNABLE TO LISTEN FOR NEW CONNECTIONS
Explanation | ADATCP is unable to listen for new connections. This usually indicates that the system resources available to complete the call are inadequate. If an error number is supplied with this message, it will help to identify the problem.
Action | If system resources are inadequate, contact your systems administrator.

ADACM028E | UNABLE TO SET SOCKOPT REUSEADDR OPTION
Explanation | An attempt to allow currently used local addresses to be bound failed. This may indicate inadequate system resources. If an error number is supplied with this message, it will help to identify the problem.
Action | If system resources are inadequate, contact your systems administrator.

ADACM029E | UNABLE TO GIVESOCKET TO NEW THREAD
Explanation | ADATCP was unable to give control of a socket to a different process. This error occurs only if there is a problem with the socket itself. If an error number is supplied with this message, it will help to identify the problem.

ADACM030E | UNABLE TO CREATE A NEW THREAD
Explanation | The system was unable to create a new thread. This indicates inadequate system resources or memory to create the thread.
Action | Contact your systems administrator.

ADACM031E | UNABLE TO CLOSE THE REQUESTED SOCKET
Explanation | ADATCP attempted to close a socket that was being used by another thread in the same process. This occurs only when the system is terminating due to some other error.
Action | Check the console for other messages.

ADACM032E | UNABLE TO MALLOC STORAGE
Explanation | ADATCP was unable to allocate storage. This may indicate that inadequate storage is available on the system.
Action | Contact your systems administrator.

ADACM034E | UNABLE TO RECEIVE DATA
Explanation | ADATCP cannot receive data from a client. This may indicate that the connection between ADATCP and the client has been severed during a transaction or that system resources are inadequate to complete the call. The error number supplied with this message will identify the problem.
Action | Contact your systems administrator.

ADACM035E | UNABLE TO TAKE THE SOCKET
Explanation | The process that send requests to and from Adabas was unable to take control of the socket that was passed to it by the listening task.
Action | Check the error number and the return code that accompany this message.

ADACM036E | UNABLE TO SET THE CANCEL TYPE
Explanation | The main request task is unable to set the cancel type for the thread that is currently running.
Action | Check the error number and the return code that accompany this message.

ADACM037E | UNABLE TO SEND DATA
Explanation | ADATCP is unable to send data from a client. The error number issued with this message indicates whether the problem is a severed connection between ADATCP and the client or insufficient system resources to complete the call.
Action | Check the error number issued with this message.

ADACM038E | UNABLE TO CLOSE THE SOCKET
Explanation | ADATCP attempted to close a socket while it was being used by another thread in the same process. This occurs if the system has tried to terminate due to another error.
Action | Check for other messages issued to the console.

ADACM039E | CONTEXT TABLE FULL
Explanation | The number of connections has reached a predefined limit; no entries can be added to the user context table.
Action | Increase the ADARUN NU parameter value to the required number of entries and restart ADATCP.