DCAM Feedback Codes

#### Search Results

Search

# DCAM Feedback Codes

Code | Explanation
--- | ---
0C04 | Application not connected with partner. LOSCON contingency processing is probably pending.
0C40 | Connection was refused by partner without reason. With TRANSIT-CD (Entire Net-Work VTAM): Line was deactivated (INACT); e.g., /DADM PX25,vr,RESET,vr11r7.
0C48 | Time-out for connection request. With TRANSIT-CD (Entire Net-Work VTAM): Cross-domain session did not notice IPL on IBM side; e.g., /DADM PNET,vr,ACT,siehost,siegat.
0C4C | DCAM partner application not active.
0C5CXX | OPNCON was rejected by partner: 00: 18: Application not active on SISNIX (via HDLC). ISO=Y on X.25 link. 2: Partner rejects connection; partner has different information (NAME) for this application; or ISO application wanted to connect to a non-ISO application. 5C: Application not active via X.25; or an X.25 "call-user-data" was probably required.
0C78 | Immediately after connection installation, the partner or system disconnected. ISO parameter missing.
1840 | Invalid processor name: Check that the processor name is in RDDF; Issue a /BCIN command.
100408 | BDCAM buffer shortage. DCAM driver waits for 5 seconds and retries operation. When GO signal is not used. retry is scheduled after DCAM has given the GO signal.
10040C | BDCAM buffer shortage. Wait for GO signal.