Supplied UES Encodings

#### Search Results

Search

# Supplied UES Encodings

The tables in this document list the encodings available with universal encoding support (UES) when executing Adabas utilities or issuing Adabas commands. Encodings represent single-byte character sets (Latin-1 or not) or double-/multiple-character sets. If encodings:

- have a character set in common with other encodings so that conversion between them is accomplished without loss of data, they are "interoperable". Two encodings are said to be interoperable when all round-trip string conversions return the same string as the original or if they have the same the CS number and F/M/S size.

- are not interoperable, they are "coexistent" with other encodings.

Columns used in the following tables are described as follows:

Key | ADAECS key number in decimal and hexadecimal
CS | character set as identified by IBM
CP | code page usually identical to the "key". It is not identical when CP does not fit into the ECS key number range 1-4095; or the encoding is constructed from two or more code pages.
F/M/S Size |
F | encoding uses all allocated graphical character space
M | maximum for given ESID
S | subset
ESID | encoding scheme identifier with the following entries:
1100 | EBCDIC fixed 1
1301 | EBCDIC mixed DBCS modal
2100 | IBM PC data fixed 1
2200 | IBM PC data DBCS only
2300 | IBM PC data mixed DBCS nonmodal
4100 | ISO-8 fixed 1
4105 | ISO-8 fixed 1 graphic characters in the range x'80'- x`9F' reserved for control codes
Fill | the hexadecimal value representing the fill character used in the encoding.
Sub | the hexadecimal value representing the substitution character used in the encoding.

Encoding categories are described in this document.

- Interoperable Encodings

- Coexistent Encodings

## Interoperable Encodings

### Single-Byte Character Sets (Latin-1)

Key | CS | CP | F/M/S Size | ESID | Fill | Sub | Description
--- | --- | --- | --- | --- | --- | --- | ---
Dec | Hex |
37 | 025 | 697 | 37 | F 190 | 1100 | 40 | 3F | CECP: USA, Canada (ESA*), Netherlands, Portugal, Brazil, Australia, New Zealand
273 | 111 | 697 | 273 | F 190 | 1100 | 40 | 3F | CECP: Austria, Germany, de_deu
277 | 115 | 697 | 277 | F 190 | 1100 | 40 | 3F | CECP: Denmark, Norway
278 | 116 | 697 | 278 | F 190 | 1100 | 40 | 3F | CECP: Finland, Sweden
280 | 118 | 697 | 280 | F 190 | 1100 | 40 | 3F | CECP: Italy, it_ita
284 | 11C | 697 | 284 | F 190 | 1100 | 40 | 3F | CECP: Spain, Latin America (Spanish), es_esp
285 | 11D | 697 | 285 | F 190 | 1100 | 40 | 3F | CECP: United Kingdom, en_gbr
297 | 129 | 697 | 297 | F 190 | 1100 | 40 | 3F | CECP: France, fr_fra
500 | 1F4 | 697 | 500 | F 190 | 1100 | 40 | 3F | CECP: Belgium, Canada (AS/400*), Switzerland, international Latin-1
819 | 333 | 697 | 819 | F 190 | 4100 | 20 | 1A | ISO 8859-1: Latin alphabet, Latin-1
871 | 367 | 697 | 871 | F 190 | 1100 | 40 | 3F | CECP: Iceland, is_ISL
1140 | 474 | ** | 1140 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 37 with euro sign
1141 | 475 | ** | 1141 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 273 with euro sign
1142 | 476 | ** | 1142 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 277 with euro sign
1143 | 477 | ** | 1143 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 278 with euro sign
1144 | 478 | ** | 1144 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 280 with euro sign
1145 | 479 | ** | 1145 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 284 with euro sign
1146 | 47A | ** | 1146 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 285 with euro sign
1147 | 47B | ** | 1147 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 297 with euro sign
1148 | 47C | ** | 1148 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 285 with euro sign
1149 | 47D | ** | 1149 | F 190 | 1100 | 40 | 3F | IBM EBCDIC 871 with euro sign
*3946 | F6A | 697 | 850 | S 190 | 2100 | 20 | 7F | PC data-190: Latin alphabet, Latin-1 (CCSID=4946)

* This code page is not yet available but may be at a later time.

** This information is not yet available.

### Single-Byte Character Sets (Non-Latin-1)

Key | CS | CP | F/M/S Size | ESID | Fill | Sub | Description
--- | --- | --- | --- | --- | --- | --- | ---
Dec | Hex |
420 | 1A4 | 235 | 420 | M 181 | 1100 | 40 | 3F | IBM, Arabic (all presentation shapes)
424 | 1A8 | 941 | 424 | M 152 | 1100 | 40 | 3F | IBM, Hebrew, iw_isr
813 | 32D | 925 | 813 | M 183 | 4100 | 20 | 1A | ISO 8859-7: Greek/Latin, el_GRC
870 | 366 | 959 | 870 | F 190 | 1100 | 40 | 3F | IBM, Latin-2
875 | 36B | 925 | 875 | M 184 | 1100 | 40 | 3F | IBM, Greek, el_GRC
912 | 390 | 959 | 912 | F 190 | 4100 | 20 | 1A | ISO 8859-2: Latin-2
914 | 392 |  | 914 | F 190 | 4100 | 20 | 1A | ISO 8859-4
915 | 393 | 1150 | 915 | F 190 | 4100 | 20 | 1A | ISO 8859-5: Cyrillic, 8-bit
916 | 394 | 941 | 916 | M 152 | 4100 | 20 | 1A | ISO 8859-8: Hebrew, iw_ISR
918 | 396 | 1160 | 918 | F 190 | 1100 | 40 | 3F | IBM, Urdu
919 | 397 |  | 919 | F190 | 4100 | 20 | 1A | ISO 8859-10
920 | 398 | 1152 | 920 | F 190 | 4100 | 20 | 1A | ISO 8859-9 Latin-5 (ECMA-128, Türkiye TS-5881), tr_TUR
921 | 399 | 1305 | 921 | F 190 | 4100 | 20 | 1A | IBM, Baltic, 8-bit
922 | 39A | 1307 | 922 | F 190 | 4100 | 20 | 1A | IBM, Estonia, 8-bit
923 | 39B | ** | 923 | F 190 | 4100 | 20 | 1A | ISO 8859-15 Latin-9 with euro sign
924 | 39C | ** | 924 | F 190 | 1100 | 40 | 3F | IBM EBCDIC Latin-9 with same character set as 923.
1006 | 3EE | 1160 | 1006 | F 190 | 4100 | 20 | 1A | IBM, Urdu
1025 | 401 | 1150 | 1025 | F 190 | 1100 | 40 | 3F | IBM, Cyrillic multilingual
1026 | 402 | 1152 | 1026 | F 190 | 1100 | 40 | 3F | IBM, Türkiye Latin-5, tr_TUR
1112 | 458 | 1307 | 1112 | F 190 | 1100 | 40 | 3F | IBM, Baltic, multilingual (EBCDIC)
1122 | 462 | 1307 | 1122 | F 190 | 1100 | 40 | 3F | IBM, Estonia (EBCDIC)
3581 | DFD | ** | 3581 | F190 | 1100 | 40 | 3F | DF.04-F Latin-9, CCSN:EDF04F, Extended BS2000 code EBCDIC)

** This information is not yet available.

### Double- and Multiple-Byte Character Sets

Key | CS | CP | F/M/S Size | ESID | Fill | Sub | Description
--- | --- | --- | --- | --- | --- | --- | ---
Dec | Hex |
290 | 122 | 1172 | 290 | M 162 | 1100 | 40 | 3F | Japanese Katakana host extended SBCS, ja_JPN
836 | 344 | 1174 | 836 | M 99 | 1100 | 40 | 3F | Simplified Chinese host extended SBCS (EBCDIC), zh_CHN
1027 | 403 | 1172 | 1027 | M 162 | 1100 | 40 | 3F | IBM, Japanese Latin host extended SBCS, ja_JPN
1041 | 411 | 1172 | 1041 | S 162 | 2100 | 20 | 1A | IBM, Japanese PC data extended SBCS, ja_JPN
1043 | 413 | 1175 | 1043 | M 97 | 2100 | 20 | 1A | IBM, traditional Chinese PC data extended SBCS, zh_TWN
1115 | 45B | 1174 | 1115 | M 99 | 2100 | 20 | 1A | IBM, simplified Chinese PC data single-byte (IBM GB) including 5 SAA SB characters, zh_CHN
1380 | 564 | 937 | 1380 | M 9355 | 2200 | A1A1 | FEFE | IBM, simplified Chinese DBCS PC (IBM GB) including 1880 UDC and 31 IBM-selected, zh_CHN
1381 | 565 | 1174937 | 11151380 | M 9454 | 2300 | 20 A1A1 | 1A FEFE | IBM, simplified Chinese PC data mixed (IBM GB) including 1880 UDC, 31 IBM-selected and 5 SAA SB characters, zh_CHN
3026 | BD2 | 1172370 | 290 300 | S 9306 | 1301 | 40 4040 | 3F FEFE | IBM CCSID 5026, Japanese Katakana-Kanji host mixed including 1880 UDC, extended SBCS, ja_JPN
3035 | BDB | 1172 370 | 1027 300 | S 9306 | 1301 | 40 4040 | 3F FEFE | IBM CCSID 5035, Japanese Latin-Kanji host mixed including 1880 UDC, extended SBCS, ja_JPN
3396 | D44 | 370 | 300 | S 9144 | 1200 | 4040 | FEFE | IBM, CCSID 4396, Japanese host double-byte including 1880 UDC, ja_JPN
3709 | E7D | 1175 | 3709 | S 97 | 1100 | 40 | 3F | IBM CCSID 28709: traditional Chinese host extended SBCS (EBCDIC), zh_TWN
4091 | FFB |  |  | F 63456 |  | 0020 | 001A | UTF-8: with user/compatibility area; without surrogates

## Coexistent Encodings

### Single-Byte Character Sets

Key | CS | CP | F/M/S Size | ESID | Fill | Sub | Description
--- | --- | --- | --- | --- | --- | --- | ---
Dec | Hex |
3 | 3 | 103 | 367 | F 94 | 5100 | 20 | 1A | US-ASCII
6 | 6 |  |  | F 190 | 4100 | 20 | 1A | ISO 8859-3, Latin-3, Afrikaans, Catalan, Dutch, English, German, Italian, Maltese, Spanish, Turkish
9 | 9 |  |  | M 145 | 4100 | 20 | 1A | ISO 8859-6, Arabic
437 | 1B5 | 697 | 437 | F 222 | 2100 | 20 | 1A | Microsoft MSDOS US, en_USA
720 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 720, Arabic
737 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 737, Greek
775 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 775, Baltic
803 | 323 | - | 803 | F 88 | 1100 | 40 | 3F | IBM-803_STD Old Hebrew EBDIC IBM-803_p100-1999
850 | 350 | 1106 | 950 | F 223 | 2100 | 20 | 1A | Microsoft multilingual code page 850, Latin-1
852 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 852, cp852_DOSLating2
857 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 857, Turkish
858 | 350 | 1106 | 950 | F 222 | 2100 | 20 | 1A | Microsoft multilingual code page 850, Latin-1, euro-ready
862 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 862, Hebrew
866 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 866, Cyrillic
874 |  |  |  | F 223 | 2100 | 20 | 1F | Microsoft Windows OEM Codepage 874, Thai
1047 |  | 697 |  | F 190 | 1100 | 40 | 3F | IBM Latin-1 Open Systems EBCDIC
1250 | 4E2 | 1400 | 1250 | M 217 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Latin-2, euro-ready
1251 | 4E3 | 1401 | 1251 | M 220 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Cyrillic, euro-ready
1252 | 4E4 | 1402 | 1252 | M 215 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Latin-1, euro-ready
1253 | 4E5 | 1403 | 1253 | M 206 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Greek, euro-ready
1254 | 4E6 | 1404 | 1254 | M 215 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Türkiye, euro-ready
1255 | 4E7 | 1405 | 1255 | M 194 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Hebrew, euro-ready
1256 | 4E8 | 1406 | 1256 | M 214 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Arabic, euro-ready
1257 | 4E9 | 1407 | 1257 | M 203 | 4105 | 20 | 1A | Microsoft, Windows ANSI, Baltic rim, euro-ready
2084 |  | 948 | 878 | F 222 | 4105 | 20 | 1F | KO18-R, Cyrillic PC
2087 |  | 813 | 775 | S 222 | 2100 | 20 | 1F | MS-DOS Baltic PC-Data
2258 |  | 1408 | 1258 | S 212 | 4105 | 20 | 1F | Microsoft, Windows-1258, Vietnam
3585 | E01 | 646 |  | S 95 | 1100 | 40 | 3F | BS2000 DF.03 International CCSN:EDF03IRV
3586 | E02 | 265 |  | S 95 | 1100 | 40 | 3F | BS2000 DF.03 CCSN:EDF03DR Austria, Germany (EBCDIC) - with Dollar
3587 | E03 |  |  | S 95 | 1100 | 40 | 3F | BS2000 DF.03 CCSN´:EDF03DRI Austria, Germany (EBCDIC) - with International Currency Sign
3588 | E04 | 697 |  | F 190 | 1100 | 40 | 3F | BS2000 DF.04-DR V LATIN 1, CCSN:EDF04DR Austria, Germany (EBCDIC)
3589 | E05 | 697 |  | F 190 | 1100 | 40 | 3F | BS2000 DF.04-1 LATIN 1, CCSN:EDF041IRV International (EBDIC)
4092 | FFC |  |  | 3 | - | 20 | A1 | Software AG, used for ECS internally
4093 | FFD |  |  |  | 4100 | 20 | 1A | Software AG, old TS default, ASCII
4094 | FFE | - | - |  | 1100 | 40 | 3F | Software AG, old TS default, EBCDIC
4095 | FFF |  |  | - | 7200 | 0020 | 001A | Unicode

### Double- and Multiple-Byte Character Sets

Key | CS | CP | F/M/S Size | ESID | Fill | Sub | Description
--- | --- | --- | --- | --- | --- | --- | ---
Dec | Hex |
18 | 12 | 103 1061 1121 1062 | 367 952 896 953 | S 13102 | 4403 | 20 8140 | 1A | IBM CCSID 1350, EUC-JP, ja_JPN composed of US-ASCII, JIS-X-0208, HW Katakana, and JIS-X-0212-90
36 | 24 |  |  |  | 5404 | 20 | 1A | ISO-2022-JP, US-ASCII, JIS-Roman, JIS-0208-1983, JIS_C_6226-1978
300 | 12C | 1001 | 300 | M 11634 | 1200 | 4040 | FEFE | IBM Japanese Latin host double-byte including 4370 UDC, ja_JPN
301 | 12D | 370 | 301 | M 9144 | 2200 | 8140 | FCFC | IBM Japanese PC double-byte including 1880 UDC, SJIS, ja_JPN
835 | 343 | 935 | 835 | M 20263 | 1200 | 4040 | FEFE | IBM traditional Chinese host double-byte including 6204 UDC (EBCDIC) zh_TWN
837 | 345 | 937 | 837 | M 9355 | 1200 | 4040 | FEFE | Simplified Chinese host double-byte including 1880 UDC (EBCDIC), zh_CHN
927 | 39F | 935 | 927 | M 20263 | 2200 | 8140 | FCFC | IBM traditional Chinese PC data double-byte including 6204 UDC, zh_TWN
932 | 3A4 | 1122370 | 897 301 | M 9301 | 2300 | 20 8140 | 1A | Microsoft, JIS Roman, JIS-X-208, half-width Katakana, ja_JPN
935 | 3A7 | 1174 937 | 836 837 | M 9454 | 1301 | 40 4040 | 3F FEFE | Simplified Chinese host mixed including 1880 UDC, extended SBCS (EBCDIC), zh_CHN
936 | 3A8 | 1185 937 | 1185 937 | M 9449 | 2300 | 20 1A1A | 1A | Microsoft, GB Roman, GB 2312-80, zh_CHN
937 | 3A9 | 1175 935 | 903 937 | S 20360 | 1301 | 40 4040 | 3F FEFE | IBM traditional Chinese host mixed including 6204 UDC, extended SBCS (EBCDIC), zh_TWN
942 | 3AE | 1172 370 | 1041 301 | M 9306 | 2300 | 20 8140 | 1A FCFC | IBM, Japanese PC data mixed including 1880 UDC, extended SBCS, ja_JPN
948 | 3B4 | 1175 935 | 948 | M 20360 | 2300 | 20 8140 | 1A FCFC | IBM, traditional Chinese PC data mixed including 6204 UDC, extended SBCS, zh_TWN
949 | 3B5 | 1278 1050 | 949 | M 10197 | 2300 | 20 A1A1 | 1A AFFE | IBM, Korean IBM KS code - PC data mixed including 1880 UDC, ko_KOR
950 | 3B6 | 103 935 | 950 | M 20357 | 2300 | 20 A140 | 1A | Microsoft, Big Five, zh_TWN
951 | 3B7 | 1050 | 951 | M 10103 | 2200 | A1A1 | AFFE | IBM, Korean IBM KS code - PC data double-byte including 1880 UDC, ko_KOR
3001 |  | 10001 | 3001 |  |  | 20 8140 | 1A | MAC Japanese, JIS-Roman, JIS-X-208, HW Katakana, ja_JPN
4037 |  | 1175 935 |  | S 20360 | 1301 | 40 4040 | 3F FEFE | Same as EDD 937 Chinese EBCDIC, with code point X'5F' mapped to Unicode U+005E and X'B0' to U+00AC

### On this page

- Interoperable Encodings
- Coexistent Encodings