User Abend Codes

#### Search Results

Search

# User Abend Codes

The decimal abend (abnormal end) codes described in this document occur in ADAInn, ADARUN, and in some utility messages or during replication or transaction manager processing. The message ADAM99 presents both system and nucleus STAE abend codes in hexadecimal; in this case, a nucleus abend code must first be changed to decimal before the description can be located here.

Most abend codes (except 20) result from errors that normally require assistance from your Adabas support technical representative. If abend codes 23 or 24 occur, save the Work data set. For all abend codes, save any dumps and note any messages or other indications that the system issues. Advise your Adabas technical support representative of the error.

Note
Entire Net-Work issues only the abend code 253 to indicate an abnormal termination occurred. The abend (abnormal end) codes described in this document are issued primarily by Adabas modules operating with Entire Net-Work. Specific information related to an error is given in the messages written to the print data set.

Code | Module | Explanation
--- | --- | ---
15 | (nucleus) | Workpool too small to execute session autorestart.
16 | (nucleus) | DTP=RM: Two-phase commit logic error.
17 | (nucleus) | DTP=RM: Work-part-4 overflow.
19 | (nucleus) | DTP=RM: Two-phase commit logic error.
20 | (nucleus) | Error during system startup (refer to descriptions of nucleus startup errors in Adabas Messages and Codes).
21 | (nucleus) | I/O error during asynchronous buffer flush (Asso/Data/Work/PLOG).
22 | (nucleus) | I/O error on sequential PLOG and PLOGRQ=YES/FORCE in effect.
23 | (nucleus) | WORK overflow.
24 | (nucleus) | Autostart canceled - protection area inconsistent.
25 | (nucleus) | Logical I/O error: Adabas was unable to track one or more I/O operations).
26 | (nucleus) | Adabas session canceled by operator command.
27 | (nucleus) | Session ended due to work pool space problems.
28 | (nucleus) | Nucleus problem during an asynchronous buffer flush.
29 | (nucleus) | Adabas Transaction Manager (ATM) initialization failed. Review the console messages for further information about the error.
30 | (nucleus) | Adabas Transaction Manager (ATM) interface error.
31 | (nucleus) | Insufficient workpool space for only active command.
32 | (nucleus) | Internal error processing search algorithm 3 command.
33 | (nucleus) | Logic error during file number validation.
33 | ADARAC | Recovery Aid logic error.
34 | utilities | Abnormal termination with dump.
35 | utilities | Abnormal termination without dump.
36 | utilities | I/O error occurred while writing to DDDRUCK or DDPRINT. Check JCL.
37 | (nucleus) | ET post logic error.
38 | (nucleus) | Unexpected response code for internal command.
39 | (nucleus) | Fatal internal response code occurred during asynchronous buffer flush.
40 | (nucleus) | Getmain failure early during session start.
40 | ADACOM | Fatal error during ADACOM processing (cluster environments).
41 | ADADSFN | Fatal error during Delta Save Facility processing.
42 | (nucleus) | A security violation occurred at startup.
43 | (nucleus) | Logic error in command selection (freeze table).
44 | (nucleus) | Logic error in an FST write or an online process.
45 | (nucleus) | Logic error in asynchronous buffer flush by volume (with ASYTVS=YES).
46 | (nucleus) | Logic error in the buffer pool manager.
47 | (nucleus) | Logic error in thread management.
48 | (nucleus) | Logic error in ADANCX (cluster environments).
49 | (nucleus) | General internal error (various reasons).
50 | (nucleus) | Logic error in SRB code (Adabas Cluster Services).
51 | (nucleus) | Logic error in dynamic Work access.
52 | (nucleus) | STCK clock not running.
53 | (nucleus) | Logic error in global hold queue element lock handling.
54 | (nucleus) | Logic error in global file lock handling.
55 | ADACLU | Fatal error during ADACLU processing (cluster environments).
56 | (nucleus) | Logic error in ET synchronization process.
57 | (nucleus) | Unexpected error during online recovery.
58 | (nucleus) | Error in protection record bookkeeping.
59 | (nucleus) | Logic error during large object (LB) processing.
60 | (nucleus) | Unique descriptor update logic error.
61 | (nucleus) | Logic error in system field update.
63 | (auditing) | Logic error in auditing processing.
65 | (replication) | Fatal error related to replication processing.
66 | (replication) | Logic error in initial-state processing.
67 | (auditing or replication) | Logic error in SLOG handling.
70 | (nucleus) | Parallel Services nucleus canceled by peer nucleus.
71 | (nucleus) | Logic error or bad data in protection data area extension on Work data set.
72 | (nucleus) | Logic error in protection data publishing.
79 | (nucleus) | Uncorrectable intracluster communication failure.
80 | (nucleus) | Logic error in update tracking.
82 | (nucleus) | Logic error in file activity bookkeeping.
83 | (nucleus) | Logic error in extended MU/PE handling.
84 | (nucleus) | Logic error in spanned record handling.
85 | (nucleus) | Logic error in spanned record read-lock handling.
86 | (nucleus) | Logic error in Adabas Fastpath multifetch processing.
87 | (nucleus) | Logic error in multiple buffers.
89 | (nucleus) | Logic error during global update command synchronization.
90 | (nucleus) | Logic error when updating a compressed record.
91 | (nucleus) | Internal error.
92 | (nucleus) | Logic error during increase of an address converter extent.
93 | (nucleus) | Logic error when processing an online function.
94 | (nucleus) | Logic error in special descriptor decompression.
95 | (nucleus) | Logic error during AAD,AA handling.
96 | (nucleus) | Logic error in command selection.
108 | ADATRA | Failure to load and install the trace module.
109 | ADAZIP | Fatal error related to the execution of Adabas code on a System z Integrated Information Processor (zIIP).
220 | MPMVSE | FREEVIS problem.
221 | MPMVSE | Invalid operating system.
222 | MPMVSE | Invalid function.
227 | MPMBS2 | Wrong ADARER module found.
228 | MPMBS2 | STXIT not successfully installed.
229 | MPMBS2 | Invalid function in dependent MPM call.
231 | MPMBS2 | The command queue referenced in the ID table does not match the target ID in the call.
232 | MPMBS2 | The ID table is being referenced but the MPM has a zero (0) address.
233 | MPMBS2 | Adabas canceled in BOURSE WAIT (see the ADAM82 message description in Adabas Messages and Codes).
234 | MPMBS2 | Enqueue to IDT failed (BS2000).
235 | MPMBS2 | Unable to acquire memory for MPM client table UTAB (BS2000).
245 | MPMMVS | Error locating ADAIOR in ESTAE recovery routine.
246 | RAOSSYDI (Adabas Review) | An error occurred when writing a message to the console (WTO).
247 | MPMMVS | Unsuccessful STAE.
248 | MPMMVS or MPMF4 | Invalid operating system or RMODE; for MPMF4, invalid operating system or RMODE; or CID GETMAIN failed The operating system check did not recognize a "known" operating system. The known system is z/OS. For z/OS: if the nucleus is running AMODE 31, then RMODE 24 was not set for at least one Adabas module other than ADALNK.
249 | MPMMVS | Invalid function.
251 | ADARST | Unrecoverable abend of the Adabas Review subtask ADARST. See the ADAM90 message description.
252 | IORSUB | Unrecoverable subtask abend. See the ADAM90 message description.
253 | MPMIND | Nonrecoverable abend (caused by STAE/STXIT processing program check or nucleus abend) See the ADAM99 message description in Adabas Messages and Codes.
254 | MPMIND | Invalid function in abnormal termination Recovery exit.
255 | MPMIND | Invalid function.
257 | MPMVSE | Return code on 24-call from FREEVIS.
435 | ADASIP | The specified subsystem name is already being used by another ADABAS SVC. This ABEND is accompanied by message ADAS16. Select another subsystem name and rerun the job.
436 | ADASIP | The currently installed SVC is using a different subsystem. This ABEND is accompanied by message ADAS16 and may be overridden by the FORCE=Y parameter.
437 | ADASIP | There are one or more potentially active targets in the IDT of the specified SVC. This ABEND is accompanied by message ADAS17 and may be overridden by the FORCE=Y parameter.
454 | SVCVSE | SVC 04-call buffer address error.
455 | SVCVSE | SVC 16-call buffer address error.
456 | SVCVSE | SVC work area allocation error.
470 | SIPMVS | SVCMVS load error.
471 | SIPMVS | Incorrect SVCMVS.
472 | SIPMVS | SSCT disappeared.
473 | SIPMVS | ADASIR non-zero return code.
474 | SIPMVS | SVC table entry changed.
475 | SIPMVS | SSCT already exists.
476 | LNKBS2 | Request for user buffer memory in ADALNK failed.
SIPMVS | GETMAIN error.
477 | SIPMVS | Incorrect ADASIR.
478 | SIPMVS | ADASIR load error.
479 | SIPMVS | ADASIR or ADASVC were not found in the load libraries provided to the ADASIP job.
480 | SIPMVS | Open error.
481 | SIPMVS | EXEC PARM error.
482 | SIPMVS | SIPMVS not authorized.
485 | LNKBS2 | Unsupported function.
LNKBTO
LNKIX1
486 | SVCMVS | Invalid PCR04 call.
487 | SVCMVS | Caller specified an unknown or invalid target. This is possibly caused by restarting an already active target using FORCE=YES.
488 | SVCMVS | Invalid PCR16 call.
489 | SVCMVS | Invalid 48-call parameters
490 | MPMBS2 | Target ID table may only be changed by a communicator.
SVCMVS
491 | SVCMVS | SVC 12-call without 16-call required
SVCVSE
492 | SVCMVS | Active dormant LX.
493 | SVCMVS | Invalid 00-call parameters.
494 | SVCMVS | Caller not authorized.
496 | SVCMVS | No IDT.
497 | SVCMVS | Invalid function.
498 | LNKBTO | Invalid UB.
LNKIX1
499 | LNKBTO | Length of user info less than zero.
LNKIX1
500 | LNKBS2 | Error in link initialization routine.
LNKBTO
LNKIX1
501 | LNKBTO | Incorrect router version.
LNKIX1
502 | LNKBTO | User exit before-call increased length of user info.
LNKIX1
509 | IORMVS | DEB error.
513 | SVCVSE | Invalid SVC-08 call.
515 | IORIND | GTALNK error.
516 | IORIND | RWINT error.
517 | IORIND | RWINT Cache Fast Write request error.
519 | IORIND | UPELE error.
539 | IORSUB | FVSE error.
540 | IORSUB | FVST error.
545 | IORMVS | BCP storage error.
547 | IORMVS | Initialization error.
548 | IORMVS | BCP error.
549 | IORMVS | DLECB error.
550 | IORMVS | QEDIT (block) error.
551 | IORMVS | CHKIO error.
559 | IORMVS | Incorrect SVC version.
560 | IORMVS | Maximum blocks/track > minimum, I/O error, global sequential BLKSIZE too big, or invalid number (ECBS).
561 | IORMVS | EVENTS error.
563 | IORBS2 | Invalid TDCE found during ADAIOR INIT.
564 | IORBS2 | Failure to load ADAIOI or AT when trying to enable EVENT NAME.
565 | IORBS2 | ECB list overflow.
566 | IORBS2 | Invalid SOLSIG return code
567 | IORBS2 | Cannot load ADAONR
568 | IORBS2 | BCP error
569 | IORBS2 | WTOR error
570 | IORBS2 | CHKIO error
571 | IORBS2 | Invalid ECB type
572 | IORBS2 | Invalid event checksum
573 | IORBS2 | SOLSIG RC operator commands/EOC
574 | IORBS2 | No multiple RSOFEI postcode mem
577 | LNKCX | User exit before-call increased length of USER INFO
578 | IORVSE | CHKIO error
579 | LNKCX | Error in link initialization routine
580 | LNKCX | Length of user info less than 0 (greater than 32K)
581 | LNKCX | Incorrect router version
582 | LNKCX | Invalid UB
583 | IORMVS | QEDIT (CIBCTR) error
584 | LNKCX | Unsupported function
591 | IORVSE | EVENTS error
592 | IORVSE | GETDVS error
593 | IORVSE | IVST error
594 | USRBTO | Invalid RMODE
595 | IORVSE | EXTRACT error
596 | IORVSE | GETLBL error
597 | IORVSE | TOPMSG error
598 | IORMVS | ADECB error
599 | IORVSE | ADECB error
600 | IORVSE | DLECB error
601 | IORVSE | SUBSID error, invalid version, or ADAIOI could not be loaded
602 | IORVSE | CKTDC error
603 | IORVSE | Global sequential block size too big or invalid number (ECBS)
604 | IORVSE | GETTVS error
605 | IORVSE | Invalid printer device
606 | LNKBS2 | Unsupported ADALNK function code
607 | LNKBS2 | UB flags in ADALNK asynchronous call incorrectly set
608 | LNKBS2 | Length of user info less than 0 (greater than 32K)
609 | LNKBS2 | Unable to acquire ID table common memory
610 | LNKBS2 | User information length at ADALNK before-call too small
611 | LNKBS2 | WAIT error
612 | RERBS2 | IDT (identification table) common memory not accessible in router
613 | RERBS2 | Invalid router function code
614 | SVCVSE | Invalid function via caller
615 | SVCVSE | No IDT (identification table)
616 | SVCVSE | Invalid 00-call parameters
617 | SVCVSE | Invalid 40-caller
618 | SVCVSE | Caller specified an unknown or invalid target. This is possibly caused by restarting an already active target using FORCE=YES.
619 | LNKxx | Invalid SVC number in link routine
SVCVSE | Power job error in SVC
620 | IORIND | IOR fatal error
622 | LNKxx | Invalid SAVE area in UB (LUEXIT1). SAVE area (USERSAV) in the Adabas link routine was less than 72 bytes and user exit 1/2 (B/A in Adabas 7) was invoked.
627 | IORVSE | 64-bit I/O not supported for dev
628 | IORVSE | GETMAIN error during startup
IORMVS
629 | IORVSE | ADAOPTD could not be found, or could not be loaded into storage
631 | IORVSE | GETVIS failed for sequential file table
632 | IORVSE | No more slots in sequential file table
633 | IORVSE | Internal error file name not found
634 | IORVSE | Return code from LABEL macro greater than 4
635 | IORVSE | PFIX/PFREE issued from dynamic partition
639 | LNKCX | A CICS GETMAIN request failed.
640 | LNKBS2 | No memory available for BS2000 LNK anchor block
640 | ADALNK | No memory available for LNK anchor block (BS2000)
641 | LNKBS2 | The SM6 ADALNK detected a router at 5.2 SP5 level or lower. The ID Table must be initialized with an Adabas nucleus at level 5.2 SP6 or higher.
642 | LNKBS2 | The ADALNK cannot read the DDLNKPAR parameter file; the file may be empty, or it may be an ISAM file. Use a SAM/V data set that was created by EDT.
643 | LNKBS2 | The ADALNK detected a syntax error in the DDLNKPAR parameters. Correct the syntax and rerun.
645 | LNKCX | The CICS macro level interface is not supported for CICS/ESA 3.2 and above.
646 | IORBS2 | Cannot read the SYSDTA data set; see the message ADAI56 description.
647 | LNKBTO | Invalid reentrant work area address
LNKIX1
648 | LNKIX1 | Invalid AIBTDLI entry address
649 | LNKCX | CICS TWA not present or too short
LNKIX1 | AIBTDLI INQY ENVIRON call failed
652 | LNKBS2 | Invalid PAL
LNKBTO
LNKCX
LNKIX1
653 | LNKCX | Attempted double wait on UB element
654 | ADALNK | ADALNK: unsupported operating system version, unsupported HSI. Adabas version 6.1 and above requires BS2000 version 10 and above and XS31 hardware.
655 | ADALNK | Incompatible versions of ADALNK and ADAL2P. Check library assignments; check TSOSLNK/BINDER protocols. See message ADAK09.
656 | ADALNI | An internal error occurred when the IMS link routine could find the proper IMS structures to properly set the value for the userid (the last eight bytes of the 28-byte Adabas communication ID). When this user abend occurs, contact your Software AG support representative and provide a dump including the registers at time of the abend so the reason code stored in R15 can be seen and evaluated.
657 | LNKBTO | Dynamic SVC lookup table missing
LNKCX
LNKIX1
658 | LNKBTO | LNKUES module not available to ADALNK
LNKCX
LNKIX1
659 | SVCMVS | PC routine invoked by invalid caller.
660 | LNKCX | CICS instructed ATM to perform a single-phase commit, but the outcome of the attempted commit could not be determined.
661 | SVCMVS | Name/Token service error.
662 | LNKBTO | Program cancel from UEXITR
LNKCX
LNKIX1
663 | LNKCX | LNCSTUB DCI initialization failed
664 | LNKBTO | SVC incompatible with install program
LNKCX
LNKIX1
SVCMVS
SVCVSE
665 | SVCMVS | Invalid SVC caller
SVCVSE
666 | RERBS2 | Invalid AB deallocation length
SVCMVS
SVCVSE
667 | SVCMVS | Unsupported z/OS release or missing CPU features. ArchLvl 2 (64-bit) is required.
668 | ATMCXRMI | A syncpoint operation was triggered by an Adabas command, but the user's communication ID was not known
LNKCX
LNKIX1
669 | SVCMVS | S64 recovery routine manager error.
670 | link routines | The CICS EXTRACT command used to obtain the Adabas Task Related User Exit (TRUE) global work area failed. The Adabas 8 or enhanced Adabas 7 CICS environment is not correctly established. To determine the cause, consult the messages associated with starting the Adabas TRUE issued from ADAENAB (if you are running Adabas 7) or from ADACIC0 (if you are running Adabas 8).
671 | RERBS2 | Attempted router call to shared 64-bit storage Recovery Routine Manager (RRM) on BS2000. Not available on this platform.
672 | SVCMVS | IDT extension not provided. Possible incorrect version of ADASIR (z/OS) or ADAIPR (z/VSE).
SVCVSE
673 | SVCMVS | Invalid PCRCLU caller.
674 | link routines | A version 8 call using the ACBX has been made, but the link routine did not detect a valid reentrancy token in direct call (field APLXRTOK) of the Adabas 8 parameter list.
675 | LNKCX | ADL consistency exit not linked
676 | link routines | The work area passed to an Adabas 8 link routine in the direct call (field APLXRTOK of the APLX) was invalid, or the attempt to obtain storage for the work area failed.
677 | LNKCX | CICS GETMAIN for a UB failed
678 | link routines | The Adabas 8 link routine could not find the address of a link global table, either because it was not linked with the Adabas 8 link routine, or because an attempt to load the link globals table failed. In BS2000 environments, the memory pool accessed does not contain an Adabas ID table.
679 | LNKBS2 | Unable to set up the DBID/IDT Table (Get Memory error)
LNKBTO | ADATMZ invalid header provided
680 | LNKBS2 | Could not get router ID table memory pool. Check the ID table name in the parameter file/module.
LNKBTO | ADATMZ unable to obtain work area
LNKCX
681 | LNKCX | There was insufficient SAF authorization to issue a CICS EXTRACT EXIT command. Ensure that all users of the Adabas link module have UPDATE access to the EXITPROGRAM CICS command resource identifier.
682 | LNKCX | TRUE name cannot be located
683 | LNKBTO | Multiple ECB wait not supported
687 | IOSMVS | Error queuing parallel request
688 | ADAIOR | Fatal error during a switch from SRB to TCB mode when Adabas is zIIP-enabled
689 | ADAIOR | Fatal error during a switch from TCB to SRB mode when Adabas is zIIP-enabled
690 | ADAIOR | A call has been issued in SRB mode, but Adabas is not zIIP-enabled
691 | IOSMVS | Error leaving or joining enclave
692 | ADAIOS | Dataset allocation error
800 | NETSIP/OS | Invalid operating system detected - not MVS
801 | NETSIP/OS | Parameter error detected
802 | NETSIP/OS | Addressing or residency mode, authorization error or operating system is not a virtual machine guest
803 | NETSIP/OS | Error detected during program loading or validation
804 | NETSIP/OS | Space allocation failure
806 | NETSIP/OS | NETSIR initialization failed