ADAI* - ADAIOR System Messages

#### Search Results

Search

# ADAI* - ADAIOR System Messages

Note
Although not considered console messages, those preceded by an asterisk (*) are also displayed on the system console.

### Overview of Messages

`ADAI01 | ADAI02 | ADAI03 | ADAI04 | ADAI05 | ADAI06 | ADAI20 | ADAI21 | ADAI22 | ADAI23 | ADAI24 | ADAI26 | ADAI27 | ADAI29 | ADAI30 | ADAI31 | ADAI32 | ADAI34 | ADAI35 | ADAI39 | ADAI40 | ADAI41 | ADAI42 | ADAI44 | ADAI51 | ADAI52 | ADAI53 | ADAI54 | ADAI55 | ADAI56 | ADAI57 | ADAI5X | ADAI62 | ADAI64 | ADAI65 | ADAI66 | ADAI67 | ADAI68 | ADAI69 | ADAI6U | ADAI6Y | ADAI70 | ADAI71 | ADAI73 | ADAI75 | ADAI76 | ADAI77 | ADAI78 | ADAI79 | ADAI83 | ADAI84 | ADAI85 | ADAI86 | ADAI87 | ADAI91 | ADAI92 | ADAI93 | ADAI94 | ADAI95`

ADAI01 | data set count {READS | WRITES}
Explanation | A sequential data set is closed. The read count is shown when a sequential input data set is closed. The write count is shown when a sequential output data set is closed.

ADAI02 | GETMAIN stor-req (source) GETMAIN stor-req stor-avail (source)
Explanation | The first form of the message is written whenever memory is dynamically acquired and the requested memory is available. The second form of the message is written whenever memory is dynamically acquired and less than the requested memory is available. In the messages, stor-req is the amount of memory requested, stor-avail is the amount of memory available, and source (printed only under z/VSE) is the source of the memory (GETVIS, COMREG, ADABUF).

ADAI03 | data set | physical-file-name countr reads data set | physical-file-name countw writes data set | physical-file-name countf format writes
Explanation | A direct access data set is closed. The physical-file-name indicates that the file was opened using dynamic allocation. The read count countr and write count countw are shown. The write count countw is the count of update writes only. If any format writes were issued, the format write count is shown in countf.

ADAI04 | countr read errors count write errors
Explanation | The message is written immediately following message ADAI03 when a direct access data set for which there had been read and/or write errors is closed.

ADAI05 | countr reads using zHPF countw writes using zHPF
Explanation | Note: This message is available in z/OS systems only. This message is written at data set close following message ADAI03 when a direct access data set used zHPF channel programs for reads or writes. This message is only generated when the zHPF read and write counts differ from the read and write counts in the preceding ADAI03 message.
Action | No action is required for this informational message.

ADAI06 | count retries using ECKD
Explanation | Note: This message is available in z/OS systems only. This message is written at data set close following message ADAI03. If it was necessary to retry any zHPF I/O requests using an ECKD channel program (for instance because zHPF became unavailable on the operating system), the retry count is supplied.
Action | No action is required for this informational message.

ADAI20 | dbid dataset physical-file-name DD: link-name
Explanation | An I/O error occurred on a file opened using dynamic allocation. This message appears immediately after the ADAI21 message.

ADAI21 | dbid IO error DD link-name DSN file-name RABN bad-rabn(start-rabn) oper from start-num Num num-rabn IOBA ioba CCWA ccwa CC ccbs CSW csw SNS sns SYS lu IEDB iedb ADDR ccw-addr CMD ccw-cmd IDA ida-data DATA ccw-data
Explanation | IBM platforms only. This message occurs when a disk I/O error is reported back to ADAIOR by the operating system. The first 3 lines of the message are sent to the console and DDPRINT. Subsequent lines are sent to DDPRINT only. The message variables and their meanings are:
Variable | Description
--- | ---
bad-rabn | The actual failing RABN.
ccbs | Communications bytes from the communications control block.
ccwa | CCW address of failing I/O.
ccw-addr | The CCW address.
ccw-cmd | The CCW data.
ccw-data | Up to 16 bytes of data pointed to by the CCW.
csw | Channel status from the channel status word (CSW).
dbid | Database ID
file-name | The physical file name of the data set.
ida-data | Indirect access address of CCW data.
iedb | The I/O error data block (z/OS only)
ioba | I/O control block address for failing I/O.
link-name | The DD name (z/OS) or DLBL name (VSE) of the data set .
lu | The logical unit where the failure occurred (z/VSE only).
num-rabn | The number of RABNs for this part of the failing I/O operation.
oper | The type of operation being performed when the failure occurred as follows: Read, Write, or Format
sns | Additional sense byte data.
start-num | The start RABN for this part of the failing I/O operation.
start-rabn | The start RABN of the failing I/O operation.
For more information on CCW, CSW and sense data, please refer to the relevant IBM publication.
Action | Use the information provided by the message to locate a possible hardware failure. Keep the information and any dumps for later use. If no hardware failure occurred, please contact your Software AG technical support representative.

ADAI22 | ADAIOR Trace table: --> is current entry
Explanation | The ADAIOR trace table has been activated and printed.

ADAI23 | dbid job-name abend code code
Explanation | z/VSE and BS2000 systems only. ADAIOR is asked to abend a job. A dump is normally also provided. The message values are:
dbid | database ID
code | the abend code (refer to the abend code descriptions in chapter 4).
job-name | the z/VSE job name or BS2000 program name.

ADAI24 | dbid Ready for operator communication
Explanation | SYSLOG displays this message once operator communications has been requested by the operator with the z/VSE MSG command. The value dbid is the database ID.
Action | Enter a valid Adabas command.

ADAI26 | dbid job-name completion code code
Explanation | BS2000 systems: This message displays the normal termination return code. If a nonzero abend code is displayed, the BS2000 program task switch 10 is set on. z/VSE systems: The end-of-job (EOJ) "RC=(RX)" sets the return code for the operating system. The message provides the database ID (dbid), job name, and return code.
Action | BS2000 systems: If job variables are installed, the abend code is passed to the controlling job variable. A job variable assigned with link "*ADA" is set with the following information: program name (8 bytes) completion code (4 bytes) error number (5 bytes) Adabas response code (5 bytes) z/VSE systems: For a nonzero abend code, refer to the description in chapter 4. If the DUMP option was specified, refer to the resulting dump, if needed, to determine the cause of the abend. The job step is terminated.

ADAI27 | dbid Timer interval exceeds maximum allowed dbid Reset to maximum
Explanation | A timer request was issued that exceeds the maximum allowed by the operating system.
Action | Reset the interval to the maximum allowed by your operating system.

ADAI29 | Oper cmd: command
Explanation | An operator command has been entered. The text of the operator command is shown in command.
Action | No action is required for this informational message.

ADAI30 | file-name number tracks formatted
Explanation | ADAIOR has completed formatting for a direct-access file.

ADAI31 | dbid Opening tape file file-name SYSnnn=cuu
Explanation | Note: This message is available in z/VSE systems only. This SYSLOG message means that a tape file was opened. Meanings of the message fields are:
dbid | Adabas database
file-name | filename of the input/output file opened
nnn | z/VSE logical unit ID
cuu | physical address of the selected drive

ADAI32 | dbid Internal error - function func-name error error
Explanation | An internal error has occurred.
Action | Make a note of all recent messages, and contact your Adabas support representative.

ADAI34 | Write to Operator failed - Reason Code nnnnnnnn
Explanation | A write to operator (WTO) request has returned a non-zero response code nnnnnnnn. Following the ADAI34 message, the message which caused the WTO failure is written to DDPRINT as normal, and processing continues.
Action | No action is required for this warning message. However, the user is advised to check the system console log for error messages issued by z/OS relating to WTO problems.

ADAI35 | zHPF channel program error – retrying I/O in ECKD mode
Explanation | Note: This message is available in z/OS systems only. An I/O error has been detected for a zHPF channel program. The zHPF I/O is retried as a non-zHPF I/O and no further zHPF I/O will be attempted on this file extent during the job step. This message is followed by message ADAI41.
Action | No action is required for this informational message.

ADAI39 | {Fixed | Pageable} {1 MB | 2 GB} large page allocation failed -- {not authorized|not available|not supported} {R15=nnnnnnnn R0=nnnnnnnnn}
Explanation | An attempt to allocate storage using fixed or pageable one-megabyte or two-gigabyte large pages failed. One of three possible reasons is listed in the message:
Reason | Description
--- | ---
not authorized | The job was not authorized. Large page allocation requests require APF-authorization.
not available | Large pages are not available on your system.
not supported | Large pages not supported by your system.
When "{R15=nnnnnnnn R0=nnnnnnnnn}" is shown in the message, it indicates that an unexpected return code was received from the z/OS IARV64 service.
Action | No immediate action is necessary, as a storage allocation not using large pages will be attempted instead. Action may be required to prevent this warning message from appearing when the job is next run: If the message indicates that the job was not authorized, ensure when rerunning the job that it is APF-authorized. If your system does not support large pages, do not use the ADARUN parameter causing the attempt to allocate using large pages. Remove it from the startup JCL of the job. If your system does support large pages of the type requested, consider increasing the number of fixed large pages specified for your operating system using the LFAREA parameter in PARMLIB member IEASYSxx. Contact your system administrator for assistance. For more information, read your IBM MVS Initialization and Tuning documentation.

ADAI40 | zHPF unavailable – retrying I/O in ECKD mode
Explanation | Note: This message is available in z/OS systems only. An I/O error has been detected for a zHPF channel program, because zHPF is no longer available. The zHPF I/O is retried as a non-zHPF I/O and no further zHPF I/O will be attempted on any file until after message ADAI42 is issued. This message is followed by message ADAI41.
Action | No action is required for this informational message.

ADAI41 | IO Retry DD link-name DSN file-name RABN bad-rabn(start-rabn) oper from start-num Num num-rabn IOBA ioba TCWA tcwa CC ccbs CSW csw SNS sns IEDB iedb TCW tcw
Explanation | Note: This message is available in z/OS systems only. This message occurs when a disk I/O error on a zHPF channel program is reported back to ADAIOR by the operating system. Message ADAI41 is issued immediately following ADAI35 or ADAI40. If ADAI41 is issued following ADAI40, only the first three lines of message ADAI41 are generated. The first three lines of the message are sent to the console and DDPRINT. Subsequent lines are sent to DDPRINT only. The message variables and their meanings are:
Variable | Description
--- | ---
bad-rabn | The actual failing RABN.
ccbs | Communications bytes from the communications control block.
csw | Channel status from the channel status word (CSW).
dbid | Database ID
file-name | The physical file name of the data set.
ida-data | Indirect access address of CCW data.
iedb | The I/O error data block (z/OS only)
ioba | I/O control block address for failing I/O.
link-name | The DD name of the data set.
num-rabn | The number of RABNs for this part of the failing I/O operation.
oper | The type of operation being performed when the failure occurred as follows: Read or Write
sns | Additional sense byte data.
start-num | The start RABN for this part of the failing I/O operation.
start-rabn | The start RABN of the failing I/O operation.
tcw | The TCW, TCCB and TIDAL data for the I/O.
tcwa | TCW address of failing I/O.
For more information on TCW, CSW and sense data, please refer to the relevant IBM publication.
Action | When preceded by message ADAI40, no further action is required. When preceded by message ADAI35, use the information provided by the message to locate a possible hardware failure. Keep the information and any dumps for later use. If no hardware failure occurred, please contact your Software AG technical support representative for assistance.

ADAI42 | zHPF enabled for I/O requests on supported devices
Explanation | Note: This message is available in z/OS systems only. zHPF has been enabled on the operating system. I/O to data sets opened in zHPF mode, on devices which support zHPF, will now use zHPF channel programs. This message is only issued after a previous ADAI40 message.
Action | No action is required for this informational message.

ADAI44 | Storage at [address] length [length] {is | is not} backed by fixed 1MB large pages | {is | is not} backed by pageable 1MB large pages | {is | is not} backed by fixed 2GB large pages | is backed by pageable 4KB pages
Explanation | A 64-bit virtual storage area was allocated with the address and length indicated in the message. Different message endings appear using this message ID, depending on the type of storage requested and the type of storage allocated. The following table lists the possible messages, their cause, and recommended actions you can take when they occur.
Message Ending | Description | Action
--- | --- | ---
"is backed by fixed 1MB large pages" | Storage backed by fixed 1M large pages was requested via ADARUN parameters; 1M large pages are successfully being used to back the storage. | No action is required for this informational message.
"is not backed by fixed 1MB large pages" | Storage backed by fixed 1M large pages was requested via ADARUN parameters, but this request was not successful. Either the system does not support fixed 1M large pages or insufficient fixed 1MB large pages were available. Instead, the allocated storage is backed by pageable 4K pages. | Consider the following actions: If your system does not support large pages, do not use the ADARUN parameter causing the attempt to allocate using large pages. Remove it from the startup JCL of the job. If your system does support large pages of the type requested, consider increasing the number of fixed large pages specified for your operating system using the LFAREA parameter in PARMLIB member IEASYSxx. Contact your system administrator for assistance. For more information, read your IBM MVS Initialization and Tuning documentation.
"is backed by pageable 1MB large pages" | Storage backed by pageable 1M large pages was requested via ADARUN parameters; 1M large pages are successfully being used to back the storage. | No action is required for this informational message.
"is not backed by pageable 1MB large pages" | Storage backed by fixed 1M large pages was requested via ADARUN parameters, but this request was not successful. Either the system does not support pageable 1M large pages or insufficient pageable 1MB large pages were available. Instead, the allocated storage is backed by pageable 4K pages. | Consider the following action: If your system does not support large pages, do not use the ADARUN parameter causing the attempt to allocate using large pages. Remove it from the startup JCL of the job.
"is backed by fixed 2GB large pages" | Storage backed by fixed 2G large pages was requested via ADARUN parameters; 2G large pages are successfully being used to back the storage. | No action is required for this informational message.
"is not backed by fixed 2GB large pages" | Storage backed by fixed 2G large pages was requested via ADARUN parameters, but this request was not successful. Either the system does not support fixed 1G large pages or insufficient fixed 2GB large pages were available. Instead, the allocated storage is backed by pageable 4K pages. | Consider the following actions: If your system does not support large pages, do not use the ADARUN parameter causing the attempt to allocate using large pages. Remove it from the startup JCL of the job. If your system does support large pages of the type requested, consider increasing the number of fixed large pages specified for your operating system using the LFAREA parameter in PARMLIB member IEASYSxx. Contact your system administrator for assistance. For more information, read your IBM MVS Initialization and Tuning documentation.
"is backed by pageable 4KB pages" | Storage backed by pageable 4K pages was requested; pageable 4K pages are successfully allocated. If 1M or 2G large pages were requested, this message appears on the operator console and on DDPRINT. If 4K pages were requested, this message appears on DDPRINT only. | No action is required for this informational message.
Action | Refer to the specific message ending in the table above to determine what action, if any, is necessary.

ADAI51 | dbid Adabas PAM BS2000 I/O error err-num in file file-name
- Explanation | BS2000 systems only: A PAM I/O error occurred on DASD file file-name. This message is issued in conjunction with message ADAI52. err-num is the DMS error code. The explanation for the error can be found out using the following online command:
      HELP-MESSAGE DMS<err-num>
file-name is the file name in which the error occurred.
Action | Use the command /HELP-MESSAGE DMS<err-num> to describe the I/O error.

ADAI52 | RABN=error-rabn (start-rabn) OP=op-code ST=fecb
- Explanation | BS2000 systems only: A PAM I/O error occurred on DASD file file-name. This message is issued in conjunction with message ADAI51. error-rabn is the RABN where the error occurred. start-rabn the RABN where the operation began. op-code comprises one or more of the following operation code values:
  X'80' | READ read operation
  X'40' | WRITE write operation
  X'20' | FORMAT format operation
  X'10' | ENDOFTRK read or write to track end
  X'08' | RENOWRT no write if read-only nucleus
fecb is the FECB block status used for the I/O error, and comprises the SENSE, GERAETE (device), ABM and NPA fields. For more information, contact your Software AG technical support representative.

ADAI53 | dbid Adabas BS2000 I/O error err-num in file file-name
Explanation | BS2000 systems only: This is the first part of an I/O error message. The message is followed by message ADAI54. The err-num is a BS2000 error code. The file-name shows the link name for the failed data set.
Action | Use the command `/HELP-MESSAGE DMS <err-num>` to describe the I/O error.

ADAI54 | dbid Exit=value, status=fcb-status
Explanation | BS2000 systems only: The value is the error exit byte of the BS2000 FCB. fcb-status is a six-byte status containing the following:
byte 0: | device byte
bytes 1-3: | sense bytes 1-3
byte 4: | executive flag byte
byte 5: | count of processed PAM pages

ADAI55 | dbid Solsig error R15=ret-code, post-code=post-code
Explanation | BS2000 systems only: The system received an invalid return code (ret-code) or post code (post-code) when issuing a Solsig WAIT supervisor call (SVC). dbid is the database ID.
Action | Refer to the BS2000 System Macros manual for information about the return code.

ADAI56 | dbid Unexpected RC ret-code from macro
Explanation | BS2000 systems only: The data set assigned to SYSDTA is either a non-SAM/V data set, or it contains records longer than 80 bytes. The value macro is RDATA.

ADAI57 | dbid Unable to load ADAIOS
Explanation | An attempt to load ADAIOS failed. Check your LOADLIB and your partition sizes; either the partition is too small or the ADAIOS member is missing from the LOADLIB.

ADAI5X | dbid Subtask name started with TSN xxxx
Explanation | The subtask listed in the message (name) started with the TSN shown in the message (xxxx). Note: This message occurs in BS2000 environments only.
Action | No action is required for this informational message.

ADAI62 | dbid Allocation error - type x retcode ret-code dbid subcode subcode dataset physical-file-name
Explanation | An attempt to allocate a file dynamically failed. x indicates the request type: A (allocation); D (deallocation); or I (information retrieval). The ret-code and subcode display the error code returned from the operating system.
Action | Interpret the error code for your system and respond accordingly.

ADAI64 | dbid {File ddname | Dataset dsn} is being opened in mode mode Block size blksize RABN range start-RABN to end-RABN {File ddname | Dataset dsn} is encrypted
Explanation | The file (ddname) or dynamically allocated data set (dsn) is being opened in the mode (mode) given in the message (CKD, ECKD or zHPF). The file resides on a storage control device that supports count key data (CKD), extended count key data (ECKD) or high performance FICON (zHPF) channel commands. Adabas generates channel programs accordingly. The block size (blksize) of the data set is given in the message. It contains the blocks with numbers start-RABN through end-RABN. If the dataset is encrypted, an additional message line is generated to indicate this.
Action | No action is required for this informational message.

ADAI65 | dbid EXCPVR is [NOT] being used for this run [in ESA64 mode ]
Explanation | z/OS systems only: If ADAIOR is loaded from an APF-authorized library concatenation, and ADARUN is linked with the SETCODE AC(1) statement, ADAIOR then performs the channel program translation/page fixing. If "NOT" appears in the message, ADAIOR will not perform channel program translation and page-fixing to improve the performance of I/O operations. If EXCPVR is in use, and the operating system and processor support the allocation of real storage above the 2 gigabyte line, "in ESA64 mode" appears in the message.
Action | None required. This message is for your information only. If the message says that EXCPVR is not being used, but you have set up ADAIOR in an APF-authorized library and linked ADARUN with SETCODE AC(1) to use EXCPVR, refer to the Adabas Installation documentation for more information.

ADAI66 | dbid ADAIO2 error-code message
Explanation | The error-code is the Fujitsu Technology Solutions macro return code. The message is one of the following produced by the database main task while attempting to start a subtask:
            enabling subtask COM memory
            Enabling wait on contingency
            Enabling Wait
            Entering Job
            Get parameter memory
            Get submit file
            Opening submit file
            SET FILE LINK
            STXIT call error
The main task may not be accessible or has terminated.
Action | Contact your Software AG technical support representative.

ADAI67 | dbid ADAI2S error-code message
Explanation | The error-code is the Fujitsu Technology Solutions macro return code. The message is one of the following produced while attempting to start a subtask in the subtask startup module:
Message | Description
--- | ---
no mother task common memory | The memory pool containing data from the mother task is not accessible. The mother task has timed out or terminated.
no enable to mother's event | Mother task-to-subtask communication cannot be established. The mother task has probably terminated.
cannot share mother's low memory | The subtask parameter address area cannot be accessed.
cannot load subtask <subtask-name> | An error occurred while loading the subtask. Check the DDLIB and BLSLIBnn link names for libraries containing the subtask name (subtask-name) given in the message.
cannot post mother program | Communication with the mother task is no longer possible. The mother task has probably terminated.
STXIT definition error | A system error occurred while establishing the ESTAE(STXIT) exit for the subtask. Check the system resources.

ADAI68 | dbid ADAIO2 message
Explanation | Note: This message appears in BS2000 systems. The message providing information about BS2000 subtasks is one of the following:
    DISABLING SUBROUTINE subtask-number subtask-startname
The subtask with the number and startup name specified is being disabled.
    SUBTASK POSTED RC: return-code
The subtask posted the specified return code.
Action | If this message occurs because of regular disabling processing, such as through the use of the ADAEND command, no action is required. If this message occurs because of an unexpected error, then either the additional message "SUBTASK POSTED RC: return-code" is printed or additional messages can be found in the subtask-specific protocol. In this case, contact your Software AG technical support representative for assistance.

ADAI69 | ADALNK is running in mode mode
Explanation | Note: This message appears in BS2000 systems. ADALNK writes this message to tell you the mode it thinks it is running in where mode is one of the following:
BATCH/TIAM | batch or Fujitsu Technology Solutions as carrier
UTM/3GL/AMS | on UTM with an Assembler or 3rd generation language such as COBOL, C, FORTRAN, etc.
UTM/NATURAL | on UTM running Natural
Note: To suppress this message, set the B2CONFIG parameter in SSFB2C: LNKMSG=NO
Action: | No action is required for this informational message, although you can use this message for diagnosing errors.

ADAI6U | File: llllllll, GCB Blksz nnnnnnnnnn > physical mmmmmmmmmm, decrease or format
Explanation | BS2000 only: For ASSO or DATA containers, the declared size nnnnnnnnnn is larger than the physical size mmmmmmmmmm for the container on link name llllllll. This happened after running the ADADBS INCREASE utility function or a wrong declaration of the size when the container was defined with the ADADEF utility. This can lead to I/O errors and database maintenance problems. It is no longer possible to start the nucleus or run Adabas utilities other than the ADADBS, ADAFRM or ADAREP utilities.
Action: | Either run the ADADBS DECREASE utility function with a size of `nnnnnnnnnn - mmmmmmmmmm` blocks or run the ADAFRM utility with FROMRABN=NEXT and a size of `nnnnnnnnnn - mmmmmmmmmm`.

ADAI6Y | file DDttttRn Device-Type 8f extension needs DEVICE=23xx
Explanation | BS2000 only: An 8f device is required for the file named in the message (file). Other substitutions in the message are:
tttt | The Adabas component type. Possible values are "ASSO", "DATA", or "WORK".
n | The device number. Possible values range from "1" through "99".
xx | The valid 8f device type. Possible values range from "00" through "02".
Note: To avoid receiving this message, set the ADARUN ALLOW8F parameter to "Y".
Action: | No action is required for this informational message, although you can use this message for diagnosing errors.

ADAI70 | {DDCARD | DDKARTE} has invalid attribute {RECFM=x | LRECL=n }
Explanation | Note: This message occurs only in z/OS environments. During a request to open DDCARD or DDDRUCK, an invalid record format or record length has been detected. DDCARD and DDDRUCK are required to be in fixed record format (RECFM=F), with a record length of 80 bytes (LRECL=80).
Action: | Correct the error and rerun the job.

ADAI71 | Error nn writing console message type x length nnnn
Explanation | An error has occurred processing a request to write a message to the console.
Action: | Contact your Software AG technical support representative for assistance.

ADAI73 | dbid Warning: ddname dataset dsn dbid has been added since nucleus start-up. dbid ddname is now required in the JCL of all nucleus and dbid utility jobs for this database.
Explanation | The file or data set listed in the message (ddname or dsn) has been dynamically allocated and added to ASSO or DATA during this nucleus session. All subsequent jobs for this database need the added DD name (ddname) in the JCL. This message is displayed at nucleus termination.
Action: | Verify that the added data set has been included in the JCL for all nucleus and utility jobs for this database. If it has not, add appropriate JCL statements for the new data set to the jobs.

ADAI75 | File ddname {add | increase | decrease} {requested | detected} nnnnn {cylinders | blocks} dataset dsn
Explanation | This message appears when either of the following situations has occurred: The Adabas nucleus issued a request to add a new ASSO or DATA data set comprising the listed number of cylinders (nnnnn) or to increase the size of the final ASSO or DATA data set by the listed number of cylinders or blocks. An Adabas utility detected that a new ASSO or DATA data set comprising the listed number of cylinders (nnnnn) has been added or the size of the final ASSO or DATA data set has been increased by the listed number of cylinders or blocks. The Adabas nucleus issued a request to decrease the size of ASSO or DATA by the listed number of cylinders or blocks. For an add request, the data set name requested is also listed in the message (dsn).
Action: | No action is required for this informational message.

ADAI76 | File ddname {add | increase | decrease} activated
Explanation | A previous request has been activated to add a new ASSO or DATA data set, increase the size of the final ASSO or DATA data set, or decrease the size of the ASSO or DATA data set. For an add or increase, the database is now ready to make use of the additional space. For a decrease, the areas of ASSO or DATA affected are no longer available to the database. The DD name (ddname) associated with the data set is given in the message.
Action: | No action is required for this informational message.

ADAI77 | File ddname {add | increase | decrease | revoke | activate} request failed rc cc/rsn
Explanation | A request has failed to add a new ASSO or DATA data set, increase the size of the final ASSO or DATA data set, decrease the size of ASSO or DATA, or to revoke or activate a previous request. The DD name (ddname) of the data set, the return code (cc) and the reason code (rsn) are given in the message.
Action: | If an add, increase or decrease request fails, the nucleus will continue running with the existing ASSO and DATA data sets and data set sizes. If a revoke or activate request fails, the nucleus will terminate abnormally (internal error).

ADAI78 | File ddname {add | increase | decrease} request revoked
Explanation | A previous request has been revoked to add a new ASSO or DATA data set, increase the size of the final ASSO or DATA data set. or decrease the size of ASSO or DATA. An add, increase. or decrease request may be revoked if an error occurs after the request has been issued. The DD name (ddname) associated with the data set is given in the message. The nucleus will continue running with the existing ASSO and DATA data sets and data set sizes.
Action: | No action is required for this informational message.

ADAI79 | Preparing to extend ddname by nnnnn {cylinders | blocks}
Explanation | This message appears during initialization of a request to extend the ASSO or DATA data set by the listed size (nnnnn). The space requested is provided either in cylinders or in blocks. The DD name (ddname) associated with the final data set comprising the ASSO or DATA database component (containers) is given in the message.
Action: | No action is required for this informational message.

ADAI83 | {ENQ | DEQ} failed for {DDPRINT | DDDRUCK} return code nnnn reason code nnnn
Explanation | Note: This message occurs only in z/OS environments. An ENQ or DEQ failure occurred when writing a print line to DDPRINT or DDDRUCK.
Action | Contact your Software AG technical support representative for assistance.

ADAI84 | Write to {DDPRINT | DDDRUCK} failed - {SYNAD exit driven | abend code nnnnnnnn } All further writes to {DDPRINT | DDDRUCK} will be ignored
Explanation | Note: This message occurs only in z/OS environments. An attempt to write to DDPRINT or DDDRUCK has failed. The job will continue processing normally, but no further writes to DDPRINT or DDDRUCK will be attempted. Note that, if the Adabas nucleus issues this message for DDPRINT, Adabas shutdown statistics on DDPRINT will be lost.
Action: | Investigate the cause of the error using the diagnostic information supplied in the message. If the error resulted from a file full condition, consider increasing the size of the file for future Adabas nucleus or utility jobs.

ADAI85 | Resource Manager page-free request successful
Explanation | Note: This message occurs only in z/OS environments. A Resource Manager invoked during termination has successfully page-freed areas of page-fixed storage. This message may appear at termination following an abnormal end or cancel request.
Action: | No action is required for this informational message.

ADAI86 | Resource Manager page-free request unsuccessful Return code nnnnnnnn Reason code nnnnnnnn
Explanation | Note: This message occurs only in z/OS environments. A Resource Manager invoked during termination has unsuccessfully attempted to page-free areas of page-fixed storage. This message may appear at termination following an abnormal end or cancel request.
Action: | Contact your Software AG technical support representative. If a system abend occurred, ensure that the dump is available for problem diagnosis

ADAI87 | Resource Manager input parameter invalid
Explanation | Note: This message occurs only in z/OS environments. A Resource Manager invoked during termination was unable to attempt to page-free areas of page-fixed storage. This message may appear at termination following an abnormal end or cancel request.
Action: | Contact your Software AG technical support representative. If a system abend occurred, ensure that the dump is available for problem diagnosis

ADAI91 | Pause Element services initialized for zIIP
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has been successfully initialized. This message is issued only when Adabas is running with ADARUN parameter ZIIP=YES.
Action: | No action is required for this informational message.

ADAI92 | Pause Element services terminated {normally │ at abend │ for zIIP │ by Resource Manager}
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has been successfully terminated. This message is only issued when Adabas is running with ADARUN parameter ZIIP=YES. This message may appear at termination following an abnormal end or cancel request.
Action: | No action is required for this informational message.

ADAI93 | Pause Element {allocate │ deallocate │ pause │ release} error code ret code/rsn code
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has returned an error. The unexpected return code (ret code) and reason (rsn code) are shown. This message is only issued when Adabas is running with ADARUN parameter ZIIP=YES. This message may appear at termination following an abnormal end or cancel request.
Action: | If this message appears at termination following an abnormal end or cancel request, no action is required. In any other circumstances, save the JES log, DDPRINT output and any dump of the Adabas nucleus and Contact your Software AG technical support representative for assistance.

ADAI94 | Storage allocation warning - descriptor xxxx
Explanation | A storage allocation request which might result in storage fragmentation has been detected. For example, a small amount of storage is being allocated on a page boundary. Additional information on the length and type of storage being allocated is supplied on DDPRINT.
Action: | This is an informational message only, but, if it appears, users are requested to pass details of the message to their Software AG technical support representative for further assistance.

ADAI95 | Storage allocation error - descriptor xxxx rc nnnnnnnn
Explanation | A storage allocation request has failed with reason code nnnnnnnn. Additional information on the length and type of storage being allocated is supplied on DDPRINT. Further error messages may appear or an abnormal end might occur as a consequence of the storage allocation failure.
Action: | Users should review the message text and attempt to correct the condition, for example by providing more virtual storage for the job. If the message persists, users should contact their Software AG technical support representative for further assistance.