ADASM* Adabas SMF Processing Messages

#### Search Results

Search

# ADASM* Adabas SMF Processing Messages

### Overview of Messages

`ADASM1 | ADASM2 | ADASM3 | ADASM4 | ADASM5 | ADASM6 | ADASM7 | ADASMA | ADASMB`

ADASM1 | SMF=YES not allowed with MODE=SINGLE
Explanation | The specified ADARUN parameters are incompatible and cannot be specified at the same time in a nucleus startup job. The nucleus fails to initialize.
Action | Correct the ADARUN parameters and restart the nucleus.

ADASM2 | ADASMF unable to obtain storage
Explanation | Sufficient virtual storage for Adabas SMF is not available. The nucleus fails to initialize.
Action | Either increase the size of the nucleus region or disable SMF recording by setting the ADARUN SMF parameter to NO.

ADASM3 | SMF89 Registration return code rc
Explanation | The IBM z/OS service IFAUSAGE produced a non-zero return code when registering for type 89 SMF records. The nucleus initializes without registering for type 89 SMF records.
Action | The return codes are documented in the z/OS MVS System Management Facilities (SMF), IBM document SA22-7630. Contact your Software AG technical support representative if you are unable to understand the error. You may disable registration attempts by setting the ADARUN SMF89 parameter to NO.

ADASM4 | Invalid syntax of value for parm
Explanation | An error was detected in the syntax of the parameter named in the message (parm). The parameter may be an ADARUN parameter or an operator command operand. The invalid value is ignored.
Action | Remove or correct the specified parameter and try again.

ADASM5 | Unknown detail section dtl ignored
Explanation | An invalid Adabas SMF record detail section mnemonic was specified in an ADARUN parameter or an operator command operand. The invalid mnemonic is given in the message (dtl). The invalid value is ignored.
Action | Remove or correct the specified detail section mnemonic and try again.

ADASM6 | dtl detail section disabled, maximum size exceeded
Explanation | A single instance of the Adabas SMF record detail section listed in the message (dtl) exceeded the size that could be contained in a single Adabas SMF record. The specified detail section is disabled.
Action | If the detail section is a USER-type detail section, correct your SMF user exit. Otherwise, contact your Software AG technical support representative for assistance.

ADASM7 | Unknown SMF operator command
Explanation | The SMF operator command was not recognized. It is ignored.
Action | Specify a valid SMF operator command.

ADASMA | Unable to get interval, using 15 minutes
Explanation | The user specified ADARUN parameter `SMFINTERVAL=[SUBSYS | GLOBAL]`. ADASMF was unable to obtain a valid SMF interval from z/OS. A default interval was used. When the default interval expires, ADASMF will make another attempt to obtain the SMF interval.
Action | If this condition persists and you are not able to identify a cause, contact your Software AG Technical Support Representative for assistance.

ADASMB | Unable to set timer, interval records suspended
Explanation | ADASMF was unable to set a timer for the next interval record.
Action | Contact your Software AG Technical Support Representative for assistance. You may try Adabas operator commands to set `SMFINTERVAL` to `NONE` and then back to the original specification.