CORD* - Adabas System Coordinator Daemon Messages

#### Search Results

Search

# CORD* - Adabas System Coordinator Daemon Messages

CORDnn messages are issued by the Adabas System Coordinator daemon.

### Overview of Messages

`CORD01S | CORD02S | CORD03E | CORD04I | CORD05E | CORD06E | CORD07E | CORD08E | CORD09I | CORD10E | CORD11I | CORD12I | CORD13E | CORD14I | CORD15I | CORD16S | CORD17E | CORD18E | CORD19E | CORD20E | CORD21I | CORD22E | CORD23I | CORD24I | CORD25E | CORD26E | CORD27S | CORD28E | CORD29E | CORD30E | CORD31E | CORD33S | CORD34E | CORD35S | CORD36S | CORD37S | CORD38S | CORD39I | CORD40S | CORD41S | CORD42S | CORD43S | CORD44I | CORD45E | CORD46I | CORD47S | CORD49I | CORD50E | CORD51S | CORD52I | CORD53I | CORD54W | CORD56E | CORD57I | CORD58I | CORD59I | CORD60S | CORD61I | CORD62E | CORD63I | CORD64S | CORD65S | CORD66S | CORD70I | CORD71W | CORD72E | CORD73E | CORD74I | CORD75I | CORD76I | CORD77I | CORD78I | CORD79I | CORD80E | CORD81E | CORD82E | CORD83E | CORD84E | CORD85I | CORD86E | CORD88I | CORD89I | CORD90I | CORD91I | CORD92E | CORD93E`

CORD01S | CAS CANNOT INITIALIZE, GETMAIN ERROR
Explanation | The Adabas System Coordinator cannot initialize because of a memory shortage.
Action | Increase the region specification for the daemon job.

CORD02S | CAS CANNOT INITIALIZE, KERNEL LOAD ERROR
Explanation | The daemon failed to locate or load the runtime kernel module CORKRN.
Action | Ensure that the load library containing the kernel module is available to the job.

CORD03E | DDCARD OPEN ERROR: ## - TERMINATING
Explanation | The DDCARD control file could not be opened.
Action | Ensure that the daemon job has a DDCARD file containing the required control cards.

CORD04I | INPUT PARAMETER: #############
Explanation | The input parameters contained in the DDCARD file are echoed in the job message output file.
Action | None. This message is for information only.

CORD05E | INVALID PARAMETER: ###########
Explanation | An invalid input parameter was found in the DDCARD file. The daemon terminates.
Action | Correct or delete the invalid parameter.

CORD06E | PRODUCT PARAMETER NOT SPECIFIED
Explanation | There was no `PRODUCT`parameter in the DDCARD file. The daemon does not know which product(s) to load.
Action | Add the required `PRODUCT` parameter and restart the daemon.

CORD07E | MPM FAILURE - FUNCTION: ## ERROR ##
Explanation | An error occurred calling ADAMPM when trying to: initialize a target (Function=00) sign off from the Adabas SVC (Function=20) sign on to the Adabas SVC (Function=24)
Action | For a sign on error, navigate to the Daemon Group Parameters in the System Coordinator Online system and ensure that the correct SVC and Node ID have been specified for the Adabas System Coordinator group. A sign-off error indicates an internal problem with the System Coordinator Daemon. Contact your Software AG technical support representative for assistance. No action is required in the Coordinator Daemon.

CORD08E | IOR FAILURE - FUNCTION: ## ERROR ##
Explanation | An error occurred during an ADAIOR service call.
Action | Contact your Software AG technical support representative for assistance.

CORD09I | SHUTDOWN REQUESTED
Explanation | The daemon has received a shutdown request.
Action | None. This message is for information only.

CORD10E | GETMAIN FOR COMMAND QUEUE FAILED
Explanation | The daemon cannot acquire memory for the command queue.
Action | Increase the region specification for the Adabas System Coordinator daemon task.

CORD11I | CORD11I SYSCO ##### IS ACTIVE ON NODE ##### ### CIB=########
Explanation | The daemon successfully signed on to the Adabas SVC and is ready for communication. The message indicates the node and SVC number used.
Action | None. This message is for information only.

CORD12I | OPER TYPEIN: #################
Explanation | The operator entered a console command to the daemon. The command is echoed back to the message output file.
Action | None. This message is for information only.

CORD13E | INVALID OPERATOR COMMAND
Explanation | The command entered is not valid.
Action | Correct the command and enter it again.

CORD14I | TARGET ##### TERMINATION IN PROGRESS
Explanation | The daemon is terminating because of operator request or unrecoverable error.
Action | None. This message is for information only.

CORD15I | TARGET ##### ENDED NORMALLY
Explanation | The daemon terminated normally as a result of an operator request.
Action | None. This message is for information only.

CORD16S | TARGET ##### ENDED ABNORMALLY
Explanation | The daemon terminated abnormally as a result of a previous error.
Action | A previous message will identify the cause of the abnormal termination. Examine the message and take appropriate recovery action.

CORD17E | PRODUCT ### DUPLICATED
Explanation | The daemon has detected multiple copies of the PRODUCT= card for a single product.
Action | Remove the duplicate entries and restart the daemon.

CORD18E | TOO MANY PRODUCTS SPECIFIED
Explanation | The daemon has detected too many copies of the PRODUCT= card.
Action | Correct the PRODUCT= cards and restart the daemon.

CORD19E | PRODUCT ### - WORK AREA CANNOT BE ALLOCATED
Explanation | This is an internal error.
Action | Contact your Software AG technical support representative for assistance.

CORD20E | INVALID PARAMETERS - TERMINATING
Explanation | The daemon has detected invalid parameter cards and has shut down.
Action | Correct the parameter cards and restart the daemon.

CORD21I | OPERATOR COMMAND PROCESSED SUCCESSFULLY
Explanation | An operator command completed successfully.
Action | None. This message is for information only.

CORD22E | LOAD FOR MODULE: ######## FAILED
Explanation | The requested module could not be located or loaded.
Action | Ensure that the requested module is available to the Adabas System Coordinator daemon task.

CORD23I | PARAMETERS FOR THIS RUN:
Explanation | The parameters in use in this instance of the daemon.
Action | None. This message is for information only.

CORD24I | ################ = ################
Explanation | Along with CORD23I gives details of the parameters in use in this instance of the daemon.
Action | None. This message is for information only.

CORD25E | ### IS AN INVALID PRODUCT NAME
Explanation | The daemon has detected invalid an invalid product name.
Action | Correct the product name and restart the daemon.

CORD26E | PROXY MODULE ######## WAS NOT FOUND, PRODUCT ### WILL NOT BE CALLED
Explanation | The daemon has been told to run with PRODUCT=nnn but cannot find nnnPXY.
Action | Ensure the daemon has access to all the products required and restart the daemon.

CORD27S | INVALID PRODUCT TABLE ENTRY FOR ###
Explanation | This is an internal error.
Action | Contact your Software AG technical support representative.

CORD28E | CAS PROXY MODULE ######## FOR PRODUCT ### IS INVALID (BAD EYECATCHER)
Explanation | The requested module could not be located or loaded.
Action | Contact your Software AG technical support representative.

CORD29E | CAS PROXY MODULE ######## FOR PRODUCT ### IS NOT SUPPORTED BY THIS VERSION OF CAS
Explanation | This is an installation error.
Action | Ensure that all product libraries used in the daemon are the same version.

CORD30E | GETMAIN FOR PRODUCT PARM BLOCK FAILED
Explanation | A memory allocation failed during the initialization.
Action | Increase the region specification for the job.

CORD31E | CAB ALLOCATION ERROR IN MODULE SYSCORU
Explanation | A memory allocation failed during the initialization of the daemon.
Action | Increase the region specification for the job.

CORD33S | APPEND OF PRODUCT V-CON LIST FAILED.
Explanation | Explanation This is an internal error.
Action | Contact your Software AG technical support representative.

CORD34E | ASA ALLOCATION ERROR IN MODULE SYSCORU
Explanation | A memory allocation failed during the initialization of the daemon.
Action | Increase the region specification for the job.

CORD35S | CONFIGURATION MODULE ###### CORCFG CANNOT BE LOCATED
Explanation | The configuration module cannot be loaded. This module contains the SVC, DBID, and file number for reading the configuration file. The daemon will not function correctly without this module.
Action | Refer to the Adabas System Coordinator Installation documentation for information about assembling a configuration module.

CORD36S | SVC/NODE DDCARD INPUT IS INVALID WITH PRODUCT=CAS
Explanation | This is an internal error.
Action | Contact your Software AG technical support representative.

CORD37S | SYSCO DAEMON member-name NOT FOUND IN CONFIGURATION FILE, RESPONSE=nnnn, SUBCODE=nnnn
Explanation | The named Adabas System Coordinator group member was not found in the group in the configuration file. Every daemon must have an equivalent group member parameter.
Action | Add the member entry for this daemon to the appropriate Adabas System Coordinator group.

CORD38S | GROUP group-name NOT FOUND IN CONFIGURATION FILE, RESPONSE=nnnn, SUBCODE=nnnn
Explanation | The named group cannot be located.
Action | An error occurred while searching for the Adabas System Coordinator group parameters. Define the Adabas System Coordinator group. If the problem persists, contact your Software AG technical support representative.

CORD39I | SHUTDOWN PENDING
Explanation | A shutdown request was entered. One or more of the subcomponents of the Adabas System Coordinator daemon suspended the request until it completes its own shutdown processing. The daemon should terminate when this is completed.
Action | None. This message is for information only.

CORD40S | ABEND #### PSW ######## ########
Explanation | An error occurred in the Adabas System Coordinator daemon. The registers, PSW, and failing module at the time of the error are displayed. The Adabas System Coordinator writes additional diagnostic information to the CORDUMP file, deletes any common memory pools in use, and terminates.
Action | Contact your Software AG technical support representative.

CORD41S | CSECT ######## ENTRY ######## OFFSET ########
Explanation | Additional information to CORD40S.
Action | Contact your Software AG technical support representative.

CORD42S | MODULE ######## ENTRY ######## OFFSET ########
Explanation | Additional information to CORD40S.
Action | Contact your Software AG technical support representative.

CORD43S | REGS ##### ######## ######## ######## ########
Explanation | Additional information to CORD40S.
Action | Contact your Software AG technical support representative.

CORD44I | PROXY ######## LOADED AT ########
Explanation | The address of the named proxy module.
Action | None. This message is for information only.

CORD45E | THREAD ######## TIMEOUT, TARGET=#####, USER=########
Explanation | The Adabas System Coordinator daemon sent an Adabas command to the indicated target, and has not received a response within the timeout interval as specified by DDCARD parameter `CT`.
Action | Check that the target database is operating correctly. If the problem persists, try increasing the `CT` timeout value. If there is still a problem, contact your Software AG technical support representative.

CORD46I | ######## Start pending, configuration file (dbid ##### fnr #####) not active
Explanation | An Adabas System Coordinator daemon has been started, but the required configuration file is not active. The daemon will wait for 60 seconds and try again. If the configuration file is still not active after 60 minutes the daemon will terminate.
Action | Start the database that contains the configuration file.

CORD47S | Halt-Load library is not Authorized
Explanation | z/OS only. An Adabas System Coordinator daemon has been started from a load library that is not APF-authorized.
Action | Ensure the specified load library is authorized and restart the daemon.

CORD49I | PRODUCT COMPONENT ENDED - ###
Explanation | The named product has ended.
Action | None. This message is for information only.

CORD50E | Shutdown rejected
Explanation | A daemon shutdown request was made, but there are active client DTR jobs connected to the daemon. This message will be preceded by message CAS004I, identifying the names of the active DTR job(s).
Action | Terminate the active client jobs and re-issue the shutdown request.

CORD51S | XCF CQ OVERFLOW – DAEMON RESTARTED
Explanation | There has been an overflow in the XCF command queue (see NXC parameter) of the current daemon resulting in a daemon restart.
Action | None. This message is for information only and indicates an exceptionally high volume of XCF messages in this System Coordinator group.

CORD52I | Configuration file: database / file
Explanation | This message shows the database ID and file number of the configuration file in use by this System Coordinator daemon.
Action | None. This message is for information only.

CORD53I | Alternate file : database / file
Explanation | This message shows the database ID and file number of the alternate configuration file in use by this System Coordinator daemon. The message only appears if an alternate configuration file has been specified.
Action | None. This message is for information only.

CORD54W | ######## shutdown rejected, configuration file ##### / ##### not active
Explanation | An Adabas System Coordinator daemon has been instructed to terminate, but an alternate configuration file is in use and one or both configuration files is not active. Both configuration files must be available at daemon termination.
Action | Ensure that the configuration file database(s) are active.

CORD56E | Latency file error: ###### - #################### rc=########
Explanation | A latency file error has occurred in the Adabas System Coordinator daemon. The message indicates the function attempted, the reason for failure, and a return code. Some of the more common reasons for failure are listed below, otherwise contact your Software AG technical support representative.
Action | "BR allocation failure" – review/increase the size of the COLAT latency file. "### getmain failure" - review and increase the storage available in the daemon region.

CORD57I | Recovery for ######## found ######## sessions at rest
Explanation | The Adabas System Coordinator daemon has been restarted after a failure and full crash recovery was active at the time of failure for the job/service indicated. This message identifies the number of sessions recovered for the services/job so they can continue without interruption if possible.
Action | This message is for information only, no action is needed.

CORD58I | Service AbTerm resource manager termination-type term
Explanation | The System Coordinator daemon resource manager was invoked at address-space (termination-type indicates AddrSpc) or task (termination-type indicates Task) termination .
Action | None. This message is for information only.

CORD59I | Resource manager activation failed, rc=hhhhhhhh
Explanation | The System Coordinator daemon was unable to activate its resource manager. hhhhhhhh indicates a reason for the failure.
Action | The daemon continues without its resource manager. Contact Software AG support to establish the reason for the failure.

CORD60S | Failure: Continuous Operation has been initiated for ###
Explanation | A failure has occurred in the component identified in the message. Continuous operation processing has been invoked to restart the appropriate component(s).
Action | None. This message is for information only.

CORD61I | ### STORAGE AREA RELEASED
Explanation | This is an information message during continuous operation recovery.
Action | Report it to your Software AG technical support representative.

CORD62E | Continuous operation error: ################### rc=#######
Explanation | The System Coordinator daemon was attempting to recover following a failure but an error occurred trying to do so.
Action | Contact your Software AG technical support representative.

CORD63I | Continuous operation recovery for ######## found ######## sessions at rest
Explanation | The Adabas System Coordinator daemon was restarted following a failure and has recovered the job/service indicated. This message identifies the number of sessions recovered for the services/job so they can continue without interruption.
Action | None. This message is for information only.

CORD64S | Shutdown activated owing to recursive failure
Explanation | There has been more than one failure in a period of 30 minutes. Continuous operation is abandoned and the daemon terminates.
Action | None. This message is for information only.

CORD65S | SHARED MEMORY ANCHOR AT ########
Explanation | Issued at startup of a Coordinator daemon, this message displays the address of the daemon’s shared memory anchor.
Action | None. This message is for information only.

CORD66S | SHARED MEMORY GETMAIN FAILED
Explanation | Issued at startup of a Coordinator daemon, when it has been configured to use shared memory for latency/pulse services but the attempt to allocate shared memory failed.
Action | The daemon continues, using private memory for latency services (pulse services are disabled). Review the daemon’s shared memory definitions and ensure that sufficient shared memory is available. Consider using a dataspace in preference to standard shared memory.

CORD70I | Resource Size Current Highwater
Explanation | CORD70I messages are displayed in response to a `DRES` operator command and show allocated size, current usage and high-water mark for various daemon resources.
Action | None. This message is for information only.

CORD71W | WARNING – XCF CQ 80% FULL
Explanation | This is a one time only warning message that the XCF command queue is 80% full, potentially a sign of an imminent overflow.
Action | Use the `DRES` operator command to monitor the `XCF` command queue. If a high percentage continues to be in use, this may indicate a high number of updates to files being optimized by Adabas Fastpath . This is not recommended and should be investigated. Note that if the number continues to increase then an overflow will occur when the maximum `XCF` command queue entries is reached, resulting in a CORD51S message and daemon auto-restart.

CORD72E | MPM FAILURE - FUNCTION: ## ERROR ## JOB=######## SESSION=################
Explanation | An error occurred calling ADAMPM when trying to: Get the command queue element (CQE) (Function=08) Post command completion to caller (Function=12) Timeout (Function=36)
Action | This message indicates a problem with the daemon caller. The message identifies the calling Job and Session ID. It may also be accompanied by an Adabas "User Gone" message (ADAM91 or ADAM92), also identifying the calling Job and Session ID. Examine the calling job to determine the reason for the failure. Probably the job has abnormally terminated. No action is required in the Coordinator Daemon.

CORD73E | Command permitted only for zIIP-enabled daemon
Explanation | The use of this operator command requires zIIP support to have been activated in the Daemon.
Action | In order to activate zIIP support for the Daemon, set ZIIP=YES in the Daemon runtime parameters.

CORD74I | zIIP-related statistics: Daemon is executing in {SRB | TCB} mode … (processor-related statistics) … … (CPU consumption statistics) … … (SRB/TCB use statistics) … … (extended pause/release statistics) … … (type-of-work statistics) …
Explanation | In response to the operator command DZSTAT, these messages display the zIIP-related statistics of the Daemon. The first line shows the current execution mode: "SRB" (execution on zIIP enabled) or "TCB" (execution on zIIP disabled). The following statistics correspond, and are equivalent to, the zIIP-related statistics at the end of the Daemon session statistics. Refer to Monitoring zIIP Usage in section "Adabas System Coordinator for zIIP"in the Adabas System Coordinator documentation for detailed information about the various statistical figures.
Action | None. This message is for information only.

CORD75I | Daemon is now executing in TCB mode
Explanation | In response to the operator command ZIIP=NO, this message indicates the Daemon is now executing in TCB mode (disabling the use of System z Integrated Information Processors). The ZIIP parameter value was changed to NO, from YES.
Action | None. This message is for information only.

CORD76I | Daemon is already executing in TCB mode
Explanation | In response to the operator command ZIIP=NO, this message indicates the Daemon was already executing in TCB mode (disabling the use of System z Integrated Information Processors). The ZIIP parameter value was not changed; it was already NO.
Action | None. This message is for information only.

CORD77I | Daemon is now executing in SRB mode
Explanation | In response to the operator command ZIIP=YES, this message indicates the Daemon is now executing in SRB mode (enabling the use of System z Integrated Information Processors). The ZIIP parameter value was changed to YES, from NO.
Action | None. This message is for information only.

CORD78I | Daemon is already executing in SRB mode
Explanation | In response to the operator command ZIIP=YES, this message indicates the Daemon was already executing in SRB mode (enabling the use of System z Integrated Information Processors). The ZIIP parameter value was not changed; it was already YES.
Action | None. This message is for information only. .

CORD79I | Operator command not executable
Explanation | The command entered is not executable.
Action | This message should be preceded by another message which explains the reason why this command could not be executed.

CORD80E | Unable to check license
Explanation | An internal error has occurred during license validation processing.
Action | First verify that the LICMAIN (MLC) module is available in the STEPLIB, otherwise increase the region size available to the Adabas System Coordinator Daemon..

CORD81E | Error opening license file (DDLAZPAD)
Explanation | An error occurred opening the license file specified by the DDLAZPAD statement.
Action | Omit the DDLAZPAD statement and use the load module method of licensing instead.

CORD82E | Error reading license file (DDLAZPAD)
Explanation | An empty file or invalid record structure was detected.
Action | Verify that the license file has been copied correctly to the license data set. The file should not be empty and the data should not have been converted to EBCDIC (it should be in ASCII format).

CORD83E | License file size exceeds limit
Explanation | The license being read is larger than expected.
Action | Verify that you are using the original license file obtained from Software AG.

CORD84E | Error license function fx subfunction sfx returned err
Explanation | An unexpected error occurred while performing the Adabas System Coordinator for zIIP license check. The license function (fx), subfunction (sfx) and return code (err) are given in the message.
Action | Examine the Adabas System Coordinator Daemon JCL and verify that the AZPAD license is available as load module AZPADLIC or is assigned with the link (DD) name DDLAZPAD.

CORD85I | License check completed
Explanation | The license check completed successfully and the Adabas System Coordinator Daemon is started.
Action | None. This message is for information only.

CORD86E | License check failed (AZPAD)
Explanation | The license file is physically correct, but some license property was found that did not match your Adabas System Coordinator Daemon execution environment. This is a final message, accompanied by another message specifying details of the failure. The Adabas System Coordinator Daemon is started but will execute in TCB mode (disabling the use of System z Integrated Information Processors). The ZIIP parameter value was changed to NO, from YES.
Action | Check the accompanying message(s) for the details of the failure. If necessary, contact your Software AG technical support representative.

CORD88I | …daemon statistics...
Explanation | In response to the operator command DSTAT, these messages display either general, disk or services related daemon statistics. Refer to the DSTAT operator command in section Daemon Operator Commands of the Adabas System Coordinator documentation for detailed information regarding the statistics provided.
Action | None. This message is for information only.

CORD89I | Connected to Cache Facility structure ################
Explanation | The daemon has succeeded in connecting to the named Cache Facility structure. This message is only applicable for members of a daemon group defined with a System Type of IBM Parallel Sysplex.
Action | None. This message is for information only.

CORD90I | COLAT Statistics:
Explanation | These messages are displayed at Daemon start-up and show general information about the size and usage of the COLAT latency disk file. Disk blocks are allocated on demand for Jobs/Services defined to use Disk Latency.
Action | None. This message is for information only.

CORD91I | CORD91I File ######## is encrypted
Explanation | The COR daemon runtime parameter ENCRYPTION is set to YES and the file/dataset being opened (denoted by ########) is encrypted.
Action | None. This message is for information only.

CORD92E | Loaded modules do not support ENCRYPTION
Explanation | The Adabas System Coordinator daemon runtime parameter ENCRYPTION is set to YES but the available modules are not correct and do not fully support Adabas Encryption. The Adabas System Coordinator daemon refuses to start.
Action | Review and correct the STEPLIB concatenation to ensure that the Adabas Encryption load library precedes the Adabas load library.

CORD93E | No licensed products are active
Explanation | The use of the LICREFRESH operator command requires either zIIP support and/or Encryption support to have been activated in the Adabas System Coordinator daemon.
Action | In order to activate zIIP and/or Encryption support for the Adabas System Coordinator daemon, set ZIIP=YES and/or ENCRYPTION=YES in the Adabas System Coordinator daemon runtime parameters.