ADAULD JCL/JCS Requirements and Examples

#### Search Results

Search

# ADAULD JCL/JCS Requirements and Examples

This section describes the job control information required to run ADAULD with BS2000/OSD, z/OS, z/VM, VSE/ESA and z/VSE systems and shows examples of each of the job streams.

This document covers the following topics:

- z/OS

## z/OS

Data Set | DD Name | Storage | More Information
--- | --- | --- | ---
Unloaded data | DDOUT1 | tape/disk | Output by ADAULD (see note)
Unloaded data | DDOUT2 | tape/disk | Output by ADAULD (see note)
Unloaded ISNs | DDISN | tape/disk | Required with DDISN
Full save tape | DDFULL | tape/disk | Required for full save tape
Delta save tape(s) | DDDEL1- DDDEL8 | tape/disk | Required for delta save tape(s)
Delta Save images | DDDSIMR1 | disk | Required for DSIM data set
Recovery log (RLOG) | DDRLOGR1 | disk | Required for ADARAI
ADAULD messages | DDDRUCK | printer | Adabas Messages and Codes
ADARUN messages | DDPRINT | printer | Adabas Messages and Codes
ADARUN parameters | DDCARD | reader | Adabas Operations
ADAULD parameters | DDKARTE | reader |

Note
DDOUT1 and DDOUT2 must have the same block size; otherwise, an ADAULD error will occur. DDOUT2 is required only if NUMOUT=2 is specified.

### z/OS Example

    //ULD       EXEC PGM=ADARUN
    //STEPLIB   DD   DISP=SHR,DSN=ADABAS.Vvrs.LOADLIB
    //*
    //DDOUT1    DD   DISP=(,KEEP),DSN=EXAMPLE.ADA99.OUT1,
    //          UNIT=SYSDA,VOL=SER=DISK01,SPACE=(TRK,200,RLSE)
    //DDFULL    DD   DISP=SHR,DSN=EXAMPLE.ADA99.FULLSAVE
    //DDDEL1    DD   DISP=SHR,DSN=EXAMPLE.ADA99.DELTA1
    //DDDEL2    DD   DISP=SHR,DSN=EXAMPLE.ADA99.DELTA2
    //SYSUDUMP  DD   SYSOUT=A
    //DDDRUCK   DD   SYSOUT=A
    //DDPRINT   DD   SYSOUT=A
    //DDCARD    DD   *
    ADARUN PROG=ADAULD,SVC=249,DEVICE=3390,DB=99,DSF=YES
    //DDKARTE   DD   *
    ADAULD    FILE=1,SAVETAPE,PATTERN=FDD