NETnnnn - Entire Net-Work Control Module Messages

#### Search Results

Search

# NETnnnn - Entire Net-Work Control Module Messages

Messages relevant to overall Entire Net-Work operation are listed below. Messages are either issued to the print data set or displayed at the operator console and logged to the print data set, as appropriate.

### Overview of Messages

`NET0001I | NET0002I | NET0003I | NET0004I | NET0005I | NET0006I | NET0007I | NET0008I | NET0009I | NET0010I | NET0011I | NET0013I | NET0014I | NET0015I | NET0016I | NET0017I | NET0018I | NET0019I | NET0020I | NET0021I | NET0022I | NET0023I | NET0024I | NET0025I | NET0026I | NET0027I | NET0028I | NET0029I | NET0031I | NET0032I | NET0033I | NET0034I | NET0035 | NET0036I | NET0037I | NET0038I | NET0039I | NET0040I | NET0041I | NET0042I | NET0043I | NET0044E | NET0045I | NET0051I | NET0052I | NET0060I | NET0061E | NET0062E | NET0063E | NET0064E | NET0086I | NET0087I | NET0088I | NET0089I | NET0090I | NET0091I | NET0092I | NET0093I | NET0094I | NET0095I | NET0096I | NET0097I | NET0098I | NET0099I | NET0101I | NET0103I | NET0104I | NET0105I | NET0106I | NET0107I | NET0108I | NET0109I | NET0110I | NET0111I | NET0112I | NET0113I | NET0114I | NET0115I | NET0116I | NET0117I | NET0118I | NET0119I | NET0120I | NET0121I | NET0122I | NET0123I | NET0124I | NET0125I | NET0126I | NET0127I | NET0128I | NET0129I | NET0130I | NET0131I | NET0133 | NET0134I | NET0135I | NET0136I | NET0137I | NET0139I | NET0141I | NET0144I | NET0145I | NET0146I | NET0147I | NET0148I | NET0149I | NET0150I | NET0151I | NET0153I | NET0154I | NET0155I | NET0170E | NET0171I | NET0172I | NET0174I | NET0175I | NET0177I | NET0178I | NET0179I | NET0180I | NET0181I | NET0182I | NET0183I | NET0184I | NET0185I | NET0190I | NET0191I | NET0200I | NET0201I | NET0240E | NET0241I | NET0242I | NET0243E | NET0244E | NET0245E | NET0246E | NET0247E | NET0250I | NET0251I | NET0306I | NET0308I | NET0322I | NET0328E | NET0333I | NET0334E | NET0335 | NET0336 | NET0337 | NET0338 | NET0339 | NET0340 | NET0341 | NET0342 | NET0343 | NET0346I | NET0404E | NET0998I | NET0999I | NET1000I | NET1001I | NET1002I | NET1003I | NET1004W | NET1005E`

NET0001I | Statement too long
Explanation | Entire Net-Work parameter statements, even though they may extend over multiple lines, may not be infinitely long. The current maximum for any one statement is approximately 4000 characters (not counting embedded comments). The statement in question is not interpreted; any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Try to abbreviate some keywords or eliminate some unnecessary blanks from the statement.

NET0002I | Invalid statement: aaaaaaaa
Explanation | The statement verb, aaaaaaaa, is not one of those recognized by Entire Net-Work (NODE, DRIVER, or LINK). The statement in question is not interpreted; any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Ensure correct coding of recognized statements; you may have coded a comment or a continuation line incorrectly.

NET0003I | Invalid keyword: aaaaaaaa
Explanation | A keyword parameter was coded (aaaaaaaa), that is not recognized in this statement. The statement in question is not interpreted beyond this point; it and any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Ensure correct coding of recognized keywords; note that the set of valid keywords is likely to be different between access methods, and between DRIVER and LINK statements of the same access method.

NET0004I | Invalid value for keyword: aaaaaaaa nnn
Explanation | There are certain constraints on valid values for some keyword parameters, such as: numeric values hexadecimal values YES or NO only, etc. In this case, parameter aaaaaaaa was not correctly specified. The nnn value in the message is specified for multiple value parameters only; if given, it specifies the position of the subparameter in error. The statement in question and any statements following it are scanned for errors; session initialization is aborted after all statements have been read.
Action | Refer to the section Entire Net-Work Parameter Statements in Entire Net-Work Reference for the allowed parameter values.

NET0005I | Duplicate NODE statement
Explanation | More than one NODE statement was coded in the parameter data set. The statement in question is not interpreted. Any statements following it are scanned for errors. Session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Eliminate all but one of the NODE statements from the parameter data set.

NET0006I | Invalid driver name: aaaaaaaa
Explanation | The value aaaaaaaa is not a valid line driver name. The statement in question is not interpreted; any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | For the valid name, see the documentation for the appropriate Entire Net-Work line driver: CTCA line driver in Entire Net-Work CTC Option Administration TCP/IP line driver in Entire Net-Work TCP/IP Option Administration VTAM line driver in Entire Net-Work Administration XCF line driver in Entire Net-Work XCF Option Administration Simple Connection Line Driver in Entire Net-Work TCP/IP Option Administration

NET0007I | Duplicate aaaaaaaa DRIVER statement
Explanation | More than one DRIVER statement was coded for the access method aaaaaaaa. The statement in question is not interpreted; any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Eliminate any extraneous DRIVER statements from the parameter data set.

NET0008I | aaaa Driver not available
Explanation | The NETaaaa line driver module could not be loaded from your libraries. This is either due to an error in specifying the line driver name, or the line driver is not installed in your libraries. The statement in question is not interpreted; any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may result from this error.
Action | Ensure that the driver NETaaaa is available and installed correctly, verify correct spelling, or check your JCL for correct library specifications.

NET0009I | More than nn values for keyword: aaaaaaaa
Explanation | More values than expected were coded for the multiple-value keyword parameter aaaaaaaa. The value nn is the maximum number of values permitted by the definition of the parameter. The statement in question and any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may be caused by this error.
Action | Refer to the section Entire Net-Work Parameter Statements in Entire Net-Work Reference for the allowed parameter values.

NET0010I | Required parameter not specified: aaaaaaaa nnn
Explanation | The keyword or positional parameter aaaaaaaa was either incorrectly specified or was missing. The value nnn is specified for multiple value parameters only; if given, it specifies the position of the missing subparameter. The statement in question and any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may be caused by this error.
Action | Refer to the section Entire Net-Work Parameter Statements in Entire Net-Work Reference for the allowed parameter values.

NET0011I | EOF found before end of statement
Explanation | The last statement line found before the end of the data set indicated that a continuation line was to be expected. The Entire Net-Work session is terminated abnormally.
Action | Correct the parameter statement.

NET0013I | Buffer pool init failed, RC=nn
Explanation | The Entire Net-Work Buffer Pool Manager failed to set up the buffer pools as specified in the BUFFERS keyword parameter on the NODE statement. Return codes of 20 and 24 indicate that the required amounts of memory were not available; other values indicate possible internal errors, and should be reported to your Software GmbH technical support representative. The Entire Net-Work session is terminated abnormally.
Action | Correct the condition that caused the buffer pool failure (provide enough storage in the partition or address space, provide enough real storage to permit page-fixing the page-fixed buffer pool, or consider reducing the buffer pool sizes).

NET0014I | Control block space unavailable
Explanation | A storage request for permanent control blocks failed. Permanent control blocks describing the network topology are not allocated from the buffer pools but obtained from the operating system instead. The Entire Net-Work session is terminated abnormally.
Action | Provide more storage in the partition or address space.

NET0015I | aaaa Driver init failed (RC=nn)
Explanation | Line driver initialization failed; an explanatory message should have been issued by the line driver. The return code (nn) is access method dependent; it may relate to possible internal errors. The statements following this DRIVER statement are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may be caused by this error.
Action | Refer to the access-method-specific messages for corrective action. If an internal error is indicated, have a system dump and any other documentation available and contact your technical support representative.

NET0016I | aaaa Driver not previously initialized
Explanation | A LINK statement referred to the access method aaaa, but either a DRIVER statement for aaaa was not specified, the specified line driver could not be loaded, or the driver initialization failed. Note that the DRIVER statement must appear before the LINK statement. The statement in question and any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may be caused by this error.
Action | Ensure that a DRIVER statement is before the LINK statement and that the LINK statement specifies the correct DRIVER statement name.

NET0017I | Duplicate link name: aaaaaaaa
Explanation | The names of all links on a node must be unique. The statement in question and any statements following it are scanned for errors; session initialization is aborted after all statements have been read. Note: Errors reported in subsequent statements may be caused by this error.
Action | Assign unique link names to all LINK statements on the node.

NET0018I | ADAMPM call nn failed
Explanation | An error occurred during interregion processing. Most likely, ADAMPM has also issued a NETMxx message to explain the problem; otherwise, an internal system error occurred. The call type is specified as nn. The Entire Net-Work session is terminated abnormally.
Action | Refer to the section ADAMPM Messages for details. If a system error occurred, have a system dump and any other documentation available, and contact your technical support representative.

NET0019I | Command queue space unavailable
Explanation | The storage request for the command queue (request queue) failed. The amount of storage necessary is (NC+1)*192 bytes, where NC is the value of the NC parameter in the ADARUN statement. The Entire Net-Work session is terminated abnormally.
Action | Provide more storage in the partition or address space or reset the NC parameter value. Note that the amount of storage required for the command queue is usually small compared to the overall storage requirements of Entire Net-Work.

NET0020I | Unresolved VCONS in driver module
Explanation | An internal error occurred; an incorrect line driver module was probably loaded. The Entire Net-Work session is terminated abnormally.
Action | Have the storage dump and/or dumps of the Entire Net-Work modules available, then contact your technical support representative.

NET0021I | Unexpected event indicator: xxxxxxxx
Explanation | An internal error occurred; an incorrect line driver module was probably loaded. The Entire Net-Work session is terminated abnormally.
Action | Have the storage dump and/or dumps of the Entire Net-Work modules available, then contact your technical support representative.

NET0022I | ACM work buffer shortage
Explanation | The access method working storage requests could not be satisfied by the line driver. This typically indicates an insufficient asynchronous buffer pool size. The Entire Net-Work session is terminated abnormally.
Action | Check the buffer pool statistics printed at the end of the session, provide more storage in the asynchronous buffer pool.

NET0023I | NODE statement missing
Explanation | A NODE statement must be given as the first parameter statement. The Entire Net-Work session is terminated abnormally.
Action | Code an appropriate NODE statement as the first parameter statement. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0024I | No driver loaded
Explanation | After initialization, the number of successfully initialized line drivers is zero. With no active line drivers, there is no point in continuing the Entire Net-Work session. The Entire Net-Work session is terminated abnormally.
Action | Verify that all line drivers and their environments have been installed correctly, and that all DRIVER statements have been coded accordingly.

NET0025I | Trace table init failed, RC=nn
Explanation | The requested trace table could not be initialized. RC=4 indicates that not enough storage was available; any other value indicates an internal error. The system continues to run, but with tracing disabled.
Action | If RC=4, either try to run with a smaller trace table or provide a larger partition or address space. If nn is other than 4, contact your Software GmbH technical support representative.

NET0026I | Initialization failed
Explanation | This is an informational message only, specific error conditions are described in preceding messages. The Entire Net-Work session is terminated abnormally.
Action | Refer to the preceding messages for the reasons for the failure.

NET0027I | Handshake buffer shortage (RC=nn)
Explanation | There were not enough short-term buffers available to sustain the handshake process. It is highly unlikely that the present amount of buffer space is adequate to handle any message traffic. Return code values other than 4 or 8 may indicate an internal problem and should be reported to your technical support representative. The Entire Net-Work session is terminated abnormally.
Action | Provide more storage in the short term (or possibly the page-fixed) buffer pool, according to the buffer pool statistics provided.

NET0028I | Message buffer shortage
Explanation | There were not enough short-term buffers available to handle message traffic. The Entire Net-Work session is terminated abnormally.
Action | No action is usually required for this mainly informational message. If followed by a NET017I Disconnect message, there is a buffer pool shortage. Provide more storage in the asynchronous buffer pool.

NET0029I | B1: Target xxxxx init on unknown node yyyyy
Explanation | A B1 broadcast message was received from an unknown node. This indicates an error condition in the internal network tables. None. This message is informational only. The Entire Net-Work session continues operation.
Action | If this message occurs repeatedly, attempt to locate inconsistent Entire Net-Work descriptions. Report the problem to your technical support representative.

NET0031I | Invalid log parameter
Explanation | The value specified for the LOG keyword on the NODE statement or the SET operator command was invalid. The erroneous parameter is ignored. Processing continues normally.
Action | Use the SET operator command to specify the correct LOG parameter value.

NET0032I | Excessive ECB count in driver aaaa
Explanation | An internal error occurred; an incorrect module was probably loaded as line driver NETaaaa. The Entire Net-Work session is terminated abnormally.
Action | Have the storage dump and/or dumps of the Entire Net-Work modules available, then contact your technical support representative.

NET0033I | aaaa driver requires page-fixed buffers
Explanation | The access method aaaa requires a page-fixed buffer pool in order to function in your operating system configuration. The line driver initialization is aborted. The system may continue operating if other line drivers are active.
Action | Use the BUFFERS parameter on the NODE statement to specify a page-fixed buffer pool. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0034I | Unsupported version of ADAIOR. NETWRK terminating
Explanation | An unsupported version of Adabas or the WAL library is being used.
Action | Supply the appropriate Adabas or WAL libraries.

NET0035 | Isolated target targetid cannot be accessed from this node
Explanation | The targetid specified in the message cannot be handled because its value is greater than 255. This should only happen when Entire Net-Work is using an unsupported release of the WAL component. This target is unavailable to this node.
Action | Verify that the Entire Net-Work node that issued this message is using a supported version of WAL.

NET0036I | rrrrrrrr mmmmmmmmmm nnnnnnnnnn
Explanation | This message is issued in response to operator command DISPLAY STATS EXTENDED. It lists statistics for internal Entire Net-Work service routines.
Action | No action is required. This message is for Software GmbH use only.

NET0037I | module (yyyy-mm-dd SP=ss) ZAP LEVEL zzzz
Explanation | This message is issued in response to operator command DISPLAY ZAPS. For each Entire Net-Work module (module), its name, assembly date, system maintenance level, and zap level are displayed. If zaps were applied after initial shipment, their numbers are listed as 'Additional Zaps .
Action | No action is required for this informational message.

NET0038I | module: NETWRK Date yyyy-mm-dd, Version: vv.rr, SP ss, Base WMnnnnnn
Explanation | This message is issued in response to operator command DISPLAY ZAPS. For each Entire Net-Work module (module), its name, Entire Net-Work version number, system maintenance level, and Entire Net-Work base level are displayed.
Action | No action is required for this informational message.

NET0039I | module, NETSAF version is invalid, shutdown
Explanation | The NETSAF module version is invalid or the NETSAF module is not available; module is the name of the module issuing the message. Entire Net-Work will shut down following this message.
Action | Save the DDPRINT and contact your technical support representative.

NET0040I | Get NETSAF work area failed for link xxxxxxxx
Explanation | An attempt to obtain buffer pool storage for the NETSAF work area failed for link xxxxxxxx. Security authorization cannot be performed without this work area, so the link is disconnected.
Action | The failure may be due to a buffer pool shortage. Check the buffer pool statistics. You may need to increase the region size.

NET0041I | NETRCV buffer shortage, NET-WORK terminating
Explanation | NETRCV was unable to get the necessary storage. Entire Net-Work will shut down following this message.
Action | Save the DDPRINT and the DUMP, if available, and contact your technical support representative.

NET0042I | Local target nnnnnn active
Explanation | This message is issued for each new target that becomes activated when Entire Net-Work is active.
Action | No action is required for this informational message.

NET0043I | Local target nnnnnn inactive
Explanation | This message is issued for each new target that becomes deactivated when Entire Net-Work is active.
Action | No action is required for this informational message.

NET0044E | License verification failed. Net-Work terminating
Explanation | The Entire Net-Work license could not be checked or is invalid. Entire Net-Work will be terminated. See other messages for details of the license error which has occurred.
Action | Investigate the cause of the error and rerun the job. If problems persist, contact your technical support representative for assistance.

NET0045I | NET-WORK running in WCA mode
Explanation | Entire Net-Work is running in Entire Net-Work Administration mode.
Action | No action is required for this informational message.

NET0051I | Nucleus extension xxxxxxxx not found
Explanation | The module xxxxxxxx has not previously been loaded as a nucleus extension. Entire Net-Work terminates the initialization process.
Action | Ensure that Entire Net-Work is being started properly. The NUCXTNTS EXEC must be run before Entire Net-Work is started.

NET0052I | Invalid LOGSIZE value; LOGSIZE set to 32000
Explanation | A value greater than 32000 has been specified for the LOGSIZE parameter. The valid range is 0 - 32000. The value is set to 32000 and Entire Net-Work continues.
Action | Specify a valid LOGSIZE value.
Module | NETWRK

NET0060I | Running without zEDC Compression Support.
Explanation | Initialization of IBM’s System zEnterprise Data Compression (zEDC) services was not requested.
Action | To activate zEDC support, the NODE parameter ZEDC must be set to "Y".

NET0061E | Unable to Initialize Compression Support. Module NETZEDC not available.
Explanation | Entire Net-Work mainline could not find an entry for module "Netzedec".
Action | Verify that Entire Net-Work's module "Netzedc" is available. If the problem persists, contact your technical support representative.

NET0062E | zEDC Compression Support Successfully Initialized
Explanation | Initialization of IBM’s System zEnterprise Data Compression (zEDC) services completed successfully.
Action | No action is required for this informational message.

NET0063E | Unable to decompress message - zEDC not initialized
Explanation | A message destined for this node is zEDC compressed, but the message cannot be decompressed because zEDC compression services are not active. The message is discarded with message NET0151, reason code 15, and the link is disconnected.
Action | Check for other messages identifying a problem with zEDC services and make appropriate corrections.

NET0064E | Decompress failed; disabling decompression for this node
Explanation | An attempt to decompress a zEDC-compressed message failed. Decompression is disabled on this node, and the other nodes in the network are notified to no longer compress messages sent to this node. The failed message is returned to the caller with response code 224 (ADARSP224), subcode 1.
Action | Verify that the z/OS system is at the right software and hardware levels. If the problem persists, contact your technical support representative.

NET0086I | Invalid SNAP parameter: xxxxxxxx
Explanation | A SNAP operator command was issued with an invalid additional parameter. Valid parameters are MAIN, MYBLK, TRACE, CURRMSG, UBQ, CQ, and BPH.
Action | Re-issue the SNAP command with valid parameters. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0087I | nnnnnnnnnn Requests from local RQ
Explanation | This is an informational message displaying the number of requests Entire Net-Work received from its local request queue (RQ) for transmission to other nodes.

NET0088I | nnnnnnnnnn Requests for target nnnnn on node aaaaaaaa
Explanation | This is an informational message displaying the number of requests Entire Net-Work handled for target nnnnn. If aaaaaaaa is the local node, the number specifies incoming requests, otherwise outgoing requests. This message is not displayed for targets with a message count of zero.

NET0089I | nnnnnnnnnn Requests total ......... for node aaaaaaaa
Explanation | This is an informational message displaying the number of requests that Entire Net-Work handled for all targets on node aaaaaaaa. If aaaaaaaa is the local node, the number specifies incoming requests, otherwise outgoing requests. This message is not displayed for nodes with a request count of zero.

NET0090I | Buffer usage statistics
Explanation | This is an informational message that immediately precedes the NET0091 message.
Action | Refer to the NET0091 message for more information.

NET0091I | resourcename: sizea (= nn.n %) of sizeb K used
Explanation | At the end of each Entire Net-Work session, usage statistics (sizea) for major buffer pool resources are displayed; values are in Kbytes (1024-byte units, or sizeb), and fractional values are rounded to the next lower value; the percentages given provide a better measurement of buffer pool usage (request queue statistics are specified in the number of queue elements).
Action | Monitor buffer usage, and take corrective action if any of the usage figures are near 100%.

NET0092I | nnnnnnnnnn node stack expansions performed
Explanation | The value provided by the MAXPATH keyword parameter on the NODE statement determines the size of the node stack in the message header, which in turn records the message's path through the network. Whenever a message path exceeds the capacity of the originally created node stack, the relay node detecting the condition has to expand the node stack by copying the message into another buffer. To avoid this overhead, specify a larger MAXPATH value on the originating node (not on the node that presents this message to alert you to the condition at session termination).
Action | If the number of node stack expansions becomes significant, try to identify the originating node and increase the MAXPATH value. A good look at the network topology is likely to provide all the necessary clues. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0093I | nnnnnnnnnn replies could not be routed
Explanation | This is an informational message giving the number of cases where a reply could not be routed to the user s node, probably because the node ended operation or became unreachable after the subject messages were sent. No provision is made to deliver the reply elsewhere. The reply is abandoned; the count in this message is the only remaining indication of the abandoned replies.

NET0094I | nnnnnnnnnn messages were stranded
Explanation | This is an informational message. Stranded messages are user requests that could not be routed to the target node, but also could not be returned to the user to provide a response code because the user s node (or the only link to it) terminated or became unusable after the message was sent. Since there is nowhere else the messages could be delivered, they were abandoned. The count in this message is the only remaining indication of the abandoned messages.

NET0095I | nnnnnnnnnn requests timed out (RSP224)
Explanation | This is an informational message displaying the number of times this Entire Net-Work node had to issue the response code 224 (ADARSP224) for message timeouts.
Action | If the number becomes significant, it indicates certain bottlenecks somewhere in the network. You should identify and eliminate these. Alternatively, increase the REPLYTIM parameter on the NODE Statement. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0096I | nnnnnnnnnn requests failed due to buffer shortage
Explanation | This is an informational message displaying the number of times this Entire Net-Work node had to issue the response code 220 (ADARSP220) for short term buffer shortage conditions.
Action | If the number becomes significant, increase the size of the short term buffer pool.

NET0097I | NETWORK terminating due to parm errors
Explanation | This informational message is issued after all parameter statements have been read, indicating that due to previously listed parameter errors the session of Entire Net-Work is about to be terminated.
Action | No action is required. This message is informational only.

NET0098I | Abnormal termination completed
Explanation | This is an informational message indicating that the abnormal termination procedures were completed successfully.

NET0099I | Normal end of run
Explanation | This is an informational message indicating that the normal termination procedures were completed successfully.

NET0101I | aaaaaaaa driver open failed (RC=nn)
Explanation | The line driver aaaaaaaa could not be opened. More specific messages should have been issued by the line driver. The return code (nn) is access method dependent. If this condition is detected during session initialization, Entire Net-Work will terminate abnormally; if it occurred during an attempt to re-open a line driver after access method failure (either manually by the START operator command or automatically based on the RESTART parameter values specified in the DRIVER statement), normal system operation continues - without the line driver in question.
Action | Refer to the related access-method-specific line driver error message for information on what condition caused this error. Correct the access method problem and issue a START operator command for the driver, or wait for the next RESTART to occur. Under certain circumstances, you may have to stop and restart the Entire Net-Work session to make the line driver available.

NET0103I | Link aaaaaaaa (bbbb) open failed (RC=nn)
Explanation | The link aaaaaaaa (of driver bbbb) could not be opened. More specific messages describing the link problem were probably issued by the line driver. The return code (nn) is access method dependent. The system continues to run normally without the link.
Action | Refer to the related line driver error message for information on the cause of this error. Rectify the access-method problem and issue a CONNECT operator command for the link, or wait for the next RESTART to occur. Under certain conditions you may have to stop and restart the Entire Net-Work session in order to make the link available.

NET0104I | Link aaaaaaaa (bbbb) connect failed
Explanation | The link aaaaaaaa (for driver bbbb) could not be connected. More specific messages describing the link problem were probably issued by the line driver. Note that this is an actual error condition. The normal operating case where one node tries to connect before the partner is available cannot cause this error. The system continues to run normally without the link.
Action | Refer to the access-method-specific error messages for information on the cause of this error. Correct the access method problem and issue a CONNECT operator command for the link, or wait for the next RESTART to occur. Under certain circumstances, you may have to stop and restart the Entire Net-Work session in order to make the link available.

NET0105I | All aaaa links closed by access method termination
Explanation | The access method aaaa was terminated. Links using that access method can no longer function. The system continues to run normally without the links.
Action | When the access method becomes available again, use the operator commands START and CONNECT to restart the line driver and links involved. You may want to specify the RESTART parameters on the DRIVER or LINK statements to automate this process. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0106I | Link aaaaaaaa can't connect to node bbbbbbbb reason rsn
Explanation | Handshaking could not be completed to node bbbbbbbb via link aaaaaaaa for the reason (rsn) given, which can be one of the following reasons:
Reason | Description
--- | ---
Inv(alid) link status | The link received a handshake request from the other side that conflicted with the current link status. A handshake error message is sent to the other node, rejecting the request.
Reject by node | A handshake request was rejected by the other node; this may be due to network conflicts (see below), in which case messages NET0108 and NET0109 are issued to describe the conflict; if no such messages appear, the problem is probably caused by an invalid link status on the other side (see above).
NETWORK conflict | Handshaking determined that conflicts exist between the network topologies as seen by this node and node bbbbbbbb; therefore, a connection via link aaaaaaaa was not established. Messages NET0108 and NET0109 are also issued before this message, defining the conflicts. Note that the connection is physically functional, but cannot be used due to the conflicts.
The link is disconnected.
Action | Remove the conflict from the network. This may require terminating and renaming a node, or terminating one or more targets with duplicate target IDs. Then use the CONNECT operator command to resume handshaking.

NET0107I | Link aaaaaaaa disconn. from node bbbbbbbb
Explanation | The link aaaaaaaa was disconnected from node bbbbbbbb by one of the following events: node termination, a DISCONNECT operator command, certain types of link failures (described by related line driver messages), or a disconnect request from the other node due to one of these causes. The system continues processing without the link.
Action | If appropriate, try to reconnect the link with the CONNECT operator command. If the cause of the disconnect has not been corrected, the reconnect attempt will fail.

NET0108I | Conflict: target nnnnn on node aaaaaaaa and bbbbbbbb
Explanation | Target IDs have to be unique throughout the network. If multiple targets with the same ID are detected during link connection, the link cannot be connected until the conflict is resolved. Message NET0106 or NET0306 is issued after all detected conflicts have been listed. The link is disconnected.
Action | Remove the conflict from the network by terminating targets with duplicate target IDs. Then use the CONNECT operator command to resume handshaking.

NET0109I | Conflict: node aaaaaaaa
Explanation | Node names must be unique throughout the network. If multiple nodes with the same name are detected during link connection, the duplicate link cannot be connected. Message NET0106 or NET0306 is issued after all detected conflicts have been listed. The link is disconnected.
Action | Remove the conflict from the network by terminating and renaming the conflicting node(s). As an alternative, first try the PROBE operator command to verify if node aaaaaaaa is actually active, then issue the CONNECT operator command to resume handshaking.

NET0110I | Link aaaaaaaa connected to node bbbbbbbb
Explanation | Link aaaaaaaa was successfully connected to node bbbbbbbb. The function may have been initiated from either side. Normal processing continues, the newly connected link will be considered for message traffic.

NET0111I | Link aaaaaaaa closed
Explanation | During Entire Net-Work termination, link aaaaaaaa was closed. Usage statistics for the link follow this message. After displaying the usage statistics, termination processing continues normally.

NET0112I | nn,nnn,nnn,nnn msgs; BLK factor = nnn.nn
Explanation | This message details the number of messages and transmission blocks sent via the link and the blocking factor achieved. This last item is only displayed if BLOCKMSG=Y and STATBLK=Y are in effect for this link. This message is displayed as a result of the DISPLAY LINK operator command. With the Simple Connection Line Driver, this count is reset to zero (0) after link connect processing.

NET0113I | nn,nnn,nnn,nnn {INPUT | OUTPUT} throwbacks;
Explanation | This message is printed in conjunction with message NET0111 if throwbacks occurred. It is an indication that not enough message buffers (short term or page-fixed buffer pool) were available at some point during the session. The worst case figure specifies how often one individual message was thrown back.
Action | Check the buffer pool usage statistics; increase the appropriate buffer pool size to prevent future occurrences of this message.

NET0114I | Snap dump written to NETPRNT / DDPRINT
Explanation | The SNAP output is written to NETPRNT if it is available; otherwise, the output is written to DDPRINT.

NET0115I | Operator command not recognized
Explanation | The last operator command entered was not recognized by Entire Net-Work. The command is ignored.
Action | For the correct syntax, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference; then reissue the operator command.

NET0116I | Link aaaaaaaa not found
Explanation | An operator command was issued to act on link aaaaaaaa, but no link with that name is defined. The command is ignored.
Action | To determine which links are defined, use the DISPLAY LINKS operator command, then reissue the corrected command.

NET0117I | Link aaaaaaaa cannot be connected, STAT=ssssss
Explanation | An operator command was issued to connect link aaaaaaaa, but the link is in a state that does not allow connection (the link is probably already connected). STAT=ssssss may be one of the following status codes:
Status Code | Description
--- | ---
NOTOPEN | The link is not open yet.
OPEN | The link is open.
CONSTA | The connection process started.
COPEND | The connection process is in waiting status.
COFAIL | The connection attempt failed.
CONN | The link requested is already connected.
HSERR | A handshaking conflict occurred.
HS1 | First handshake message was sent.
HS2 | Second handshake message was sent.
HSING | An interim status during handshake.
ACTIVE | Active for payload message traffic.
SUSPND | Connection process was suspended.
DISCRQ | Other party requested to be disconnected.
DISC | Successful disconnection completed.
The command is ignored.

NET0118I | Invalid RQE address in reply; detailed snap dump
Explanation | A reply was received for a user request originating at this node. The message header's pointer to this request s Request Queue Element (RQE) is invalid. This is probably an internal error. A possible valid cause for this condition could be that the node was terminated and restarted while the message was under way in the network. The message in error is dumped to the printer data set for diagnostic pureness and then discarded. A user waiting for this reply is timed out with response code 224 (ADARSP224).
Action | If a node restart did not cause the message, have the printout (as well as any other related information) available, and contact your technical support representative.

NET0119I | Reply cannot be matched to; user=userid
Explanation | A reply to user userid s message has arrived, but the user no longer owns the request queue element (RQE) associated with the dialogue. This might be caused by the user program terminating abnormally or by a timeout condition due to the REPLYTIM parameter on the NODE statement. In either case, the user program that requested the reply is no longer waiting for it. This condition is very similar to the 'USER GONE' error detailed in messages NETM91, NETM92, and NETM93. The message in error is discarded.
Action | To reduce the chance of this error, increase the REPLYTIM parameter value on the NODE statement to accommodate the longest transmission time that typically occurs in the network. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0120I | aaaa Link bbbbbbbb to node cccccccc stat=ssssss
Explanation | This message is issued in response to the DISPLAY LINKS operator command. aaaa specifies the access method for the link, bbbbbbbb is the link name from the LINK parameter statement, cccccccc is the name of the node on the other side of the link, and ssssss is the link status. Refer to the status code descriptions for NET0117 explaining the meaning of the link status codes. If the link is a TCPX link, the partner's TCP/IP address is displayed rather than the node name (cccccccc setting).

NET0121I | Output queue: nnnnmsgs, mmmm tr.blks
Explanation | This message is issued in response to the DISPLAY LINKS operator command unless both nnnn and mmmm are zero. It indicates a transmission backlog for the link. A small backlog is normally not an error condition, but a backlog that increases over time may indicate a problem with the link. Note that there are usually no messages in the input queue when operator commands are handled.

NET0122I | Node aaaaaaaa (bbbbbbbb) dist nnnnnn (lll) via link cccccccc
Explanation | This message is issued in response to the DISPLAY NODES, DISPLAY PATHS, or PROBE operator command. The node name (aaaaaaaa) from the NODE parameter statement, the node ID (bbbbbbbb) or target ID of the communicator, the distance (nnnnnn) to the node (computed by adding all link weights along the path to the node), the number (lll) of links between this Entire Net-Work node and node aaaaaaaa, and the name of the first link (cccccccc) on the path are given in the message. See the WEIGHT parameter in the section Entire Net-Work LINK Statement in Entire Net-Work Reference) for more information about link weights. In the case of a DISPLAY NODES command, only the shortest path is shown; in this case, the local node is shown with the term LOCAL in place of the distance information. Either a DISPLAY NODES command specifying a node name or a PROBE command can cause 'INACTIVE' or 'NOT FOUND' to be displayed in place of the link information. For a DISPLAY PATHS command, all paths to all nodes are displayed; that is; each node is listed once for each link which has a path to it. The distance shown is the shortest path length via the link.

NET0123I | Targets: nnnnn,mmmmm, ... j NONE
Explanation | This message is issued in response to the DISPLAY NODES operator command. It lists the IDs of all targets currently active on the node named in the preceding message NET0122; the communicator's ID is not listed again in this message. The term NONE indicates that no targets except the communicator are active on that node.

NET0124I | Target nnnnn (tt - tr) LOCKED | ACTIVE | INACTIVE on node aaaaaaaa
Explanation | This message is issued in response to the DISPLAY TARGETS operator command or at Entire Net-Work startup. All targets that were ever active in the network are listed. The target ID (nnnnn), the target type (tt), and the name of the node (aaaaaaaa) on which the target is or was active are given in the message. The value of tr is T if the target uses Adabas Version 7 translation or N if it does not. At Entire Net-Work startup, this message is issued only for the local target; remote targets will not be displayed. Inactive targets are shown on the node where they were last active. The following table contains the possible target types:
Target Type Code | Description
--- | ---
A | Anchor (e.g., Natural Global Buffer Pool)
c | Client-only Element
C | Communicator (Entire Net-Work)
I | Global isolated database
L | Local isolated database
N | Non-database target (ACCESS)
T | Translation / UES-enabled database
V | Adabas Cluster Services database

NET0125I | No active paths
Explanation | This message is displayed in response to a DISPLAY PATHS operator command when no paths are currently active.

NET0126I | No links found
Explanation | This message is displayed in response to a DISPLAY LINKS operator command when no links have been defined or no links match the qualifier specified. Note: Although it may seem pointless to have a communicator active with no links defined, a DRIVER statement specifying ACCEPTUI=YES could be used to generate links dynamically when other nodes attempt to connect.

NET0127I | SET command accepted
Explanation | This message is displayed to acknowledge a SET operator command.

NET0128I | Entire Net-Work terminating targetnnnnn due to
Explanation | Entire Net-Work usually prevents concurrent sessions by more than one target with the same ID. If targets with the same ID are started simultaneously on different nodes, the condition is recognized as soon as the broadcast messages meet. All targets with the same ID are terminated by their respective communicators, and this message is displayed on the operator consoles.
Action | One of the conflicting targets may be started again.

NET0129I | aaaa driver opened
Explanation | This message acknowledges the successful execution of a OPEN driver (or START driver) operator command. aaaa defines the access method of the driver that was restarted.

NET0130I | aaaa driver not opened
Explanation | The CONNECT link operator command could not be executed because the associated line driver was not open. aaaa is the access method of the line driver. The command is ignored.

NET0131I | aaaa driver already open
Explanation | The START driver operator command could not be executed because the line driver is already open. aaaa is the access method of the line driver. The command is ignored.

NET0133 | Invalid trace argument: aaaaaaaa
Explanation | An invalid argument aaaaaaaa was given for either the TRACE, TRON or TROFF parameter on the NODE statement or on a SET operator command. Valid trace arguments are 'MAIN' for the control module, 'BPM for the buffer pool manager, "TQM" for the Transmission Queue Manager, and "RQM" for the Receive Queue Manager as well as the access method names of all loaded line drivers. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.

NET0134I | No such target
Explanation | The target ID specified as an argument of a DISPLAY TARGETS operator command was either invalid, or does not exist. The command is ignored.
Action | Re-specify the command with a valid target ID.

NET0135I | Probe for node aaaaaaaa (nnnn.nnn sec)
Explanation | A PROBE operator command was issued for node aaaaaaaa, and the resulting message was returned. PROBE messages are time-stamped to measure the time needed to communicate between the local node and node aaaaaaaa. The required time is displayed in nnnn.nnn seconds.

NET0136I | Probe msg sent. User data length: nnnnn
Explanation | This message acknowledges a PROBE operator command and displays the length of the random user data sent (maximum length is 64512 bytes). Message NET0135 is displayed when the PROBE reply is returned.

NET0137I | Link aaaaaaaa connect initiated
Explanation | This is an informational message indicating that a connect request was issued for link aaaaaaaa. Further message will be displayed as the connection process progresses. If the partner node is not active some access methods may display appropriate messages, others may not. The link is placed in 'Connect Pending' status; when all required actions by both nodes are completed, the link will be placed in 'Active' status and message NET0110 will be displayed.

NET0139I | nn,nnn a bytes sent; compression rate nnn.nn
Explanation | This is an informational message displaying the number of (uncompressed) bytes sent via this link and the compression rate that was accomplished. The multiplier character '"a"' may take on one of the following values:
Value | Description
--- | ---
blank | = bytes
K | = kilobytes
M | = megabytes
G | = gigabytes
T | = terabytes

NET0141I | via node(s): nodename
Explanation | This message appears in response to a PROBE command if the node being probed is not directly connected; that is, it is reached via some other node. The message shows the relay node(s) used to complete the end-to-end connections.

NET0144I | CSCI function not available
Explanation | A DISPLAY CSCI operator command was issued, but the NETCSI module is not linked to Entire Net-Work and is not available for dynamic load.

NET0145I | Link xxxxxxxx disabled
Explanation | This message is a confirmation message in response to a DISABLE operator command. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0146I | Link xxxxxxxx suspended
Explanation | This message is a confirmation message in response to a SUSPEND operator command. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0147I | Link xxxxxxxx is not active
Explanation | A SUSPEND operator command was issued for a link whose status is not active. Only active links can be suspended. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0148I | Link xxxxxxxx is not suspended
Explanation | A RESUME operator command was issued for a link that was not previously SUSPENDed. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0149I | Link xxxxxxxx resumed
Explanation | This message is a confirmation message in response to a RESUME operator command. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0150I | 'NODE DOWN' message sent
Explanation | This is the response to the Entire Net-Work operator command FORCE node. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0151I | Invalid NET-WORK message on link xxxxxxxx (reason=nn)
Explanation | A message was received on link xxxxxxxx that violates the internal Entire Net-Work message protocol. The reason code (nn) indicates the type of error detected, as follows:
Reason Code | Description
--- | ---
1 | Invalid message header
2 | Invalid control message
3 | Invalid probe message
4 | Invalid probe reply
5 | Message length exceeds 16 megabytes
6 | Invalid distribution list pointer
7 | Invalid node name reported in message
8 | Target number zero reported in message
9 | Target list exceeds message length
10 | Node list exceeds message length
11 | Invalid extra buffers in control message
12 | Buffer space exhausted
13 | Message header invalid or not specified
14 | NETZEDC returned a non-zero return code when attempting to decompress a zEDC-compressed message.
15 | A zEDC-compressed message was destined for this node, but zEDC services are not available.
A hexadecimal dump of the message is written to DDPRINT, and link xxxxxxxx is disconnected.
Action | Retain all related information and contact your technical support representative.

NET0153I | PARMS: link parameters
Explanation | This message is issued in response to operator command DEFINE LINK. It lists the parameters initially in effect for the new link. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference.

NET0154I | Link xxxxxxxx user exit detected on partner system
Explanation | A message was received on link xxxxxxx that was manipulated by a user exit on the sending Entire Net-Work node. A corresponding user exit was not defined on this Entire Net-Work node. The link is disconnected.
Action | Ensure that the adjacent Entire Net-Work nodes both have a user exit defined, or delete the user exit on the other side.

NET0155I | Operator command: hex-cmd-from-remote-node
Explanation | This message displays the operator command issued using the Programmable Command Interface (PCI) from the remote node. The command is shown on the line immediately following this message.
Action | No action is required for this informational message.

NET0170E | Verify argument not valid
Explanation | A non-numeric or out of range(1-65535) target ID was specified for the VERIFY operator command.
Action | Correct the VERIFY operator command input

NET0171I | Verify target target-id already active
Explanation | The target to be verified and listed in the message (target-id) is in the network and is active.
Action | No action is required for this informational message.

NET0172I | Verify target target-id not in this Net-Work
Explanation | The target to be verified and listed in the message (target-id) is not in this network.
Action | No action is required for this informational message.

NET0174I | Verify target target-id is relocatable or virtual
Explanation | The target to be verified and listed in the message (target-id) is relocatable or virtual.
Action | No action is required for this informational message.

NET0175I | Current CQ Cmd=cmd,Db=dbid,File=fn,Len=nnnnnn,Seq-Nr=rrr Time=ss sec ago,Job='jobname',TID=tid,Active -- yy CQEs displayed
Explanation | This message is issued in response to the DISPLAY CQ operator command. The command name (cmd), DBID (dbid), file number (fn), length (nnnnnn), sequence number (rrr), seconds (ss), job name (jobname), terminal ID (tid), status, and total number of CQEs (yy) are listed in the message.
Action | No action is required for this informational message.

NET0177I | CQE Seq-Nr=num,Status=status Addr=cqeaddr,Cmd=cc,Db=dbid,File=fn,Len=length Bin/out=xnnnn,Flags=xyyyy,AB=abaddr,UB=ubaddr Job='jobname',TID=tid Uid=uid Time=stcktime; ss sec ago
Explanation | This message is issued in response to the DISPLAY CQE operator command. For the specified command sequence number, the following are listed in the message: the command sequence number (num), status (status), address of the CQE, command code(cqeaddr), database and file numbers (dbid and fn), length of attached buffers (length), buffer in/out flags (nnnn), CQE flags (yyyy), address of the attached buffers (abaddr), address of the user buffer (ubaddr), job name (jobname), terminal identifier (tid), user ID (uid), the time in STCK format (stcktime), and the age in seconds (ss).
Action | No action is required for this informational message.

NET0178I | UBQ Cmd=cmd,Db=dbid,Fnr=fn,Checksum=cksum Addr=ubaddr,Flags=ubflags,Job=jobname,time ago=sec Uid=userid -- yy UBs displayed
Explanation | This message is issued in response to the DISPLAY UBQ operator command. The command name (cmd), DBID (dbid), file number (fn), Checksum (cksum) , user buffer (UB) address (ubaddr), UB flag and flag1 (ubflags), job name (jobname), time elapsed since the command was sent, in seconds (sec), 28-byte user ID in hexadecimal (userid), and total number of CQEs (yy) are listed in the message.
Action | No action is required for this informational message.

NET0179I | UBQ - Queue empty
Explanation | This message is issued in response to the DISPLAY UBQ operator command when there are currently no user buffers (UBs) in the transmit queue.
Action | No action is required for this informational message.

NET0180I | nnnnn{K | G | T} messages were compressed
Explanation | This message shows the number of messages that were successfully compressed with zEDC.
Action | No action is required for this informational message.

NET0181I | nnnnn{K | G | T} bytes uncompressed data
Explanation | This message shows the total number of uncompressed bytes that were successfully compressed.
Action | No action is required for this informational message.

NET0182I | nnnnn{K | G | T} bytes compressed data
Explanation | This message shows the total number of bytes of compressed data.
Action | No action is required for this informational message.

NET0183I | nnnnn% compression rate
Explanation | This message shows the compression rate as a percentage.
Action | No action is required for this informational message.

NET0184I | Uncompressed: smallest-msg largest-msg avg-msg
Explanation | This message shows size of the smallest and largest messages that were successfully compressed, and the overall average size of those messages before compression.
Action | No action is required for this informational message.

NET0185I | Compressed: smallest-msg largest-msg avg-msg
Explanation | This message shows size of the smallest and largest messages after they were compressed, and the overall average size of those compressed messages.
Action | No action is required for this informational message.

NET0190I | Node=nodename,Nodeid=nodeid,Host=hostname targetid[(clnucid)]: product code and version type,Jobname=jobname,Jobid=jobid
Explanation | This message is issued in response to the DISPLAY DETAIL operator command. It displays the network node name (nodename), the node ID (nodeid), and the host/LPAR name (hostname). The target number (targetid) and optional cluster nucleus ID (clnucid) are displayed as well as the product name and version number with which the target was started. The job name (jobname) and job ID (jobid) of the startup job are also shown. The target types (type) can be: Communicator - usually an Entire Net-Work; Database - a database accessible by Entire Net-Work; Isolated - usually a target accessible by Entire Net-Work; Local - A local database, not accessible by Entire Net-Work; Non-Database - not a database target; Translator - a translation target, probably a UES database; or Virtual - a target that has only registered with the Entire Net-Work.
Action | No action is required for this informational message.

NET0191I | No target found
Explanation | This message is issued in response to the DISPLAY DETAIL operator command when there are currently no targets in the requested range to be displayed.
Action | No action is required for this informational message.

NET0200I | zIIP-related statistics
Explanation | This message displays a variety of zIIP-related statistics.
Action | No action is required for this informational message.

NET0201I | zIIP processing is not enabled
Explanation | The DISPLAY ZSTATS operator command can only be used when ADARUN parameter ZIIP=YES is specified.
Action | No action is required for this informational message.

NET0240E | Unknown NETPRNT request
Explanation | An invalid NETPRNT request was detected. The only requests currently supported are OPEN, CLOSE, and WRITE.
Action | This message indicates a logic problem in Entire Net-Work and should be reported to your technical support representative.
Module | NETDUMP

NET0241I | NETPRNT file closed
Explanation | The NETPRNT file has been closed. All print output is sent to DDPRINT until this file is re-opened. While the file is closed it remains allocated, but it can be copied and re-opened.
Action | No action is required. This message is informational only.
Module | NETDUMP

NET0242I | NETPRNT file opened
Explanation | The NETPRNT file has been opened. All print output is sent to the file allocated to the NETPRNT DD statement. If the file was allocated SHR or OLD, it contains no existing print records. If the file was allocated MOD, the new records are placed after the existing records.
Action | No action is normally required. However, if the initial space allocation becomes exhausted, you will need to specify a secondary extent allocation.
Module | NETDUMP

NET0243E | NETPRNT file open failed - using DD PRINT
Explanation | The NETPRNT file failed to open. This may be caused by a missing NETPRNT DD statement or some other allocation error. All output is sent to the DDPRINT file until the NETPRNT file can be successfully opened.
Action | Check the JOBLOG and SYSLOG for operating system messages that indicate the cause of the allocation failure.
Module | NETDUMP

NET0244E | Write failed to NETPRNT file
Explanation | A WRITE to the NETPRNT file failed. The cause may be an out-of-space condition such as ABENDSD37 or other I/O error or short-on-storage condition (e.g., IOR failed to get the storage it needed). The NETPRNT file is closed and all output is sent to the DDPRINT file. It may be possible to re-open the NETPRNT file if it was allocated SHR. The data set should be copied before reopening because all records will be deleted.
Action | Check the JOBLOG and SYSLOG for operating system messages that indicate the cause of the I/O error.
Module | NETDUMP

NET0245E | Write failed to NETPRNT file
Explanation | A CLOSE of the NETPRNT file failed. This is an internal logic error or I/O error. The NETPRNT file will be unusable until Entire Net-Work is brought down.
Action | Check the JOBLOG and SYSLOG for operating system messages that indicate the cause of an I/O error. If no I/O error can be found, report this to your technical support representative.
Module | NETDUMP

NET0246E | LOGBUFSZ=0; log buffer not allocated
Explanation | The LOGBUF parameter is set "ON" and logging is active, but there is no log buffer available because the LOGBUFSZ parameter is set to "0". As a result, LOGBUF is turned off (set to "OFF").
Action | Specify a size for the LOGBUFSZ parameter and set the LOGBUF parameter to "ON" again.

NET0247E | Failed to get log buffer storage
Explanation | An attempt to get the storage specified by the LOGBUFSZ parameter failed. As a result, LOGBUF is turned off (set to "OFF").
Action | Increase the amount of storage available to Entire Net-Work or specify a smaller value for the LOGBUFSZ parameter. In either case, set the LOGBUF parameter to "ON" again.

NET0250I | Dump options aaaaaaaa
Explanation | This message lists the values specified for the DUMP parameter on the NODE statement. This message will also be seen as a reply to the SET DUMP operator command. For more information, see the section Entire Net-Work Parameter Statements in Entire Net-Work Reference.
Action | This is an informational message only and no action is required.
Module | NETMAIN

NET0251I | Invalid dump options aaaaaaaa
Explanation | An invalid value was specified for the DUMP parameter on the NODE statement. The default value 'ALL' is used to dump all areas. This message may also be seen as a reply to an invalid SET DUMP operator command specification.
Action | Correct the DUMP parameter specification on the NODE statement before restarting Entire Net-Work (see the DUMP parameter in the section NODE Statement Parameters). A SET DUMP operator command can be used to specify the dump options for the currently running Entire Net-Work (see SET DUMP in the section Entire Net-Work Operator Commands). Both sections are in Entire Net-Work Reference .
Module | NETMAIN

NET0306I | Disconnecting link xxxxxxxx due to network conflict
Explanation | An Entire Net-Work conflict was detected in a control message received on link xxxxxxxx. The nature of the conflict is reported in preceding messages NET0108, NET0109, or NET0308. The link is disconnected.
Action | Follow the user action recommended in the description of the preceding message, i.e., NET0108, NET0109, or NET0308.

NET0308I | NODEID on xxxxxxxx in conflict with target ttttt
Explanation | An Entire Net-Work control message reported a node xxxxxxxx whose target ID is already active elsewhere in the network. This presents a network conflict, as target IDs must be unique throughout the network. Message NET0106 or NET0306 is issued after all detected conflicts have been listed. The link is disconnected.
Action | Remove the conflict from the network by either terminating target ttttt, or assigning a new unique target ID to node xxxxxxxx.

NET0322I | Node dddddd.aaaaaaaa (bbbbb) dist nnnnnn (lll) via cccccccc
Explanation | This message replaces the corresponding form of NET0122, when a node is listed that has a non-blank domain name. Also see the DOMAIN parameter in the section NODE Statement Parameters in Entire Net-Work Reference.

NET0328E | Message buffer shortage. Sending deferred
Explanation | A message is to be sent on a link that has a user exit defined. There is not enough buffer space to provide a work area to the user exit. The message is not sent at this time. An attempt is made to free enough working storage. Sending the message is then tried again.
Action | Increase the size of the Short Term Buffer Pool to prevent future occurrences of this problem.

NET0333I | operator command - short description
Explanation | Multiple messages NET0333 are issued in response to the HELP command. The available operator commands are listed with a short explanation of their function.

NET0334E | ADAIOR function call nnn failed with RC=xxx; terminating
Explanation | The ADAIOR function call named in the message failed with the return code given in the message. The values are displayed in decimal. This is a critical error; Entire Net-Work terminates. Probable causes are a storage shortage or incompatible version of the WAL data set.
Action | Determine if the problem is caused by a storage shortage or if there is an incompatibility with the WAL data set version and fix the problem. If neither of these conditions are causing the problem, contact your Customer Support representative.

NET0335 | ZIIP=YES is not allowed with SSL/SSLI Driver
Explanation | ADARUN parameter ZIIP cannot be set to YES if the SSL or SSLI Driver is defined. zIIP processing is disabled.
Action | Set ZIIP=NO if using SSL or SSLI.

NET0336 | Error during zIIP initialization
Explanation | zIIP initialization failed due to an error or incompatible configuration. zIIP processing is disabled.
Action | Look for a previous error message that will explain the cause of the error.

NET0337 | zIIP processing has been disabled
Explanation | zIIP processing has been disabled due to an error, incompatible configuration, or license check failure. zIIP processing is disabled.
Action | Look for a previous error message that will explain the cause of the error.

NET0338 | Net-Work is now executing in SRB mode
Explanation | Operator command SET ZIIP=YES was specified. Net-Work is now executing in SRB mode and is eligible to run on zIIP processors when possible.
Action | No action required.

NET0339 | Net-Work is now executing in TCB mode
Explanation | Operator command SET ZIIP=NO was specified. Net-Work is now executing in TCB mode; zIIP processing is deactivated.
Action | No action required.

NET0340 | Command permitted only when zIIP-enabled
Explanation | The SET ZIIP operator command can only be used when ADARUN parameter ZIIP=YES is specified.
Action | No action required.

NET0341 | Command rejected; zIIP support is disabled
Explanation | The SET ZIIP operator command was rejected because zIIP processing has been disabled.
Action | Look for a previous error message explaining why zIIP processing was disabled.

NET0342 | ZIIP is already set to NO
Explanation | The operator command SET ZIIP=NO was entered, but zIIP processing is already deactivated.
Action | No action required.

NET0343 | ZIIP is already set to YES
Explanation | The operator command SET ZIIP=YES was entered, but zIIP processing is already active.
Action | No action required.

NET0346I | KC1NET1 : Command from Adabas Manager: xxxxxxxxxxxxxxxxxxx
Explanation | The command shown is being processed based on a request from Adabas Manager. Additional messages may indicate the success or failure of the command.
Action | No action required, this is an informational message.

NET0404E | Operator command not applicable to WCT
Explanation | The following operator commands are not applicable to Net-Work running in WCT mode: DEFINE, DISABLE, DISPLAY (NODES, PATHS, CSCI, CQ and CQE), DISCONNECT, ENABLE, PROBE, RESUME and SUSPEND.
Action | Exchange the operator command with an applicable one.

NET0998I | Entire Net-Work node aaaaaaaa abnormal end
Explanation | This is an informational console message indicating that abnormal termination procedures have been started.

NET0999I | Entire Net-Work node aaaaaaaa terminating
Explanation | This is an informational console message indicating that normal termination procedures have been started.

NET1000I | Entire Net-Work node aaaaaaaa active
Explanation | This is an informational console message indicating that the Entire Net-Work session has successfully completed initialization and is now ready for processing.

NET1001I | Current date is yyyy-mm-dd
Explanation | This message is displayed on the operator console and on the Entire Net-Work log data set at the beginning and end of a session as well as just after midnight. It helps to identify the exact time and date of any events recorded in the log.

NET1002I | NET-WORK node xxxxxxxx active since yyyy-mm-dd hh:mm:ss
Explanation | This message is issued in response to the operator command DISPLAY STATS. It shows the startup date and time of the local node xxxxxxxx.

NET1003I | DBID dbid relocated from local node to node
Explanation | The database target identified in the message (dbid) was previously active on this Entire Net-Work node. The target has been relocated to the node identified in the message (node). This message is associated with Adabas Cluster Services and Adabas Parallel Services database ID targets. Relocation was done on behalf of a command issued by an Adabas nucleus.
Action | No action is required for this informational message.

NET1004W | Link linkname zEDC compression not active; disabled
Explanation | ZEDC=Y was specified for this link, but ZEDC compression services are not available. zEDC compression is disabled for the link.
Action | Verify that the NODE parameter ZEDCINIT=Y was specified. Check for other error messages indicating that initialization of zEDC services failed and make appropriate corrections.

NET1005E | Link linkname zEDC error limit exceeded; disabled
Explanation | The limit for the number of zEDC compression errors has been reached for the specified link. The limit is ten errors. To prevent a looping error condition, zEDC compression is disabled for the link.
Action | Check for other error messages and investigate the cause of those errors. Make appropriate corrections.