NETX* - XCF OptionMessages

#### Search Results

Search

# NETX* - XCF OptionMessages

### Overview of Messages

`NETX001I | NETX006I | NETX007I | NETX008I | NETX026E | NETX027I | NETX028I | NETX029I | NETX030E | NETX031I | NETX032I | NETX033I | NETX040I | NETX100I | NETX104E | NETX108W | NETX113E | NETX114E | NETX115W | NETX119W | NETX124E | NETX125E | NETX126E | NETX127W | NETX130E | NETX131E | NETX132E | NETX133E | NETX140E | NETX141E | NETX142I | NETX150I | NETX151I | NETX152I | NETX159I | NETX160I | NETX169I | NETX170I | NETX171I | NETX172I | NETX173I | NETX174I | NETX175I | NETX176I | NETX180I | NETX181I | NETX182I | NETX184I | NETX185I | NETX186I | NETX187I | NETX188I | NETX189I`

NETX001I | fxname FUNCTION => RC = rc, RS = rs
Explanation | The XCF function fxname has completed with a return code (rc) and a reason code (rs) given in the message. Normal processing continues.
Action | None required. This message is informational only.

NETX006I | MEMBER member-name HAS JOINED THE group-name GROUP
Explanation | The group exit has detected that member member-name has joined the group group-name. Communication with the member has started.
Action | None required. This message is informational only.

NETX007I | MEMBER member-name HAS LEFT THE group-name GROUP
Explanation | The group exit has detected that member member-name has left the group group-name. Communication with the member has ended.
Action | None required. This message is informational only.

NETX008I | COMMUNICATION WITH UNDEFINED MEMBER member-name DISALLOWED
Explanation | Member member-name has joined this node's group. However, the member was not defined and ACCEPTUI=N was specified (by default) on the DRIVER statement. Communication with this partner will not be allowed.
Action | None required. This message is informational only.

NETX026E | LINK COULD NOT BE LOCATED FOR OPERATOR COMMAND
Explanation | An operator command specified an unknown link name. Normal processing continues.
Action | Reissue the operator command with a valid link name.

NETX027I | OPERATOR COMMAND COMPLETED: cccccccccccccccccccccccccccccc
Explanation | The operator command shown in the message has completed successfully. Normal processing continues.
Action | None required. This message is informational only.

NETX028I | OPERATOR COMMAND REJECTED: cccccccccccccccccccccccccccc
Explanation | The operator command shown in the message was rejected for one of the following reasons: The link name specified was not found. The command is not valid. The required operands were not entered (ALTER command). The driver is not in the proper state. Normal processing continues.
Action | Correct the operator command and reissue the command.

NETX029I | NETXCF AVAILABLE OPERATOR COMMANDS
Explanation | This is the first of a group of messages generated in response to the HELP operator command. All valid operator commands are listed on the console.
Action | None required. This message is informational only.

NETX030E | KEYWORD/VALUE ERROR => eeeeeeeeeeeeeeeeeeeeeeeeeeeeeeeeeeeee
Explanation | An ALTER operator command was entered with an invalid keyword or an invalid value. Some DRIVER statement and LINK statement parameters can be altered only when the driver or link is closed. All parameters following the invalid keyword or value are ignored.
Action | Either correct the keyword or value, or close the driver or link. Then reissue the command.

NETX031I | +----------------------------------------------------+
Explanation | This message is the first of a group of messages generated in response to the SHOW or STATS operator commands. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference. This message is written to the console and DDPRINT.
Action | None required. This message is informational only.

NETX032I | + llllllll STATE(xxxxxxxxxxxx) MSGS SENT(xxxxxxxx) RCVD(xxxxxxxx) +
Explanation | One of a group of messages generated in response to the SHOW or STATS operator commands. It shows the driver or link name, its state, and the number of messages sent/received. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference. This message is written to the console and DDPRINT.
Action | None required. This message is informational only.

NETX033I | + BYTES SENT( xxxxxxx.xxxu) BYTES RCVD( xxxxxxx.xxxu) +
Explanation | One of a group of messages generated in response to the SHOW or STATS operator commands. It shows the total number of bytes sent/received. For more information, see the section Entire Net-Work Operator Commands in Entire Net-Work Reference. This message is written to the console and DDPRINT.
Action | None required. This message is informational only.

NETX040I | NETWORK XCF CLOSE COMPLETE, GROUP=gggggggg, MEMBER=mmmmmmmmmmmmmmmm
Explanation | The XCF line driver has closed successfully. Normal processing continues.
Action | None required. This message is informational only.

NETX100I | DRIVBLK @aaaaaaaa NWXCFDRV @ aaaaaaaa
Explanation | The XCF driver has initialized successfully. The message provides the address of the XCF driver block and the address of the driver itself.
Action | None
Module | NWXCFDRV
Routine | DINIT

NETX104E | FAILED TO GET BUFFER FOR LINKBLK
Explanation | An attempt to get a buffer for a LINKBLK from the buffer pool failed. This message indicates a 'short on storage' problem
Action | Look for other messages that might indicate the cause of the storage shortage.
Module | NWXCFDRV
Routine | GEXIT

NETX108W | UNKNOWN MEMBER mmmmmmmm with ACCEPTUI=N
Explanation | The identified member has joined the XCF group used for this Entire Net-Work node. The member does not have a LINK statement defined, and unsolicited connections are not allowed.
Action | Add an XCF LINK statement to your parameters for the member or set ACCEPTUI=Y.
Module | NWXCFDRV
Routine | GEXIT

NETX113E | IXCCALL FAILED RC=xxxx RS=nnnn
Explanation | An XCF IXCJOIN or IXCQUERY call failed with the identified return code and reason code. This may be caused by invalid parameters defined to Entire Net-Work or system parameters (policy) defined for your SYSPLEX.
Action | Look up the return code and reason code in the IBM messages and codes documentation to determine if this is a configuration problem and, if so, take the necessary corrective action. If this is not a configuration problem, obtain the JOBLOG and NETPRNT or DDPRNT file, then report the problem to your technical support representative.
Module | NWXCFDRV
Routine | OPEND

NETX114E | IXCLEAVE FAILED RC=xxxx RS=nnnn
Explanation | An XDF IXCLEAVE call failed with the identified return code and reason code.
Action | Look up the return code and reason code in the IBM messages and codes documentation to determine if this is a configuration problem and, if so, take the necessary corrective action. If this is not a configuration problem, obtain the JOBLOG and NETPRNT or DDPRNT file, then report the problem to your technical support representative.
Module | NWXCFDRV
Routine | CLOSD

NETX115W | NODE nnnnnnnn IS NOT COMPATIBLE
Explanation | The identified node has joined the XCF group in use by this Entire Net-Work node, but the node is using an older version of the XCF driver that is not compatible with the current version. Entire Net-Work 5.8 introduced a new XCF driver that can only connect with other Entire Net-Work version 5.8 or later nodes. Entire Net-Work will continue to run, but no link is established with the incompatible node.
Action | Specify a different GROUP value on the driver parameter for this Entire Net-Work node.
Module | NWXCFDRV
Routine | OPEND

NETX119W | NODE nnnnnnnn IS NOT COMPATIBLE
Explanation | The identified node, which has joined the XCF group in use by this Entire Net-Work, is using an older version of the XCF driver that is not compatible with the current version. Entire Net-Work 5.8 introduced a new XCF driver that can only connect with other Entire Net-Work 5.8 or later nodes. Entire Net-Work continues to run, but no link is established with the incompatible node.
Action | Specify a different GROUP value on the driver parameter for this Entire Net-Work node.
Module | NWXCFDRV
Routine | GEXIT

NETX124E | IXCMSGO FAILED RC=xxxx RS=nnnn
Explanation | An XCF IXCMSGO call to send data to another member failed with the identified return code and reason code.
Action | Look up the return code and reason codes in the IBM messages and codes book to determine if this is a configuration problem. Obtain the JOBLOG and NETPRNT or DDPRNT file, then report this problem to your technical support representative.
Module | NWXCFDRV
Routine | SENDM

NETX125E | IXCMSGO FAILED RC=xxxx RS=nnnn FOR CONNECT
Explanation | An XCF IXCMSGO call to send a connection request to another member failed with the identified return code and reason code.
Action | Look up the return code and reason codes in the IBM messages and codes book to determine if this is a configuration problem and, if so, take the necessary corrective action. If this is not a configuration problem, obtain the JOBLOG and NETPRNT or DDPRNT file, then report the problem to your technical support representative.
Module | NWXCFDRV
Routine | CONNL

NETX126E | IXCMSGO FAILED RC=0000 RS=0000 FOR DISCONNECT
Explanation | An XCF IXCMSGO call to send a disconnection request to another member failed with the identified return code and reason code.
Action | Look up the return code and reason codes in the IBM messages and codes book to determine if this is a configuration problem and, if so, take the necessary corrective action. If this is not a configuration problem, obtain the JOBLOG and NETPRNT or DDPRNT file, then report the problem to your technical support representative.
Module | NWXCFDRV
Routine | DISCL

NETX127W | UNKNOWN NEXIT REQUEST
Explanation | The XCF Notify exit was called with an unknown request. Entire Net-Work ignores the request and continues to run.
Action | Obtain the JOBLOG and NETPRNT or DDPRNT file, then contact your technical support representative.
Module | NWXCFDRV
Routine | NEXIT

NETX130E | UNABLE TO GET STORAGE FOR MESSAGE
Explanation | Both a call to the buffer pool and a direct storage request failed. This is most likely caused by an out of storage condition. The system will ignore the message and disconnect the link.
Action | Increase the amount of virtual storage available to the Entire Net-Work address space.
Module | NWXCFDRV
Routine | MEXIT

NETX131E | MESSAGE FROM UNKNOWN VERSION OF NET-WORK
Explanation | A message received from a member of the XCF group in use by this Entire Net-Work is from a node using an older version of the XCF driver that is not compatible with the current version. Entire Net-Work 5.8 introduced a new XCF driver that can only connect with other Entire Net-Work 5.8 or later nodes. Entire Net-Work ignores the message and continues to run.
Action | Specify a different GROUP value on the driver parameter for this Entire Net-Work. Obtain the JOBLOG and NETPRNT or DDPRNT file, then contact your technical support representative.
Module | NWXCFDRV
Routine | MEXIT

NETX132E | BUFFER TABLE OVERFLOW
Explanation | The buffer table in the XCF driver has filled up. All of the entries in the table are currently allocated. These reusable table entries are used to temporarily save the address of an input buffer. This condition should not occur and indicates a logic problem or a severe performance problem.
Action | Contact your technical support representative.
Module | NWXCFDRV
Routine | MEXIT

NETX133E | UNABLE TO GET IDD
Explanation | An attempt to get an IDD control block failed. The request will be retried at a later time. This may be a temporary resource shortage or an out-of-storage condition.
Action | Increase the amount of virtual storage available to the Entire Net-Work address space. Contact your technical support representative if the problem persists.
Module | NWXCFDRV
Routine | DRIVE

NETX140E | INVALID COMMAND SYNTAX ENTERED
Explanation | An operator command was entered with a syntax error.
Action | Either correct the keyword or value, or close the driver or link. Then reissue the command. For the correct syntax, see the section XCF Operator Commands in Entire Net-Work XCF Option Administration.
Module | NWXCFDRV
Routine | OPCMD

NETX141E | UNKNOWN COMMAND ENTERED - xxxxxxxx
Explanation | The identified command was entered and is unknown.
Action | Use the HELP command or refer to the section XCF Operator Commands in Entire Net-Work XCF Option Administration .
Module | NWXCFDRV
Routine | OPCMD

NETX142I | XCF COMMAND EXECUTED
Explanation | This message informs you that the command entered was executed.
Action | None
Module | NWXCFDRV
Routine | OPCMD

NETX150I | LINK xxxxxxxx SENT RECEIVED
Explanation | This message is displayed in response to the STATS command for the identified link. It displays a header for Sent and Received statistical information that will follow in message NETX151I.
Action | None
Module | NWXCFDRV
Routine | CLKSTAT

NETX151I | ccccccccccc n,nnn,nnn,nnn,nnn n,nnn,nnn,nnn,nnn
Explanation | This message displays statistical information for the link displayed in message NETX150I. The size of the data is followed by the number of messages sent and the number of messages received. The displayed size is SMALL for messages that are smaller than the size specified by the driver parameter SMALLMSG. The displayed size is MEDIUM for messages larger than SMALLMSG and smaller than LARGEMSG. The displayed size is LARGE for messages that are larger than the size specified by the driver parameter LARGEMSG. The total of all message sizes is displayed as TOTAL message sizes. This information may be helpful in tuning the XCF group policy parameters.
Action | None
Module | NWXCFDRV
Routine | CLKSTAT

NETX152I | LINK xxxxxxxx STATISTICS RESET
Explanation | The statistics for link xxxxxxxx have been reset to zero.
Action | None
Module | NWXCFDRV
Routine | CLKRESET

NETX159I | VALID LINK COMMANDS
Explanation | This message is in response to a link HELP command.
Action | See following messages for command help information.
Module | NWXCFDRV
Routine | CLKHELP

NETX160I | NO STATISTICS ARE RECORDED FOR DRIVER
Explanation | A command to display or reset statistics for the XCF driver was attempted. There are no statistics recorded at the driver level to be displayed or reset. The command is accepted to prevent problems with automated command systems.
Action | None
Module | NWXCFDRV
Routine | CDVSTAT, CDVRESET

NETX169I | VALID DRIVER COMMANDS
Explanation | This message is in response to a driver HELP command.
Action | See following messages for command help information.
Module | NWXCFDRV
Routine | CDVHELP

NETX170I | RESET - RESETS STATISTIC VALUES TO ZERO
Explanation | This message is in response to a HELP command. It describes the RESET command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX171I | SHOW - SHOWS CONFIGURATION INFORMATION
Explanation | This message is in response to a HELP command. It describes the SHOW command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX172I | STATS - SHOWS CURRENT STATISTICS
Explanation | This message is in response to a HELP command. It describes the STATS command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX173I | SNAP - PRINTS DUMP OF STORAGE AREAS
Explanation | This message is in response to a HELP command. It describes the SNAP command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX174I | TRACE - PRINTS FORMATTED TRACE TABLE
Explanation | This message is in response to a HELP command. It describes the TRACE command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX175I | HELP - DISPLAYS COMMAND HELP
Explanation | This message is in response to a HELP command. It describes the HELP command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX176I | ALTER - USED TO ALTER PARAMETERS
Explanation | This message is in response to a HELP command. It describes the ALTER command.
Action | None
Module | NWXCFDRV
Routine | CDVHELP, CLKHELP

NETX180I | XCF GROUP=cccccccc TOKEN=xxxxxxxxxxxxxxxx
Explanation | This message is a response to the driver SHOW command. It displays the group and the XCF member token associated for this group member.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW

NETX181I | ACCEPTUI=Y, TRACESIZ=nnnk
Explanation | This message is a response to the driver SHOW command. It displays whether unsolicited connections are allowed (Y or N) and the size of the trace table.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW

NETX182I | SMALLMSG=nnnk, LARGEMSG=nnnk
Explanation | This message is a response to the driver SHOW command. It displays the values for messages considered to be small and large. These values are used for statistics kept by the links for messages sent and received.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW

NETX184I | XCF LINK=cccccccc TOKEN=xxxxxxxxxxxxxxxx
Explanation | This message is a response to the link SHOW command. It displays the name of the link and the XCF member token associated for this group member.
Action | None
Module | NWXCFDRV
Routine | CLKSHOW

NETX185I | PSTAT=N, RSTAT=Y, STATINT=nnnnn
Explanation | This message is a response to the driver or link SHOW command. It displays whether statistics should be printed (Y or N) and reset (Y or N) at the identified intervals, in seconds.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW, CLKSHOW

NETX186I | WEIGHT=nnn, SAF=N, ZEDC=N, ZEDCLOG=N
Explanation | This message is a response to the link SHOW command. It displays the relative weight assigned to this link, whether the SAF interface will be called for this link, and the values of ZEDC and ZEDCLOG.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW, CLKSHOW

NETX187I | RCVBFNUM=04096, RESTART=(n, n)
Explanation | This message is a response to the driver SHOW command. It displays the values of the RESTART and RCVBFNUM parameters.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW

NETX188I | RESTART=(nnnnn,nnnnn)
Explanation | This message is a response to the link SHOW command. It displays the values of the RESTART parameter.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW, CLKSHOW

NETX189I | SENDMULT=Y
Explanation | This message is a response to the driver or link SHOW command. It displays whether or not multiple messages can be send together in one send call.
Action | None
Module | NWXCFDRV
Routine | CDVSHOW, CLKSHOW