NETT* - Translation Routine Messages

#### Search Results

Search

# NETT* - Translation Routine Messages

NETTnnn messages are specific messages coming from the translation routines.

### Overview of Messages

`NETT001 | NETT002 | NETT003 | NETT004 | NETT005 | NETT006 | NETT007 | NETT008 | NETT010 | NETT011 | NETT012 | NETT013 | NETT014 | NETT015 | NETT016 | NETT017 | NETT018 | NETT019 | NETT021 | NETT024 | NETT025 | NETT026 | NETT027 | NETT028`

NETT001 | INPUT BUFFER TRANSLATION ERROR; RESULT RSP=229
Explanation | An error has been detected in the application's FB (Format buffer) or SB (Search Buffer). All the buffers are snapped to help assist in the application debugging. Forces an RSP=229 to be returned to the application.
Action | Verify that the application s format and/or search buffer is specified in valid syntax.

NETT002 | ENTIRE BUFFER NOT TRANSLATED
Explanation | An error has been detected in user buffer translation. The length specified for a buffer is less than the actual length returned by Adabas. Translation for this request is terminated.
Action | Verify that each field specified in the format buffer has a related format and length.

NETT003 | DBID dbid AVAILABLE ON NODE nodeid
Explanation | A connection to an RDA message-based remote node has been established. The messages displays a list of targets available on the node.
Action | No action is required. This message is informational only.

NETT004 | message-identifier ADMIN MSG FROM NODE nodeid RECEIVED
Explanation | An administration message has been received from an RDA message-based remote node.
Action | No action is required. This message is informational only.

NETT005 | INCOMING ADMIN MSG NOT A REQUEST
Explanation | An administration message has been received from an RDA message-based remote node but the request indicator has not been set. The incoming message is ignored and processing continues.
Action | Contact your technical support representative.

NETT006 | UNKNOWN OUTPUT MESSAGE
Explanation | It has been determined that a message that is to be sent cannot be properly translated. The message is neither translated nor sent, and processing continues.
Action | Contact your technical support representative.

NETT007 | UNKNOWN INPUT MESSAGE
Explanation | It has been determined that a message that has been received cannot be properly translated. The message is ignored, and processing continues.
Action | Contact your technical support representative.

NETT008 | COMPRESSED MESSAGE NOT SUPPORTED
Explanation | A message to be sent to a remote VMS, UNIX, or OS/2 node is in compressed format. The outgoing message is ignored.
Action | Make sure that the compression option is not turned on for any other links within the network task.

NETT010 | REPLY DISCARDED ON LINK xxxxxxxx
Explanation | The link was reconnected after a request was received from the link, but before the reply was received from the target and sent back across the link. The message is discarded.
Action | No action is required. This message is informational only.

NETT011 | nnnnn OUTSTANDING REQUESTS FREED ON LINK xxxxxxxx
Explanation | nnnnn messages were discarded as a result of the link being disconnected. Messages were discarded.
Action | No action is required.

NETT012 | SHORT TERM BUFFER SHORTAGE/ERRORS
Explanation | A failure occurred trying to obtain or release Entire Net-Work short-term buffers. The link is marked "suspended".
Action | Increase the short-term buffer allocation.

NETT013 | TRANSLATION DEFINITION ADDED SUCCESSFULLY
Explanation | A translation add request was issued to Entire Net-Work and was successfully added to the active translation table.
Action | No action is required. This message is informational only.

NETT014 | TRANSLATION DEFINITION DELETED SUCCESSFULLY
Explanation | A translation delete/remove request was issued to Entire Net-Work and a translation definition with matching criteria was successfully removed from the active translation table.
Action | No action is required. This message is informational only.

NETT015 | TRANSLATION DEFINITION DELETE FAILED
Explanation | A translation delete/remove request was issued to Entire Net-Work and no translation definition with matching criteria could be located in the active translation table.
Action | Check the translation delete/remove request for correctness.

NETT016 | DBID FILE FIELD ATOE ETOA EXIT FORMAT

NETT017 | output from the translat display list operator command

NETT018 | TRANSLATION DISPLAY COMPLETE
Explanation | This group of messages is issued for each TRANSLAT DISPLAY LIST command issued to Entire Net-Work. Message NETT017 will be issued for each active translation definition.
Action | No action is required. This message is informational only.

NETT019 | TRANSLATION DEFINITION ALREADY EXISTS - IGNORED
Explanation | A TRANSLAT DEFINE ADD request was issued to Entire Net-Work and was not added to the active translation table due to an active translation definition already existing for the specified database ID, file ID and field ID.
Action | Check the translation define/add request for correctness. If correct, a duplicate already exists. Otherwise, correct the request and try again.

NETT021 | CONVERTER LOGGING DATA
Explanation | If logging is turned on (LOGGING=Y), this DDPRINT message precedes the actual logging data.
Action | No action is required. This message is informational only.

NETT024 | CONNECTION REJECTED DUE TO INVALID NODE ID FROM NODE xxxxxxxx
Explanation | A UNIX or OpenVMS Entire Net-Work node tried to connect with node ID = 0.
Action | Specify a node ID in the configuration file on the UNIX or OpenVMS node.

NETT025 | TEXT MESSAGE RECEIVED ON LINK linkname
Explanation | A text message from an Entire Net-Work workstation node has been received on the identified link. The message is displayed immediately following the NETT025 message.
Action | See the Entire Net-Work 7 User's Guide or the Entire Net-Work 7 online documentation for a description of the message received from the workstation node.

NETT026 | SERVER MESSAGE DISCARDED FROM CLIENT ONLY LINK xxxxxxxx
Explanation | A server broadcast message was received from a partner Entire Net-Work node with a node ID of 0. The message is ignored and the servers listed in the message are inaccessible.
Action | If the servers on the partner machine need to be accessible from the mainframe, a node ID must be specified in the configuration file of the partner node.

NETT027 | NODE MESSAGE DISCARDED FROM CLIENT ONLY LINK
Explanation | A node message was received from a partner Entire Net-Work node with a node ID of 0. The message is ignored.
Action | No action is required for this informational message.

NETT028 | Entire Net-Work V5 IGNORES SERVERS ON NODES WITH A NODE ID OF 0
Explanation | A server broadcast message was received from a partner Entire Net-Work node with a node ID of 0. The servers on the partner node are ignored. This message is sent to the partner node as an informational message.
Action | No action is required for this informational messsage.