NETInn - ADAIOR Messages

#### Search Results

Search

# NETInn - ADAIOR Messages

These Entire Net-Work system messages are identical to the corresponding ADAInn messages documented in Adabas Messages and Codes documentation.

### Overview of Messages

`NETI02 | NETI22 | NETI23 | NETI24 | NETI29 | NETI32 | NETI91 | NETI92 | NETI93`

NETI02 | GETMAIN mmmmmmmm (ssssss)
Explanation | The first form of the message is written whenever memory is dynamically acquired and the requested memory is available. The second form of the message is written whenever memory is dynamically acquired and less than the requested memory is available. In the messages, mmmmmmmm is the amount of memory requested; aaaaaaaa is the amount of memory available; and ssssss (printed only under z/VSE), is the source of the memory (GETVIS, COMREG, ADABUF).

NETI22 | ADAIOR TRACE TABLE: --> IS CURRENT ENTRY
Explanation | This is an informational message that occurs when the ADAIOR TRACE TABLE is made active and printed.

NETI23 | node-id jobname ABEND CODE code
Explanation | z/VSE or BS2000: This message indicates that Entire Net-Work requested cancellation. A dump is normally also provided. The value code corresponds to the user abend code. For more information, see the section Entire Net-Work Abend Codes. The value jobname is the z/VSE job name or BS2000 program name.

NETI24 | node-id READY FOR OPERATOR COMMUNICATION
Explanation | SYSLOG displays this message once operator communications has been requested by the operator with the z/VSE 'MSG' command. The value 'node-id' is the target ID of the node.
Action | Enter a valid Entire Net-Work command.

NETI29 | OPER CMD: command
Explanation | z/VSE and BS2000: This message occurs in SYSLST as part of the session statistics during Adabas session termination. The value 'command' is the operator command last entered from SYSLOG.

NETI32 | node-id INTERNAL ERROR - FUNCTION funcname ERROR error
Explanation | An internal error has occurred in ADAIOR.
Action | Make a note of all recent messages, and contact your Software AG technical support representative.

NETI91 | Pause Element services initialized for zIIP
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has been successfully initialized. This message is issued only when Adabas is running with ADARUN parameter ZIIP=YES.
Action: | No action is required for this informational message.

NETI92 | Pause Element services terminated {normally │ at abend │ for zIIP │ by Resource Manager}
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has been successfully terminated. This message is only issued when Adabas is running with ADARUN parameter ZIIP=YES. This message may appear at termination following an abnormal end or cancel request.
Action: | No action is required for this informational message.

NETI93 | Pause Element {allocate │ deallocate │ pause │ release} error code ret code/rsn code
Explanation | Note: This message occurs only in z/OS environments. Event management using z/OS Pause Elements has returned an error. The unexpected return code (ret code) and reason (rsn code) are shown. This message is only issued when Adabas is running with ADARUN parameter ZIIP=YES. This message may appear at termination following an abnormal end or cancel request.
Action: | If this message appears at termination following an abnormal end or cancel request, no action is required. In any other circumstances, save the JES log, DDPRINT output and any dump of the Adabas nucleus and Contact your Software AG technical support representative for assistance.