About the Installation Tape

#### Search Results

Search

# About the Installation Tape

This document describes the installation tape. It covers the following topics:

- Data Sets Delivered

- Copying the Tape Contents

## Data Sets Delivered

This section describes the data sets that are delivered with the Event Replicator for Adabas. In all data set names, vrs represents the version, release, and maintenance level numbers of the release of the Event Replicator for Adabas.

The following data sets are delivered with the Event Replicator for Adabas on z/OS platforms:

Data Set Name | Contains
--- | ---
ARFvrs.INPL | INPL of the online application
ARFvrs.JOBS | Sample JCL
ARFvrs.LOAD | Load modules
ARFvrs.MTSI | Sample input to ADAMTS
ARFvrs.SRCE | Sample source members
ARFvrs.ZAPS | Zaps for support of the Event Replicator for Adabas

## Copying the Tape Contents

Copy the data sets from the supplied installation medium to your disk before you perform the individual installation procedure for each component to be installed.

The way you copy the data sets depends on the installation method and the medium used:

- If you use System Maintenance Aid (SMA), refer to the copy job instructions provided in the System Maintenance Aid documentation.

- If you are not using SMA and want to copy the data sets from CD-ROM, refer to the README.TXT file on the CD-ROM.

- If you are not using SMA and want to copy the data sets from tape, follow the instructions in this section.

This section explains how to copy all data sets from tape to disk.

#### Step 1: Copy Data Set COPY.JOB from Tape to Disk

- Modify the following sample job according to your requirements:

      //SAGTAPE JOB SAG,CLASS=1,MSGCLASS=X
      //* ---------------------------------
      //COPY EXEC PGM=IEBGENER
      //SYSUT1 DD DSN=COPY.JOB,
      // DISP=(OLD,PASS),
      // UNIT=(CASS,,DEFER),
      // VOL=(,RETAIN,SER=tape-volser),
      // LABEL=(2,SL)
      //SYSUT2 DD DSN=hilev.COPY.JOB,
      // DISP=(NEW,CATLG,DELETE),
      // UNIT=3390,VOL=SER=disk-volser,
      // SPACE=(TRK,(1,1),RLSE),
      // DCB=*.SYSUT1
      //SYSPRINT DD SYSOUT=*
      //SYSIN DD DUMMY
      //

  where:

  `tape-volser` is the VOLSER of the tape, for example: `T12345`,
  `hilev` is a valid high-level qualifier, and
  `disk-volser` is the VOLSER of the disk.

- Execute the job to copy the data set `COPY.JOB` to your disk.

#### Step 2: Modify hilev.COPY.JOB on Your Disk

- Modify `hilev.COPY.JOB` according to your requirements:

  Set `EXPDT` to a valid expiration date, for example, `99365`.

  Set `HILEV` to a valid high-level qualifier, for example, `USERLIB`.

  Set `LOCATION` to a storage location, for example, `STORCLAS=ABC` or `UNIT=3390,VOL=SER=USR123`.

#### Step 3: Submit COPY.JOB

- Execute `hilev.COPY.JOB` to copy single, multiple, or all data sets to your disk.

### On this page

- Data Sets Delivered
- Copying the Tape Contents