Zap Naming Convention

#### Search Results

Search

# Zap Naming Convention

The naming convention used for Entire Net-Work zaps is:

    Wcvrsnnn

Each of the letters in this naming convention is now described.

> W

>   The letter W is used to indicate that the zap is for the Software AG Entire Net-Work product.

> c

>   Specifies a system component code that identifies the Entire Net-Work component to which the zap applies. The following table describes the component codes that might be used in an Entire Net-Work zap:

>   Code | Entire Net-Work Component
>   --- | ---
>   D | z/VSE-dependent mainline
>   M | Operating system-independent mainline
>   O | OS/390 and z/OS-dependent mainline
>   T | Operating system-independent, Simple Connection Line Driver
>   U | Simple Connection Line Driver z/OS-dependent
>   V | Simple Connection Line Driver z/VSE-dependent
>   Y | Optional zaps, placed in the ZAPOPT member in the WCPvrs.MVSSRCE library.
>   Z | Simple Connection Line Driver BS2000-dependent

> v

>   Identifies the version number of Entire Net-Work.

> r

>   Identifies the release number of Entire Net-Work.

> s

>   Identifies the system maintenance (SP) level number of Entire Net-Work.

> nnn

>   Specifies the actual zap number.