APSPSX* - ADAECS or ADATCP Messages

#### Search Results

Search

# APSPSX* - ADAECS or ADATCP Messages

The informational messages beginning with APSPSX are ADAECS (Conversion Services) or ADATCP (TCP/IP interface) messages from the ISE/POSIX subsystem that occur when running the nucleus. The same messages appear with ADACMP and other programs that call the modules ADAECS or ADATCP.

### Overview of Messages

`APSPSX0008 | APSPSX0012 | APSPSX0015 | APSPSX0027 | APSPSX0036 | APSPSX0049 | APSPSX0050`

APSPSX0008 | {ADAECS | ADATCP} ISE/POSIX Vvrs system initialized nucleus size bytesK bytes
Explanation | The ISE/POSIX subsystem has been successfully initialized.
Action | No action necessary for this informational message.

APSPSX0012 | {ADAECS | ADATCP} ISE/POSIX {CDI PH FILE | Vvrs} system terminated
Explanation | The ISE/POSIX subsystem server has terminated.
Action | No action necessary for this informational message.

APSPSX0015 | {ADAECS | ADATCP} ISE/POSIX Vvrs initialization in progress
Explanation | The ISE/POSIX subsystem server has started its initialization processing.
Action | No action necessary for this informational message.

APSPSX0027 | {ADAECS | ADATCP} initializing with configuration 'PAANCONF'
Explanation | Indicates the ISE/POSIX subsystem configuration module is being used.
Action | No action necessary for this informational message.

APSPSX0036 | {ADAECS | ADATCP} global environment variables processed successfully
Explanation | The global environment variable file of the ISE/POSIX subsystem was processed successfully and the global environment variables specified in the file were successfully defined.
Action | No action necessary for this informational message.

APSPSX0049 | Required configuration parameter parameter missing or invalid
Explanation | During the initialization of a CDI protocol driver, a required configuration parameter was missing or invalid. This initialization cannot proceed.
Action | Add or correct the specified parameter and restart the nucleus. See the Adabas Installation documentation for more information.

APSPSX0050 | {ADAECS | ADATCP} ISE/POSIX CDI file protocol initialized
Explanation | The ISE/POSIX subsystem CDI protocol driver implementing the file protocol was successfully initialized.
Action | No action necessary for this informational message.