SMARTS Messages and Codes

#### Search Results

Search

# SMARTS Messages and Codes

This documentation describes the SMARTS messages and codes issued by the SMARTS system. Some messages and codes appear in all SMARTS environments; other messages and codes appear only in the SMARTS server environment.

The documentation also contains errno mapping tables for the various errors returned by program functions and the various CDI modules used by SMARTS.

This information is organized as follows:

Introduction | Explains message format and structure .
SMARTS Abend Codes | Messages with prefix U, ABEND
SMARTS API Messages | Messages with prefix APSPSX
SMARTS Server Environment Messages | Messages with prefix ABE, ABS, ADA, BPM, DIS, INI, INP, LOD, OPC, OUS, RES, ROL, RSM, STG, SVR, TIB, TMR, ZDM, ZLA, ZOS, ZTR, ZTS
Allocated Error Numbers | Each errno value that may be returned to a PAANHLL request, its equivalent C macro name and a short description of what the errno means.
SMARTS Server Environment Internal Macro Description | Return codes from SMARTS internal functions.
Request Status Codes | Return and feedback codes indicating processing results of the request.