UDUMP Utility

#### Search Results

Search

# UDUMP Utility

### Overview of Messages

`DMP0001 | DMP0002 | DMP0003 | DMP0100 | DMP0101 | DMP1000 | DMP1001 | DMP1002`

DMP0001 | Invalid dump number requested from TTTLOG
Explanation: | This message is associated with the Com-plete utility UDUMP. It appears when the Com-plete module TTTLOG requested a non-existent dump number.
System action: | The dump request is ignored. Normal processing continues.
Terminal operator info: | Notify the Com-plete system programmer.
System programmer info: | This message indicates a logic error in the Com-plete user program abend recovery routine of Com-plete . Contact Com-plete technical support.

DMP0002 | Disk error on dump read or write from TTABND
Explanation: | This message is associated with the Com-plete utility UDUMP. It appears when a disk error was detected while the Com-plete module TTDUMP was either reading the message file or writing the contents of main storage to a disk.
System action: | The dump is not read or written. Normal processing continues.
Terminal operator info: | This error was probably caused by a hardware failure. Notify the Com-plete system programmer.
System programmer info: | If this problem continues to appear, take appropriate action to reinitialize and restore the Com-plete SD.

DMP0003 | Invalid device type requested dump
Explanation: | This message is associated with the Com-plete utility UDUMP. It appears when a UDUMP request was entered from a terminal device type that may not use UDUMP.
System action: | The requested operation is not performed. UDUMP is cancelled.
Terminal operator info: | The terminal being used may not use the UDUMP utility. Examine program's dump from another device type.

DMP0100 | Invalid dump no in parm list
Explanation: | This message is associated with the Com-plete utility TUDUMP. It appears when a dump number outside the permitted range is detected - either in (field) size or in value.
System action: | The last dump is not printed. The output shows all input parameters and contains all dumps requested in SD-file sequence prior to the dump that led to abortion.
Terminal operator info: | This error should not occur. Its occurrence points to a serious impact in either the dump file organization or the executing module. Inform the system programmer.

DMP0101 | Parm list name/number mismatch
Explanation: | This message is associated with the Com-plete utility TUDUMP. It appears when a dump is requested, that is found to contain a different program name in the header record than the one associated with the dump number before invoking the print routine.
System action: | The last dump is not printed. The output shows all input parameters and contains all dumps requested in SD-file sequence prior to the dump that led to abortion.
Terminal operator info: | This error should not occur. Its occurrence points to a serious impact in either the dump file organization or the executing module. Inform the system programmer.

DMP1000 | No dump
Explanation: | This message is associated with the Com-plete utility TUDUMP. It appears when the read subroutine is unable to address a desired record by the calculated record number.
System action: | The last dump is not printed. The output shows all input parameters and contains all dumps requested in SD-file sequence prior to the dump that led to abortion.
Terminal operator info: | This error should not occur. Its occurrence points to a serious impact in either the dump file organization or the executing module. Inform the system programmer.

DMP1001 | Disk error
Explanation: | This message is associated with the Com-plete utility TUDUMP. It appears when the read subroutine is unable to access a requested record.
System action: | The last dump is not printed. The output shows all input parameters and contains all dumps requested in SD-file sequence prior to the dump that led to abortion.
Terminal operator info: | This error should not occur. Its occurrence points to a serious impact in either the dump file organization or the executing module. Inform the system programmer.

DMP1002 | Dump address outside dump
Explanation: | This message is associated with the Com-plete utility TUDUMP. It appears when the dump record addressed contains invalid or uninterpretable data and/or is found to be not a dump record.
System action: | The last dump is not printed. The output shows all input parameters and contains all dumps requested in SD-file sequence prior to the dump that led to abortion.
Terminal operator info: | This error should not occur. Its occurrence points to a serious impact in either the dump file organization or the executing module. Inform the system programmer.