2740 Device Support

#### Search Results

Search

# 2740 Device Support

### Overview of Messages

`ZA10001 | ZA10002 | ZA10003`

ZA10001 | Permanent error - Tid $1 - Sense $2 - Input
Explanation: | This message is associated with the Com-plete 2740 device module. It appears when four successive hardware errors have occurred while Com-plete was attempting to read TID $1.
System action: | If TID $1 was in conversation with a program when the errors occurred, control is passed to the program at the point immediately following the WRITE instruction and a return code of 12 is set. If TID $1 was not in conversation with a program when the errors occurred, Com-plete not responds as if null input had been entered and attempts to print the ZAM00001 message again.
System programmer info: | The value $2 is the hardware sense information describing the error. The bit settings are as follows: bit 0 - command reject bit 1 - intervention required bit 2 - bus out check bit 3 - equipment check bit 4 - data check bit 5 - overrun bit 6 - lost data (BID key) bit 7 - timeout
Computer operator info: | Seek assistance of the Com-plete system programmer. Place the terminal indicated by TID $1 on IGNORE status until the problem can be resolved.

ZA10002 | Permanent error - Tid $1 - Sense $2 - Output
Explanation: | This message is associated with the Com-plete 2740 device module. It appears when four successive hardware errors have occurred while Com-plete was attempting to write to TID $1.
System action: | If TID $1 was in conversation with a program when the errors occurred, control is passed to the program at the point immediately following the WRITE instruction and a return code of 12 is set. If the write operation was not a conversational write but was performed at the request of a user program, Com-plete attempts to write the ZAM00012 message and aborts the output that was to be written.
System programmer info: | The value $2 is the hardware sense information describing the error. The bit settings are as follows: bit 0 - command reject bit 1 - intervention required bit 2 - bus out check bit 3 - equipment check bit 4 - data check bit 5 - overrun bit 6 - lost data (BID key) bit 7 - timeout
Computer operator info: | Seek the assistance of the Com-plete system programmer. If the message continues to appear, it may be necessary to place the terminal indicated by TID $1 on IGNORE status until the problem can be determined.

ZA10003 | Tid $1 had been deleted due to 4 successive timeouts
Explanation: | This message is associated with the Com-plete 2740 device module. It appears when four successive timeouts have occurred due to hardware errors occurring while Com-plete is attempting to write to TID $1.
System action: | Com-plete attempts to write the ZAM00012 message and aborts any output that was to be written. Any programs in conversation with the terminal are abnormally terminated, and an online dump is generated.
System programmer info: | The terminal identified by $1 has been placed in deleted status because of permanent hardware errors. Additional messages have been written to the operator console that further identify the nature of the errors.
Computer operator info: | Seek the assistance of the Com-plete system programmer.