Teletype Support

#### Search Results

Search

# Teletype Support

### Overview of Messages

`ZA60001 | ZA60002 | ZA60003 | ZA60004 | ZA60005 | ZA60010 | ZA60011`

ZA60001 | Com-plete is active
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that communications have been established with the Com-plete system after successfully dialing in with a dialup terminal.
System action: | This message is informational only; processing continues normally.
Terminal operator info: | The Com-plete system is now available for communication.
System programmer info: | This message is generated by module TLAMTTY and exists in TTY character code.

ZA60002 | Data check - please reenter
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that an input data check or parity error has occurred.
System action: | This message is informational only. Processing continues normally.
Terminal operator info: | Reenter the input. If the error persists, consult the Com-plete system programmer.
System programmer info: | If this message persists, check to ensure that the terminal and line devices are functioning properly. Verify that the terminal parity settings match the value specified for the PARITY= parameter of the LGCB macro statement in TIBTAB for the line in question.

ZA60003 | Input data too long - please reenter
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that too many characters have been entered. The maximum number of characters that may be entered is controlled by the Com-plete system programmer.
System action: | This message is informational only. Processing continues normally.
Terminal operator info: | Reenter the input. Note that backspace characters count as entered characters. If the error persists, consult the Com-plete system programmer.
System programmer info: | The maximum number of input characters is controlled by the BUFFER= parameter of the LGCB macro in TIBTAB for the line in question. For more information, refer to the Com-plete System Programmer's Manual.

ZA60004 | Timeout - please reenter
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that too much time has been taken to enter data. The normal limit is 23 seconds between each character.
System action: | This message is informational only. Processing continues normally.
Terminal operator info: | Reenter the input and decrease the amount of pause time between entries.
System programmer info: | The timeout value is affected by the terminal control unit either hardware or software (e.g., 3705 EP), and by specification of OPT=READ with the LGCB macro in TIBTAB. OPT=INHIBIT, which is the default, will inhibit timeouts.

ZA60005 | Tib $1 ignored due to 9 successive errors
Explanation: | This message is associated with the teletype support of Com-plete . It is issued when Com-plete detects that all I/O to a specific TTY device has failed nine successive times. The specific nature of the I/O failures is listed individually when each failure occurs as separate ZA6 messages.
System action: | Com-plete considers the device to be permanently inoperative. A 'DISABLE' is written to the device and processing is discontinued (as though an IGN command had been received from the computer operator).
Computer operator info: | When the device becomes operational again, reactivate it using the RES command.

ZA60010 | CCWOP=$1 LID=$2 SENSE=$3 CSW=$4 TTY line or model error
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that an apparent line or modem error has occurred.
System action: | This message is informational only; processing continues normally.
System programmer info: | The data in the message indicates the nature of the problem. The fields are defined as follows: $1 - Channel program op code: 2F=disable, 27=enable, 01=write 02=read, 0A=inhibit $2 - Line ID $3 - Sense data from terminal control unit (see the appropriate hardware manual) $4 - Device and channel status from CSW.
Computer operator info: | Ignore the message and restart the line. If the problem persists, notify the Com-plete system programmer of the problem.

ZA60011 | CCWOP=$1 LID=$2 SENSE=$3 CSW=$4 TTY unusual error
Explanation: | This message is associated with the teletype support of Com-plete . It indicates that an unknown type of error has occurred.
System action: | This message is informational only; processing continues normally.
System programmer info: | The data in the message indicates the nature of the problem. The fields are defined as follows: $1 - Channel program op code: 2F=disable, 27=enable, 01=write, 02=read, 0A=inhibit $2 - Line ID $3 - Sense data from terminal control unit (see the appropriate hardware manual) $4 - Device and channel status from CSW.
Computer operator info: | Ignore the message and restart the line. If the problem persists, notify the Com-plete system programmer of the problem.