2741 Support

#### Search Results

Search

# 2741 Support

### Overview of Messages

`ZA70001 | ZA70002 | ZA70003 | ZA70004 | ZA70005 | ZA70010 | ZA70011`

ZA70001 | Com-plete IS ACTIVE
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that communications have been established with the Com-plete system after successfully dialing in with a dialup terminal.
System action: | This message is informational only; processing continues normally.
Terminal operator info: | The Com-plete system is now available for communication.

ZA70002 | DATA CHECK - PLEASE REENTER
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that an input data check or parity error has occurred.
System action: | This message is informational only; processing continues normally.
Terminal operator info: | Reenter the input. If the error persists, consult the Com-plete system programmer.
System programmer info: | If message ZA700002 persists, check to ensure that the terminal and line devices are functioning properly. Verify that the terminal parity settings match the value specified for the PARITY= parameter of the LGCB macro statement in TIBTAB for the line in question.

ZA70003 | INPUT DATA TOO LONG - PLEASE REENTER
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that too many characters have been entered. The maximum number of characters that may be entered is controlled by the Com-plete system programmer.
System action: | This message is informational only; processing continues normally.
Terminal operator info: | Reenter the input. Note that backspace characters count as entered characters. If the error persists, see the Com-plete system programmer.
System programmer info: | The maximum number of input characters is controlled by the BUFFER= parameter of the LGCB macro in TIBTAB for the line in question. For more information, refer to the Com-plete System Programmer's Manual.

ZA70004 | TIMEOUT - PLEASE REENTER
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that too much time has been taken to enter data. The normal limit is 23 seconds between each character.
System action: | This message is informational only; processing continues normally.
Terminal operator info: | Reenter the input and decrease the amount of pause time between entries.
System programmer info: | The timeout value is affected by the terminal control unit, either either hardware or software (e.g., 3705 EP), and by specification of OPT=READ with the LGCB macro in TIBTAB. OPT=INHIBIT, which is the default, will inhibit timeouts.

ZA70005 | TIB $1 IGNORED DUE TO 9 SUCCESSIVE ERRORS
Explanation: | This message is associated with the 2741 support of Com-plete . It is issued when Com-plete detects that all I/O to a specific device has failed nine successive times. The specific nature of the I/O failure is listed individually when each failure occurs as separate ZA7 message.
System action: | Com-plete considers the device to be permanently inoperative. A 'DISABLE' is written to the device and processing is dicontinued (as though an IGN command had been received from the computer operator).
Computer operator info: | When the device becomes operational again, reactivate it using the RES command.

ZA70010 | CCWOP=$1 LID=$2 SENSE=$3 CSW=$4 2741 LINE OR MODEM ERROR
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that an apparent line or modem error has occurred.
System action: | This message is informational only. Processing continues normally.
System programmer info: | The data in the message indicates the nature of the problem. The fields are defined as follows: $1 - Channel program op code: 2F=disable, 27=enable, 01=write, 02=read, 0A=inhibit $2 - Line ID $3 - Sense data from terminal control unit (see the appropriate hardware manual) $4 - Device and channel status from CSW.
Computer operator info: | Ignore and restart the line. If the problem persists, notify the Com-plete system programmer of the problem.

ZA70011 | CCWOP=$1 LID=$2 SENSE=$3 CSW=$4 2741 UNUSUAL ERROR
Explanation: | This message is associated with the 2741 support of Com-plete . It indicates that an unknown type of error has occurred.
System action: | This message is informational only. Processing continues normally.
System programmer info: | The data in the message indicates the nature of the problem. The fields are defined as follows: $1 - Channel, program op code: 2F=disable, 27=enable, 01=write, 02=read, 0A=inhibit $2 - Line ID $3 - Sense data from terminal control unit (see the appropriate hardware manual) $4 - Device and channel status from CSW.
Computer operator info: | Ignore and restart the line. If the problem persists, notify the Com-plete system programmer of the problem.