Terminal Device Type Codes

#### Search Results

Search

# Terminal Device Type Codes

The terminal device type codes listed in the following figure are used exclusively in the creation of TIBTAB. The columns abbreviated SS, LL, and LD represent:

Default SS | Screen Size, in characters
Default LL | Line Length
Default LD | Line Depth (number of lines)

The values listed for these items can be changed within the TIBTAB by specifying the keyword arguments FORMAT, LEN, and LINES when coding the TIB.

Terminal | Terminal Type | SS | LL | LD
--- | --- | --- | --- | ---
Device Code |
BATCH | (Indicates that TIB may be used by batch)
TTY | TELETYPE | - | 80 | 26
TTYD | TELETYPE (DIAL) | - | 80 | 26
3270 L | IBM 3270 LOCAL | 1920 | 80 | 24
3270 R | IBM 3270 REMOTE | 1920 | 80 | 24
3275 R | IBM 3275 REMOTE | 1920 | 80 | 24
3278 L | IBM 3278 LOCAL | 1920 | 80 | 24
3278 R | IBM 3278 REMOTE | 1920 | 80 | 24
3279 L | IBM 3279 LOCAL | 2560 | 80 | 32
3279 R | IBM 3279 REMOTE | 2560 | 80 | 32
3284 L | IBM 3284 LOCAL | - | 120 | 20
3284 R | IBM 3284 REMOTE | - | 120 | 20
3286 L | IBM 3286 LOCAL | - | 120 | 20
3286 R | IBM 3286 REMOTE | - | 120 | 20
3287 L | IBM 3287 LOCAL | - | 132 | 18
3287 R | IBM 3287 REMOTE | - | 132 | 18
3288 L | IBM 3288 LOCAL | - | 132 | 18
3288 R | IBM 3288 REMOTE | - | 132 | 18