Terminal Device Type Codes

#### Search Results

Search

# Terminal Device Type Codes

The terminal device type codes listed in the following table are used exclusively in the creation of TIBTAB. The columns abbreviated SS, LL, and LD represent:

SS = Screen Size (in characters)
LL = Line Length
LD = Line Depth (number of lines)

The values listed for these items can be changed within the TIBTAB by specifications of the keyword arguments FORMAT, LEN, and LINES when coding the TIB and LGCB macros.

Terminal Device Code | Terminal Type | Groupname | SS | LL | LD
--- | --- | --- | --- | --- | ---
BATCH | (Indicates that TIB may be used by batch)
TTY | TELETYPE | TTY | - | 80 | 26
TTYD | TELETYPE (DIAL) | TTYD | - | 80 | 26
3270 L | IBM 3270 LOCAL | 3270I | 1920 | 80 | 24
3270 R | IBM 3270 REMOTE | 3270R | 1920 | 80 | 24
3275 R | IBM 3275 REMOTE | 3275R | 1920 | 80 | 24
3278 L | IBM 3278 LOCAL | LOCAL |  | 80 | 24
3278 R | IBM 3278 REMOTE | 3270R |  | 80 | 24
3279 L | IBM 3279 LOCAL | LOCAL | - | 80 | 32
3279 R | IBM 3279 LOCAL | 3270R | - | 80 | 32
3284 L | IBM 3284 LOCAL | LOCAL | - | 120 | 20
3284 R | IBM 3284 REMOTE | 3270R | - | 120 | 20
3286 L | IBM 3286 LOCAL | LOCAL | - | 120 | 20
3286 P | IBM 3286 REMOTE | 3270R | - | 120 | 20
3288 L | IBM 3288 LOCAL | LOCAL | - | 132 | 18
3288 R | IBM 3288 REMOTE | 3270R | - | 132 | 18