Operator Command Overview

#### Search Results

Search

# Operator Command Overview

The following table summarizes the Com-plete operator commands:

Command | Purpose
--- | ---
ACCESS | Allows the operator to start or shutdown the ACCESS interface.
ALLOW | Enables the computer operator to allow use of the following Com-plete facilities by terminal users: remote job entry and ULOG ON functions.
CANCEL | Enables the computer operator to terminate an online application program abnormally.
CLOSE | Causes the current Com-plete capture data set to be closed, and, therefore, available for access by batch jobs.
COMSEC | Allows the computer operator to issue Com-plete security commands (only available if Com-plete security is installed.
DCTRL | Allows the computer operator to display and monitor terminals with control status in the Com-plete network.
DISALLO | Enables the computer operator to disallow use of the following facilities by terminal users: remote job entry and ULOG ON functions.
DTASKS | Displays the status of all Com-plete tasks (including the threads) and batch jobs using Com-plete functions.
DUMP | z/VSE: Write a dump of the Com-plete partition to POWER.
ENQ | Displays a selection of or all outstanding ENQs from Com-plete's threads.
EOJ | Causes a logical shutdown to occur for the Com-plete system.
FORCE | Enables the computer operator to force a terminal or user from the Com-plete system.
HMSG | Causes Com-plete to reissue the message Com-plete IS NOW OPERATIONAL to all or selected terminals.
IGNORE | Causes immediate termination of terminal I/O for one or more terminals, lines, or user IDs. If a user is logged on, and the IGNORE command is entered for the user's terminal or user ID, the user is logged off from the terminal.
LOGOFF | Logs off one or more terminals or users.
MSG | Sends a message to one or more terminals or users.
PGM | Enables the computer operator to load, delete, or refresh RESIDENTPAGE modules.
PLIST | Displays a list of the current tasks defined in the requested task group and the status of each.
QOVER | Displays a list of the current queues defined in the system and the status of each.
QUIESCE | Causes Com-plete's VTAM application to quiesce.
RESTART | Restarts terminal I/O for one or more terminals or lines.
SERV | Enables a server to be stopped or started.
SETCTL | Enables the computer operator to dynamically set a designated terminal to control or privileged status, allowing it to perform functions not normally permitted.
STATS | Writes the current Com-plete statistics to the sysout data set.
STOP | Synonym for the EOJ command.
TASKS | Attaches additional operating system tasks in a Com-plete task group or to detach some of the tasks of a task group.
TLIST | Displays a list of the current threads defined in the requested thread group and the status of each.
UNCTL | Enables the computer operator to remove control status from a specified terminal.
USER | Enables a user program to be attached with or without data. A special parameter, UFILE, allows the operator to change the status of a file.
UU | Allows the display of information about one or more active users.
VTAM | Allows the computer operator to perform certain functions on the Com-plete VTAM interface.