Using Non-Standard Uncompressed Format within SCT Plus2000-Specific Rotated Arrays
1. Select Import from RMS SCT COBOL FD Files or Import from VSAM SCT COBOL FD Files in the Import CDD dialog box.
2. Type an RMS or VSAM SCT COBOL FD file name.
3. Select Use uncompressed format and click OK.
You can also use the Browse button below the text box to locate files to import.
If you are not connected to a VMS server, the CONNX Database Login dialog box appears.
You can use the following wildcard syntax to import multiple SCT COBOL FD files from the SIS module: SI$SOURCE:*RC.LIB
Note:
If CONNX detects more than one record layout when importing, multiple data dictionary entries are created.
Note:
Multiple files can be specified in the Enter an SCT COBOL FD file name text box by separating each file name with a comma. The allowed limit is 255 characters.
Type the server name or IP address, a user name, and password in the corresponding text boxes. Port 6500 is listed in the TCPIP Port text box by default. Click OK.
4. The Browse dialog box appears. Select the file(s) and click OK to return to the Import CDD dialog box.
5. Type the server name or IP address, a user name, and password in the corresponding text boxes on the Logon Information tab.
6. Port 6500 is listed in the TCP/IP Port text box by default. Any change made to the port setting in this text box becomes a permanent change to the port setting of the imported database.
7. Select the destination database from the Destination Database list box.
8. Click OK.
The RMS data files name is automatically entered in the table properties using the standard SCT data logicals.
9. Save the CDD.
The selected RMS or VSAM SCT COBOL FD files appear in the CONNX Data Dictionary Manager window.