Installing the CONNX Components
Installing the Selected Components on the OS/390 Target
1. Log on the target OS/390 system. Given the default data set prefix of CONNX.CICS, the ftp process creates a JCL control record partitioned data set with the name and members listed in the following table.
2. Edit the INST member and change the job card to match your site standards.
3. Submit this job to the batch execution queue.
Default Partitioned Data Set Name = CONNX.CICS.CNTL

Member | Purpose
INST | The CONNX and SAS/C 7.00 installation job built by the CONNX VSAM installation program.
INST02 | The CONNX installation job created by the CONNX PC installation program. Submit this job to install CONNX onto a second CICS region.
REMOV0 | CONNX for VSAM uninstallation JCL.
CICSALOC | JCL Procedure to allocate the SAS/C CICS transient data queues.
CICSDCT | Sample CICS Destination Control Table (DCT) source with entries for the IBM CICS TCP/IP interface and the SAS/C extra-partition transient data queues.
CICSDCTJ | Sample JCL to assemble / link-edit the CICSDCT source code into a target CICS load library.
CNXCSD | JCL procedure to execute IBM DFHCSDUP utility and define CONNX CICS components to a target RDO VSAM file.
CNXFCT0 | FCT source for CONNX CICS/VSAM configuration and sample files.
CNXIDC | JCL procedure to execute IDCAMS to delete/define/load CONNX VSAM components.
CNXLINK | JCL procedure to execute the IBM linkage editor against CONNX prelinked SAS/C 7.00 object code and to create the CONNX CICS and batch load modules.
CNXLOAD | JCL procedure to delete/allocate a separate load library for the CONNX CICS programs.
CNXPPT0 | PPT source for CONNX CICS/VSAM programs.
CSDFILE0 | IBM DFHCSDUP utility control records to define the CONNX TCP/IP server VSAM configuration file to the target CICS RDO VSAM file.
CSDPROG0 | IBM DFHCSDUP utility control records to define the CONNX CICS programs and transactions to the target CICS RDO VSAM file.
CSDSAMP0 | IBM DFHCSDUP utility control records to define the CONNX CICS sample VSAM files, paths, and alternate indexes to the target CICS RDO VSAM file.
IDCCNX0 | IDCAMS control records to drop the CONNX TCP/IP server VSAM configuration file.
IDCCUST0 | IDCAMS control records to delete/define/load the CONNX sample VSAM customer file.
IDCEQU00 | IDCAMS control records to delete/define/load the CONNX sample VSAM equipment file.
IDCEQU01 | IDCAMS control records to define the CONNX sample VSAM equipment file alternate index #1.
IDCEQU02 | IDCAMS control records to define the CONNX sample VSAM equipment file alternate index #2.
IDCEQU03 | IDCAMS control records to build the CONNX sample VSAM equipment file alternate index #1.
IDCEQU04 | IDCAMS control records to build the CONNX sample VSAM equipment file alternate index #2.
IDCORD00 | IDCAMS control records to delete/define/load the CONNX sample VSAM order file.
IDCORD01 | IDCAMS control records to define the CONNX sample VSAM order file alternate index #1.
IDCORD02 | IDCAMS control records to define the CONNX sample VSAM order file alternate index #2.
IDCORD03 | IDCAMS control records to build the CONNX sample VSAM order file alternate index #1.
IDCORD04 | IDCAMS control records to build the CONNX sample VSAM order file alternate index #2.
IDCPGRP0 | IDCAMS control records to delete/define/load the CONNX sample VSAM product group file.
IDCPROD0 | IDCAMS control records to delete/define/load the CONNX sample VSAM product file.
LNKCFG | IBM linkage editor control records for CONNX CICS load module CNXCFG.
LNKRUN | IBM linkage editor control records for CONNX CICS load module CNXRUN.
LNKSTOP | IBM linkage editor control records for CONNX load module CNXSTOP.
LNKVSAM | IBM linkage editor control records for CONNX CICS load module CNXVSD0.

If you requested that a new CONNX load library be created by specifying a new PDS name in the Target Load Library text box of the installation program, then the example CONNX CICS load library is allocated. In both cases, the CONNX load module members are linked into the Target Load Library PDS:
CONNX.CICS.LOAD
CNXCFG
CNXRUN
CNXVSD0
CNXSTOP
After the required CONNX CICS components are installed, they must be defined to the target CICS region. The CONNX installation automates the definition of CONNX CICS programs, files, and transactions to the target region RDO file. Depending on the CICS version and release installed on the target region, optional manual steps include updating the DCT (Destination Control Table), the PPT (Program Processing Table), and PCT (Program Control Table). If the CONNX load modules were linked into a new load library, then the final required manual step is to add the CONNX load library (default name = CONNX.CICS.LOAD) to the target CICS region startup JCL DFHRPL (Run Program List) DDNAME.