Installing the CONNX VSAM Components on a VSE System

  Installing the CONNX for VSAM-VSE Components
  Required and Optional Entry Fields for VSAM TCP/IP Server Setup
  VSAM Objects for CONNX.CICS.SAMPLES

Installing the CONNX for VSAM-VSE Components
This step copies the CONNX VSAM server components from a client PC to a VSE target. The CONNX Administrator component must be installed on the client PC.
When installing the VSAM components, select a VSE user account name and password with privileges that allow you to create VSE libraries in VSAM-managed space and to copy, read, and write files via FTP to the target host.
1. Launch CONNX Server Setup.
2. In the CONNX Server Component Installation dialog box, select the VSE tab.
3. In the CONNX Server Library area, enter the fully qualified VSE cluster name which contains the CONNX VVRR library in CONNX Library DSN and its VOLSER in the VOLSER text box. Enter the CONNX library name defined in the CONNX library cluster in CONNX Library Label, the data set name of the VSE user catalog where the CONNX sample files and managed library are defined in Catalog DSN, and the system data label which references the physical data set name of the User Catalog in Catalog Label.
Note:
If CONNX Library Label is blank, the library name defaults to CNXWRR. If Catalog DSN is blank, CONNX files are defined in the default VSE system catalog. If Catalog Label is blank, the data label defaults to IJSYSCT.
4. In the Login Information area, type the TCP/IP symbolic host name or dotted numeric address for your VSE server in the Server text box, a privileged user account name in the User ID text box and its password in the Password text boxes. Under Product, click VSAM and under Server Type, click CICS.
5. In the TCP/IP Stack area, if you are using the Barnard TCP/IP stack rather than CSI, select the Barnard radio button. For Mode, select either Active or Passive FTP mode. Unless your system is not configured to support Passive mode FTP, you should select Passive. If the FTP transfer fails for any reason other than the user id or password was entered incorrectly, switch modes and try again.
Enter the TCP/IP stack location in TCP/IP HLQ.
Note:
To enable the environment variable for the Barnard TCP/IP stack, set CNXBARNARD to 1 in the CONNX Configuration Utility.
6. In the CICS Parameters area, see the table in Required and Optional Entry Fields for VSAM TCP/IP Server Setup for a detailed explanation of the information required in Target RDO File.
7. In the VSAM Samples Group area, if you clear the Create check box, CONNX will not create the CONNX VSAM sample KSDS, RRDS, and ESDS data sets. If the Create check box is selected, the CONNX VSAM sample KSDS, RRDS, and ESDS data sets and the VSAM clusters described in VSAM Objects for CONNX.CICS.SAMPLES are created, defined to the target CICS region, and given the data set prefix specified in Database HLQ.