Uninstalling CONNX Started Task Components
Overview
The CONNX for VSAM TCP/IP Server Setup client application transfers the CONNX components to the target MVS-OS/390 host via TCP FTP. After the initial FTP step, the CONNX installation continues via a batch job submission using TSO ISPF. Final installation steps for the CONNX for VSAM Started Task components include manual additions of JCL procedures (CNXVSAM and CNXVSCT) and a REXX exec file (CNXCFG) to the system PROCLIB and SYSPROC partitioned data sets.
Given a default CONNX installation prefix of CONNX.V08R09.STASK, the CONNX for VSAM Started Task installation JCL partitioned data set is CONNX.V08R09.STASK.CNTL. Members REMOVE and REMOV01 contain batch uninstallation JCL. Use REMOVE if you installed the CONNX sample VSAM / QSAM / PDS data sets; otherwise, use REMOV01.