Required and Optional Entry Fields for Adabas TCP/IP Server Setup - VSE

Group Box | Term | Description
Login Information | Server | A symbolic or dotted numeric TCP/IP address, for example: MVS or 123.123.123.123
User ID | Your 1-8 character VSE logon ID. All characters convert from lowercase to uppercase.
Password | Your 1-8 character VSE password. All characters convert from lowercase to uppercase.
TCP/IP Stack | CSI | CSI International TCP/IP connectivity.
Barnard | The Barnard TCP/IP communications stack.
TCP/IP HLQ | The TCP/IP symbolic host name or dotted numeric address for your VSE system.
CONNX Server Library | CONNX Library DSN | A one- or multi-part high-level data set name, which is used to create the CONNX installation sequential and partitioned data sets on the target host.
VOLSER | The DASD volume serial on which the CONNX.Adabas sequential and partitioned data sets are created. Optional: The DASD volume serial on which the CONNX.ADABAS sequential and partitioned data sets are created.
CONNX Library Label | The 1-44 character fully qualified VSE Adabas SQL Cluster name that contains the CONNX VVRR Adabas SQL Gateway library. The default is CNXV9R0.
Catalog DSN | The 1-44 character physical data set name of the VSE Adabas SQL Gateway user catalog into which the Adabas SQL Gateway-managed library are defined. If left blank, the CONNX files are defined in the default VSE system catalog.
Catalog Label | The 1-7 character system data label which references the physical data set name of the Adabas SQL Gateway User Catalog.
CICS Parameters | Target RDO File | System Management File location.
Adabas Parameters | Link Stub Library | Location of the Software AG CICS High Performance Stub Routine.