Component Configuration
Consider the following when planning the CONNX install service configuration:
The CONNX Client must be installed on every machine that accesses data. This means that you could need many CONNX Client installations for a desktop application, or only a few installations for organizations using a distributed or web service framework. Each configuration has its particular installation, administration, and maintenance constraints.
The CDD repository location is very important. The CDDs must be available to every client machine; you could need to open a share on a file server and set appropriate access permissions. You could need multiple CDD copies (the development, test, and deploy cycles could each require a separate copy). This ncreases administration complexity.
A CONNX Remote server must be installed on remote hosts when a local server DLL cannot access data. You may have to open up a range of firewall ports and coordinate across departments to gain access to a particular machine.
The CONNX License server must be installed on a single server that has access to the LAN. Choose a dedicated server to ensure uninterrupted access to CONNX features.
The following discussion will be broken down into the aspects of a typical CONNX installation. Please refer to the organizational chart of CONNX Client and Server Components) throughout the discussion to help facilitate a clearer understanding.