Error Messages
The Adabas Event Replicator for LUW error message format is:
Error Code (Error Class): Explanation
There are six types of error messages:

Error Code | Message Type
1001 through 1999 | General Messages
2001 through 2999 | Admin
3001 through 4999 | Controller
5001 through 5999 | Event Consumer
6001 through 8999 | Event Producer
9001 through 9999 | Debug

There are two error classes:

Error Class | Description
W | Warning/ Informational
E | Error

There are four kinds of error actions:

Error Action Code | Error Action | Values
X | No action is performed. | N/A
L | A message is logged. | N/A
Nx | Message will notify. | Values N1 (infrequent notification) through N4 (always notify). Notification must be enabled.
L/Nx | Message will log and notify. | Values L/N1 (infrequent notification and always log) through L/N4 (always notify and log). Message always logs. Notification must be enabled to occur.

There are five error states:

Error State Code | Error State | Description
U | Uninitialized | No CDD is deployed.
N | Normal | System is running normally.
C | Configure | System is processing deployment information.
D | Disable Process | System is disabled. This usually happens due to an error or a Stop Server message. If this code is issued due to an error rather than a shutdown command, the default setting is for replication to continue. However, the error should be investigated, because there is a high probability that the transaction was not replicated.
S | Shutdown | System has received a Shutdown message.

The Message IDs below is composed of the error code, error class, error action, and error state.
General Messages
WARNINGS

Message ID | Explanation | Resolution
1001 | W | L | N | The application is initialized. | This message is informational.
1002 | W | L | S | The application is shutting down. | This message is informational.
1300 | W | L | N | The application state changed to: (ACTIVE). | The server has entered an active state.
1301 | W | L | C | The application state changed to: (CONFIGURE). | The server is processing a CDD for deployment.
1302 | W | L | D | The application state changed to: (DISABLED). | The server entered an inactive state. This could indicate that an error has occurred. Check log for more information.
1303 | W | L | S | The application state changed to: (SHUTDOWN). | The server has entered a shutdown state due to normal process control.
1304 | W | L | N | Application is attempting to switch identity: (<old identity>)-->(<new identity>). | No action is required.

ERRORS

Message ID | Explanation | Resolution
1501 | E | X | U | Unable to initialize application state. | An error has occurred while reading internal configuration files. Please contact technical support.
1502 | E | X | D | Unable to write to system log: (<path to log file>). | An error occurred while writing to log file. Verify that the log file directory is writable and that the user ID has appropriate permissions.
1503 | E | X | D | Unable to execute user notification. Return code from OS Command (<error code>) | Verify that the notification command can be executed. Refer to the User Guide.
1504 | E | L/N3 | D | Unable to allocate dynamic memory. | Check system resources.
1505 | E | L/N3 | D | System call failure (<system call>): (<OS specific error>). | Contact technical support.
1506 | E | L/N3 | S | The process configuration path length exceeds the maximum allowed. | Reinstall to allocation with a shorter install path length. See your OS documentation for path length limits.
1507 | E | L/N3 | S | Unable to create a data directory (<directory name>): (<OS specific error msg>). | See OS error message and correct as appropriate.
1508 | E | X | S | Unable to initialize the Exec sub-system. | Contact technical support.
1509 | E | X | S | The CONNX registry cannot be read or does not contain a value for: (CONNX.REPLICATION.INSTALLPATH). | Windows: Verify that the INSTALLPATH value is correct in the CONNX Configuration Manager (CONNX\Replication). Unix/Linux: Use the SqlRegistry tool to verify the INSTALLPATH value is correct.
1510 | E | L/N3 | S | Adabas Event Replicator for LUW message API version mismatch. | Verify that all Adabas Event Replicator for LUW components are upgraded to a compatible version.
1511 | E | L/N3 | D | Unable to resolve host (<host>). | DNS name did not resolve. Specify dot notation addresses.
1512 | E | L | N | Bad multi-packet message. Fragment sequence out of order. | Message queue internal error. Contact technical support.
1800 | E | X | U | The process configuration path is either blank or the length exceeds the maximum allowed. | Reinstall to allocation with a shorter install path length. See your OS documentation for path length limits.
1801 | E | X | U | The process name is either blank or the length exceeds the maximum allowed. | Internal error. Contact technical support.
1802 | E | X | U | The specified configuration directory does not exist. | Windows: Verify that the INSTALLPATH value is correct in the CONNX Configuration Manager (CONNX\Replication). Unix/Linux: Use the SqlRegistry tool to verify that the INSTALLPATH value is correct.
1803 | E | X | U | Unable to create a log file directory. | Verify that the installation directory is writable and user ID has appropriate permissions.
1804 | E | X | U | Unable to initialize process log (<logfile>) | Verify that the installation directory is writable and user ID has appropriate permissions.
1805 | E | X | U | Unable to install signal handler: (<OS-specific error message>). | See OS error message and correct as appropriate.
1806 | E | X | U | Application is attempting to switch identity: (<Engine ID>)-->(<Engine ID>). | Error notification is enabled and the notification command is either blank or the length exceeds the maximum allowed.
1807 | E | X | U | The process version is either blank or the length exceeds the maximum allowed. | Contact technical support.

Admin
WARNINGS

Message ID | Explanation | Resolution
2001 | W | L | N | Deployment message is queued. | Deployment message was sent to the controller's message queue. No action required.
2002 | W | L | N | Preparing to queue Deployment message. | No action required.
2003 | W | L | N | Deployment CDD initialized. | No action required.

ERRORS

Message ID | Explanation | Resolution
2501 | E | L | N | Invalid configuration path. | Path does not exist. Windows: Verify that the INSTALLPATH value is correct in the CONNX Configuration Manager (CONNX\Replication). Unix/Linux: Use the SqlRegistry tool to verify the INSTALLPATH value is correct.
2502 | E | L | N | Unable to open master configuration file: API Error (<OS-specific error>). | Verify installation directory is writable to the Admin process.
2503 | E | L | N | Unable to initialize replications. | Contact technical support.
2504 | E | L | N | Unsupported source database type. | An internal error has occurred in the deployed CDD. Contact technical support.
2505 | E | L | N | Replication configuration contains no active replications. | Deploy replications.
2506 | E | L | N | System call failure (<system call>): (<OS specific error>). | See OS error message and correct as appropriate.
2507 | E | L | N | Unable to open master configuration file: IO Error (<OS specific error>). | Ensure that the install directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
2508 | E | L | N | Unable to connect to Adabas Event Replicator for LUW queue service on (<queue server host>):(<server port>): (<queue sub-system error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
2509 | E | L | N | Unable to open InstantdsbSync work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
2510 | E | L | N | Unable to enqueue work message: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
2511 | E | L | N | Unable to retrieve Support DLL instance. | Contact technical support.
2512 | E | L | N | Unable to initialize Support DLL. | Contact technical support.
2513 | E | L | N | Unable to find CDD Object (<CDD object>). | Contact technical support.
2514 | E | L | N | Unable to update CDD Object (<CDD object>). | Contact technical support.
2515 | E | L | N | Unable to find Replication server information. | Contact technical support.
2516 | E | L | N | Unable to open Replication Work Queue (<queue subsystem error>). Queue does not exist. | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
2517 | E | L | N | Unable to initialize Replication Server Map. | Contact technical support.
2518 | E | L | N | Bad Reply from Status Message. | Contact technical support.
2519 | E | L | N | Replication Server Map not found. | CDD not deployed properly. Re-deploy CDD.
2520 | E | L | N | Failed to retrieve Server Status. | Refresh Server Status. If the problem persists, contact technical support.
2521 | E | L | N | Failed to write Server Status. | Ensure that install directory is writable to the current process.
2522 | E | L | N | Invalid Server Status path: (<server status database path>). | Ensure that INSTALLPATH is set correctly.
2523 | E | L | N | Invalid replication server ID: (<replication server ID>). | Contact technical support.
2524 | E | L | N | Invalid replication server name: (<replication server name>). | Validate the server name on the Configure Servers dialog in the Replication Administrator. If the server name is correct, ensure that the server is connected to the network and is operating correctly.
2525 | E | L | N | Invalid server state request: (<server state>). | Contact technical support.
2526 | E | L | N | Unable to delete status queue (<queue name>): (<queue subsystem error>). | Non-fatal error; if problem persists, start and stop the CONNX message queue service (Windows) or Daemon (Unix/Linux).
2527 | E | L | N | Invalid target table ID: (<table ID>). | Contact technical support.
2528 | E | L | N | Configuration API error: (<API error>). | Contact technical support.
2529 | E | L | N | Failed to purge existing Server Status. | Ensure that the install directory is writable to the Replication Administrator and retry Server Status. If problem persists, contact technical support.
2530 | E | L | N | Failed to dequeue Server Status: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
2531 | E | L | N | Incompatible API version in ADM message reply. | One or more components are at a different version level than the Administrator. Ensure that all components of the Replication Server have the same build number and version.
2532 | E | L | N | Unable to allocate dynamic memory. | Check system resources for available memory.
2533 | E | L | N | Unable to initialize status queue. Unable to report status. | Ensure that the CONNX message queue service is running.
2534 | E | L | N | Unable to gain exclusive access to deployment CDD. | Ensure that the CDD is not open by another Event Replication Administrator or the CONNX Data Dictionary Manager.
2535 | E | L | N | Unable to purge the Controller work queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.

Controller
WARNINGS

Message ID | Explanation | Resolution
3001 | W | L | N | De-initializing driver support failed. | Non-fatal warning. No action necessary.
3002 | W | L | N | Recovering from an unclean shutdown. | Previous shutdown was not executed via normal process mechanism. No action necessary.
3003 | W | L | N | Engine unreachable: PID:(<process ID>). Attempting to re-spawn: (<engine ID>). | Controller lost TCP/IP connection to Replication Engine and is attempting to restart Engine.
3004 | W | L | S | Stop service request received. | No action necessary.
3005 | W | L | N | Monitor accept for unknown engine: (<engine ID>). | No action necessary.
3006 | W | L | N | Master configuration contains invalid engine count. Defaulting to 1. | No action necessary.
3007 | W | L | N | Engine spawned: PID:(<process ID>). ID:(<engine ID>). | Engine has been started successfully. No action necessary.
3008 | W | L | N | Engine initialization complete: PID:(<process ID>) ID:(<engine ID>). | No action necessary.
3009 | W | L | N | Event producer initialization complete. ID:(<engine ID>). | No action necessary.
3010 | W | L | N | Deploy succeeded. | No action necessary.
3011 | W | L | N | Deploy failed. | Check the Controller log file for the preceding messages containing additional error information and take action based on those messages.

ERRORS

Message ID | Explanation | Resolution
4001 | E | L/N1 | N | Unable to connect to local queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4002 | E | L/N1 | N | Unable to open controller work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4003 | E | L/N2 | N | Unable to dequeue work message: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4004 | E | L/N3 | N | Unable to open master configuration file: IO Error: (<OS specific error>). | See OS error message and correct as appropriate.
4005 | E | L/N1 | N | Unable to open EP Identity queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4006 | E | L/N3 | N | Unable to spawn engine: (<OS specific error>). | See OS error message and correct as appropriate.
4007 | E | L/N1 | N | Unable to connect to EP queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4008 | E | L/N1 | N | Unable to open EP work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4009 | E | L/N1 | N | Unable to open EP target queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4010 | E | L/N2 | N | Unable to enqueue EP work message: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4011 | E | L/N2 | N | Unable to enqueue Engine work message: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4012 | E | L/N3 | N | Unable to open master configuration file: (<OS specific error>). | See OS error message and correct as appropriate.
4013 | E | L/N3 | N | Unable to initialize replications: (<API error message>). | Contact technical support.
4014 | E | L/N3 | N | Unsupported backend for replication source. | Configuration files may have been modified outside Event Replication. Re-deploy replications.
4015 | E | L/N1 | N | Invalid target table id for replication | Configuration files may have been modified outside Event Replication. Re-deploy replications.
4016 | E | L/N1 | N | Replication configuration contains no active replications. | Configuration files may have been modified outside Event Replication. Re-deploy replications.
4017 | E | L/N3 | N | Unable to write master configuration file: IO Error: (<OS specific error>). | Verify install directory is writable and user ID has appropriate permissions.
4018 | E | L/N3 | S | Unable to open replication license file: (<API error message>). | Ensure that a valid Event Replication license is installed and registered.
4019 | E | L/N3 | S | Unable to lock replication license file: (<API error message>). | User license count has been exceeded. Ensure that a valid Event Replication license is installed and registered.
4020 | E | L/N3 | S | Driver support initialization failed: (<API error message>). | Windows: DLL was not registered. Ensure that the system was rebooted after installation. Unix/Linux: Shared library could not be located or loaded. Check dependencies.
4021 | E | L | N | Unable to delete failed configuration: (<config file name>): (<OS specific error>). | Ensure that the install directory is writable to the Controller user/process. See OS error message and correct as appropriate.
4022 | E | L | N | Bad work message. Unexpected message fragment type: (<embedded message type>). | Contact technical support.
4023 | E | L | N | Unable to flush configuration to disk: (<OS specific error>). | See OS error message and correct as appropriate.
4024 | E | L | N | Unable to open existing config (<config file name>): (<OS specific error>) Starting over. | See OS error message and correct as appropriate.
4025 | E | L | N | Unable to map existing config (<config file name>): (<OS specific error>). Starting over. | See OS error m
4026 | E | L | N | Configuration mapped to NULL. Starting over. | Out of resources. Check disk space and available memory.
4027 | E | L | N | Unable to create new configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory.
4028 | E | L | N | Unable to map new configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory.
4029 | E | L | N | New configuration mapped to NULL. | Out of resources. Check disk space and available memory.
4030 | E | L/N1 | N | Unable to initialize target queues. Exceeded maximum attempts to connect to queue service. | Ensure that the CONNX message queue service is running.
4031 | E | L/N1 | N | Invalid replication server ID. Unable to process configuration. | Configuration files may have been modified outside Event Replication. Re-deploy replications.
4032 | E | L/N1 | N | Cannot retrieve object from master configuration: (<configuration object>). | Contact technical support.
4033 | E | L/N1 | N | Invalid source table id for replication: (<table ID>). | Contact technical support.
4035 | E | L/N1 | C | Socket error sending status change to producer | This error indicates a problem with the communication between the controller and the producer. Ensure that the source nucleus is running and the nucleus log indicates that replication was successfully initialized. Also ensure that there are no firewalls present between the controller and the producer that would prevent communication. If the producer is running and there are no network issues, contact technical support.
4036 | E | L/N1 | N | Unable to create control reply queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4037 | E | L/N1 | S | Configuration reset. Stopping all servers and shutting down. | Invalid license or all active replications removed from this CDD. Either correct the license file,
4038 | E | L/N3 | S | Unable to accept connections on port (<port number>). | Attempted to accept connections on the first available port. No ports were available. Ensure that there is a range of ports available. If configured to a specific port, ensure that port is available.
4039 | E | L | N | Monitor request timed out. | Attempted to communicate with the Replication Engine but did not receive a timely reply. Check the Event Consumer log files.
4040 | E | L | N | Unable to send engine monitor request: (<socket error>). | TCP/IP error. Check the Event Consumer log files.
4041 | E | L | N | Monitor accept for active or deactivated engine. | Sequence error detected and corrected. No action necessary.
4042 | E | L | N | Monitor unable to retrieve configuration for re-spawned engine. | Controller is in an invalid state. Contact technical support.
4043 | E | L | N | Monitor timed out sending configuration to re-spawned engine. | Communication with engine lost; system will attempt to reconnect. No action necessary.
4044 | E | L | N | Monitor error sending configuration to re-spawned engine: (<socket error>). | TCP/IP error. Check the Event Consumer log files.
4045 | E | L | N | Monitor request reply timed out. | Engine failed to respond in a timely manner. Check the Event Consumer log files.
4046 | E | L | N | Unable to receive engine monitor request reply: (<socket error>). | TCP/IP error. Check the Event Consumer log files.
4047 | E | L/N3 | S | Unable to restart acceptor for connections on port (<port number>). | Controller was configured to accept on a specific port and port is no longer available. Specify an available port. or Controller was configured to accept on a range of ports and no ports in the range were available. Ensure that there are available ports.
4048 | E | L/N3 | S | Monitor accept for an engine with a mis-matched process ID (<engine ID>_<engine ID>): (<current process ID>) != (<incoming process ID>). | Contact technical support.
4049 | E | L | N | Database specific configuration missing table descriptors. | Contact technical support.
4050 | E | L | N | Invalid user/pass length in master configuration. Please re-configure and re-deploy. | Contact technical support.
4051 | E | L/N1 | N | Invalid source database id for replication: (<database ID>). | Contact technical support.
4052 | E | L | N | Connection timed out sending configuration to engine. | Non-fatal error; engine will re-attempt connection. No action necessary.
4053 | E | L | N | Connection error sending configuration to engine: (<socket error>). | TCP/IP error. Check the Event Consumer log files.
4054 | E | L | N | Unknown engine dereferenced: (<engine ID>). | Contact technical support.
4055 | E | L | N | Unable to connect to Admin queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4056 | E | L | N | Unable to open Admin status queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4057 | E | L | N | Unable to enqueue message on Admin status queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
4058 | E | L/N1 | N | Master configuration file does not exist: (<config file name>). Unable to process. | Configuration files may have been deleted outside Event Replication. Redeploy replication CDD.
4059 | E | L/N1 | N | Unable to load replication columns from master configuration for ID: (<table ID>). Error: (<API error>). | Contact technical support.
4060 | E | L | N | Unable to remove old configuration: (<config file name>) Error: (<OS specific error>). | See OS error message and correct as appropriate.
4061 | E | L | N | Unable to initialize engine: PID: (<process ID>) ID: (<engine ID>). | Contact technical support.
4062 | E | L | N | Unable to initialize event producer. | Contact technical support.
4063 | E | L | N | Monitor accept for disabled engine. | Sequence error detected and corrected. No action necessary.
4064 | E | L/N3 | N | Engine request for respawn denied. Engine disabled: PID: (<process ID>) ID: (<engine ID>). Please contact technical support. | Contact technical support.
4065 | E | L | N | Version mismatch for engine: ID: (<engine ID>). | One or more components are at a different version level than the Controller. Ensure that all components of the Replication Server have the same build number and version.
4066 | E | L | N | Engine configuration status check send timed out. ID: (<engine ID>). | Ensure that the system has sufficient resources and that the install directory is readable and writable. Check the Engine logs.
4067 | E | L | N | Engine configuration status check send error: ID: (<engine ID> ) Error: (<socket error>). | Ensure that the system has sufficient resources and that the install directory is readable and writable. Check the Engine logs.
4068 | E | L | N | Engine configuration status check reply error: ID:(<engine ID>) Error: (Status not NORMAL) | Check the Engine logs.
4069 | E | L | N | Engine configuration status check reply timed out. ID: (<engine ID>). | Ensure that the system has sufficient resources and that the install directory is readable and writable. Check the Engine logs.
4070 | E | L | N | Engine configuration status check reply error: ID: (<engine ID>) Error: (<socket error>). | Ensure that the system has sufficient resources and that the install directory is readable and writable. Check the Engine logs.
4071 | E | L | N | Unable to create Controller to EP status queue: (<API error>). | Ensure that the system has sufficient resources and that the install directory is readable and writable.
4072 | E | L | N | The Controller to EP status queue has been deleted: (<queue name>). | Contact technical support.
4073 | E | L | N | Unable to open Controller to EP status queue (<queue name>): (<queue API error>). | Ensure that the system has sufficient resources and that the install directory is readable and writable.
4074 | E | L | N | Controller to EP status queue message version mismatch detected. | Ensure that the latest version of Adabas Event Replicator for LUW is installed on all machines.
4075 | E | L | N | Unknown message type encountered on Controller to EP status queue: (<internal message type>). | Contact technical support.
4076 | E | L | N | The EP has reported a failed deploy. | Consult the appropriate EP log and correct environment. Re-deploy.
4077 | E | L | N | Unknown EP encountered in post-deploy enquiry: (<EP id>). | Contact technical support.
4078 | E | L | N | Error in message dequeue on Controller to EP status queue (<queue name>): (<queue API error>). | Ensure that the CONNX message queue is active on all machines involved in replication, the queue directory is readable and writable, and that the system has sufficient resources.
4079 | E | L | N | Duplicate source column detected: TBL: (<table name>) COL: (<column name>). | Contact technical support.
4080 | E | L | N | Unable to resolve target table column: TBL: (<table name>) COL: (<column name>). | Contact technical support.
4081 | E | L | N | Non-unique table column ordinal detected: (<table name>). | Contact technical support.
4082 | E | L | N | Fatal error. Unable to configure producer identities. | Contact technical support.
4083 | E | L | N | Post-deploy EP status check exceeded maximum time limit. | Ensure that the Adabas nucleus has been started and has been correctly configured for replication.
4084 | E | L | N | Source table has no index defined: (<table name>). | Replications must be configured with at least one primary index.
4085 | E | L | N | Target table has no index defined: (<table name>). | Replications must be configured with at least one primary index.
4086 | E | L/N1 | N | Unable to open license for database involved in replication (<DB name>): (<API error message>) | Each database involved in replication must have a corresponding license file. Ensure that your license server is properly configured and running.
4087 | E | L/N1 | N | Unable to lock license for database involved in replication (<DB name>): (<API error message>) | Each database involved in replication must have a corresponding license file. Ensure that your license server is properly configured and running.
4200 | E | L | N | Unrecognized ADABAS table name format: (<Adabas table name>). Table: (<table name>). | Contact technical support.
4201 | E | L | N | Invalid column name exceeds maximum length. Column: (<column name>). Table: (<table name>). | Contact technical support.
4202 | E | L | N | Invalid virtual column type in configuration. Column: (<column name>). Table: (<table name>). | Contact technical support.
4203 | E | L | N | Invalid index column type in configuration. Column: (<column name>). Table: (<table name>). | Contact technical support.
4204 | E | L | N | Duplicate table encountered in ADABAS cluster definition: Table: (<table name>): ({int}). | Contact technical support.
4205 | E | L | N | Non-MU/PE column encountered in rotated table descriptors (<column name>): (<table name>). | Contact technical support.
4206 | E | L | N | MU/PE column encountered in table index descriptors (<column name>): (<table name>). | Contact technical support.
4207 | E | L | N | Unrecognized physical DB Name format for ADABAS: (<internal DB name>). | Contact technical support.
4208 | E | L | N | Unable to create queue name. Max queue name exceeded (<max value>): (<supplied value>). | Contact technical support.
4209 | E | L | N | No ADABAS cluster definitions match the requested source information. | Contact technical support.
4303 | E | L/N1 | N | Unable to perform Adabas to Adabas Initial State | The Adabas to Adabas initial state process uses the Adabas utility ADABCK to do a DUMP of the source files and an OVERLAY on the target. Error 4303 indicates that there was an error in either the source or target ADABCK process. Please check the ADABCK log files for information about the error. These log files are located in the replicator's log directory (connx32\replication\log on Windows and connx/replicator/log on Unix/Linux) in a subdirectory named DBxxx where xxx is the 3 digit number of the database ID. Please check the logs for both the source and target. Note, if an error on the source prevented any processing, there my not be an ADABCK log on the target.

Event Consumer
WARNING

Message ID | Explanation | Resolution
5001 | W | L | C | Loading new EC configuration. | Informational.
5002 | W | L | D | Request to DISABLE PROCESS received. | Informational. A Stop Target was issued from the Administrator.
5003 | W | L | N | Request to initial state source. | Informational.
5004 | W | L | U | EC Configuration locked by another process: (<Configuration Path>). Exiting. | Duplicate engine respawned due to temporary communication failure. No action required.
5005 | W | L | N | Configuration is dirty: recovering from bad shutdown. | Informational
5005 | W | L | N | Configuration is dirty: recovering from bad shutdown. | Informational
5006 | W | L | N | Engine active: Source: (<DB name>):(<internal DB ID>) --> Target: (<DB name>):(<internal DB ID>). | Informational
5201, 5202 | W | L | N | Record information pertaining to a 5203 informational message | Informational
5203 | W | L | N | Engine encountered an SQL error. The operation will be retried. The SQL error can be found in the body of the error message. This message is issued for SQL errors that are transient. They normally succeed on a retry. If they do not succeed after 3 retries, error 5702 will be issued. | Informational
5301 | W | L | S | Shut down occurring before enqueue of Initial State end card. Initial state will be replayed. | Informational.
5302 | W | L | S | Shut down occurring before dequeue of Initial State. Initial State will be replayed. | Informational.
5303 | W | L | S | Shut down occurring before dequeue of transaction. | Informational.

ERRORS

Message ID | Explanation | Resolution
5501 | E | L/N2 | N | Unable to connect to EP queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5502 | E | L/N2 | N | Unable to open cursor for EP transaction queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5503 | E | L/N2 | N | Unable to get message from EP transaction queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5504 | E | L/N1 | N | Unable to dequeue message from EC work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information...
5505 | E | L/N1 | N | Unable to connect to local queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5506 | E | L/N1 | N | Unable to open EC work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5507 | E | L/N3 | N | Unable to create new replication. | Check system resources for available memory.
5508 | E | X | U | Unable to initialize the process name. | Non-fatal error. No action necessary.
5509 | E | L | N | Unable to open connection to status queue service on (<queue service host>): (<port>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5510 | E | L | N | Unable to open status queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5511 | E | L/N3 | D | Unable to set the process name. Unable to initialize logfile. Deploy failed. | Contact technical support.
5512 | E | L/N3 | D | Null record loader returned. Unable to continue processing. | Check system resources for available memory.
5513 | E | L/N3 | D | Duplicate initial state end received. | Contact technical support.
5514 | E | L/N3 | D | Unexpected message in queue. | Contact technical support.
5515 | E | L | N | Unable to open existing config (<config file name>): (<OS specific error>). Starting over. | Non-fatal error. System will recover automatically.
5516 | E | L | N | Unable to map existing config (<config file name>): (<OS specific error>). Starting over. | Non-fatal error. System will recover automatically.
5517 | E | L | N | Configuration mapped to NULL. Starting over. | Out of resources. Check disk space and available memory.
5518 | E | L | N | Configuration file does not belong to this engine: Expected: (<engine ID>) Mapped: (<engine ID>). Starting over. | Non-fatal error. System will recover automatically.
5519 | E | L/N3 | S | Unable to create new configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory. See OS error message and correct as appropriate.
5520 | E | L/N3 | S | Unable to map new configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory. See OS error message and correct as appropriate.
5521 | E | L/N3 | S | New configuration mapped to NULL. | Out of resources. Check disk space and available memory.
5522 | E | L | N | Configuration is dirty: recovering from bad shutdown. | Non-fatal error. No action necessary.
5523 | E | L/N3 | S | Unable to flush configuration to disk: (<OS specific error>). | See OS error message and correct as appropriate.
5524 | E | L/N3 | S | Unexpected message state initializing queue. | Contact technical support.
5525 | E | L/N3 | S | Duplicate initial state found while initializing queue. | Contact technical support.
5526 | E | L | N | Unable to enqueue status message on queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5527 | E | L | N | Unable to set SQL statement for replicating: Length is zero. | Contact technical support.
5528 | E | L | N | Unable to enqueue init marker: (<queue interface error>). | Ensure that the CONNX message queue service is running.
5531 | E | L/N3 | D | Unable to restart engine. Queue initialization failure. | Contact technical support.
5532 | E | L/N3 | S | Control host address has an invalid length: (<host address>). | Contact technical support.
5533 | E | L/N3 | S | Unable to connect to Controller service: (<socket error>). | Check controller log.
5534 | E | L | S | Timeout waiting for initial configuration. Exiting. | System unable to process all replications. Check for resource availability.
5535 | E | L | S | Connection to Controller service lost: (<socket error>). Exiting. | Check controller log.
5536 | E | L/N3 | D | Corrupt queue. Partial message detected. | Contact technical support.
5537 | E | L/N3 | D | Corrupt queue. Message sequence out of order. | Contact technical support.
5538 | E | L/N3 | D | Corrupt queue. Message sequence out of order. | Contact technical support.
5539 | E | L/N3 | D | Corrupt queue. Message sequence out of order. | Contact technical support.
5540 | E | L/N3 | D | Corrupt queue. Message sequence out of order. | Contact technical support.
5541 | E | L/N3 | D | Corrupt queue. Message sequence out of order. | Contact technical support.
5700 | E | L/N2 | D | Unable to connect to Target DB: (<SQL error>). | Check API error and correct problem. When problem has been corrected, restart servers from the Status Tab in the Replication Administrator.
5701 | E | L/N2 | D | End Transaction error: (<SQL error>). | Check SQL error and correct problem. When problem has been corrected, restart servers from the Status Tab in the Replication Administrator.
5702 | E | L/N2 | N | SQL error (<SQL error type>): (<SQL error>). Final try, giving up. Process will disable. | Target table may have been modified externally. Check SQL error and correct problem. When problem has been corrected, restart servers from the Status Tab in the Replication Administrator. An initial state may be required.
5703 | E | L/N2 | N | SQL action affected 0 records: (<SQL error>). | Target table may have been modified externally. An initial state may be required.
5704 | E | L | N | Unable to set connection information: Logical DB name length exceeds maximum: (<logical DB name>). | Contact technical support.
5705 | E | L | N | Unable to set connection information: Connection string length exceeds maximum: (<connection string>). | Contact technical support.
5706 | E | L/N3 | D | Unable to set connection attributes: (<SQL error>). | Contact technical support.
5707 | E | L/N2 | D | Current transaction rolled back. | Application state is disabled. Check Event Consumer logs, fix problems and re-deploy.
5708 | E | L/N2 | D | Begin transaction failed: (<SQL error>). | Application state is disabled. Check Event Consumer logs, fix problems and re-deploy.
5709 | E | L/N2 | D | Invalid transaction. NULL source map. | Contact technical support.
5710 | E | L | N | SQL error: (<SQL error>). | Transaction event has failed. Event Consumer will re-connect and retry the transaction.
5711 | E | L | N | Current transaction rolled back. | No action required.
5712 | E | L/N2 | D | Application has entered an exception state. Current transaction rolled back | No action required.
5713 | E | L/N3 | D | An error occurred during initial state processing. | Compound error state within the engine is preventing clean error handling. Prior error messages contain additional information. Contact technical support.
5800 | E | L/N2 | N | Unable to connect to EP queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5801 | E | L/N2 | N | Unable to open EP transaction queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5802 | E | L/N2 | N | Unable to enqueue message on EP transaction queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5803 | E | L/N2 | N | Unable to dequeue message from EP transaction queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
5804 | E | L/N2 | S | Error in COMMIT. Transaction not committable due to application exception state. | Compound error state within the engine is preventing clean error handling. Prior error messages contain additional information. Contact technical support.
5805 | E | L/N2 | S | Unexpected end of queue. Transaction manager out of sync with event consumer. QUEUE:(<queue name>). | Contact technical support.

Event Producer
WARNINGS

Message ID | Explanation | Resolution
6001 | W | L | U | No existing configuration found. Creating new configuration. | Informational.
6002 | W | L | U | Event producer: Identity configured. | Informational.
6003 | W | L | N | The transaction cache is not empty at shutdown. | Informational.
6004 | W | L | N | The transaction queue is not empty at shutdown. | Informational.
6005 | W | L | N | Processing empty transaction. | Informational.
6006 | W | L | D | Resetting the Event Producer. Deleting current configuration. | Informational. Response to a request to remove all replications.
6007 | W | L | U | Recovering from dirty shutdown. | Informational.
6008 | W | L | C | Processing existing configuration. | Informational.
6009 | W | L | N | Existing configuration loaded. | Informational.
6010 | W | L | C | Processing new configuration. | Informational.
6011 | W | L | N | Dynamic configuration loaded. | Informational.
6012 | W | L | N | Process configuration unloaded successfully | Informational.
6200 | W | L | N | Spawned ep_config: PORT:(<port number>). | Informational.
6250 | W | L | S | Listener exiting main control loop. | Informational.

ERRORS

Message ID | Explanation | Resolution
7001 | E | L/N2 | N | Unable to connect to local queue service: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7002 | E | L/N2 | N | Unable to open target queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7003 | E | L/N2 | N | Unable to enqueue on target queue (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7004 | E | L/N2 | N | Unable to open EP work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7005 | E | L | N | Unable to delete unused record caches: DIR:(<queue directory) ERR:(<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7006 | E | L/N2 | N | Unable to dequeue EP work queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7007 | E | L | S | Queue unreachable and shutdown called during transaction queue processing: TXID:(<internal transaction ID>). | Ensure that the CONNX message queue is the last process to stop when stopping all Adabas Event Replicator for LUW services.
7008 | E | L | S | Queue unreachable and shutdown called during initial state queue processing: TXID: (<queue subsystem error>). | Ensure that the CONNX message queue is the last process to stop when stopping all Adabas Event Replicator for LUW services.
7009 | E | L | N | Unable to purge target queue (<queue name>): (<queue subsystem error>). | Ensure that the CONNX message queue is the last process to stop when stopping all Adabas Event Replicator for LUW services.
7010 | E | L/N2 | N | EP configuration error: duplicate source. | Contact technical support.
7011 | E | L/N2 | N | Unable to open EP control queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7012 | E | L/N2 | N | Unable to peek EP control queue: (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7013 | E | L | U | Unable to open configuration cache for EP (<config file name>): IO Error: (<OS specific error>). | Verify installation directory is readable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7014 | E | L | U | Unable to read cached configuration for EP (<config file name>): IO Error: (<OS specific error>) | Verify installation directory is readable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7015 | E | L | U | Unable to create configuration cache for EP (<config file name>): IO Error: (<OS specific error>) | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7016 | E | L | U | Unable to cache configuration for EP (<config file name>): IO Error: (<OS specific error>). | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7017 | E | L/N1 | U | Unable to open existing configuration (<config file name>): (<OS specific error>). Initial state required. | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7018 | E | L/N1 | U | Unable to map existing configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory.
7019 | E | L/N1 | U | Pointer to existing configuration is NULL: (<OS specific error>). | Out of resources. Check disk space and available memory.
7020 | E | L/N3 | U | Unable to initialize mapped allocator: (<API error>). | Contact technical support.
7021 | E | L/N3 | U | Unable to initialize transaction data. | Contact technical support.
7022 | E | L/N3 | U | Unable to initialize record data. | Contact technical support.
7023 | E | X | S | The CONNX registry cannot be read or does not contain a value for: (CONNX.REPLICATION.INSTALLPATH). | Adabas nucleus was terminated unexpectedly. Initial state required to regain data integrity.
7024 | E | L | U | Unable to delete dirty configuration (<config file name>): (<OS specific error>). | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7025 | E | L/N3 | D | Unable to create new configuration (<config file name>): (<OS specific error>). | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7026 | E | L/N3 | D | Unable to map new configuration (<config file name>): (<OS specific error>). | Out of resources. Check disk space and available memory.
7027 | E | L/N3 | D | Pointer to new configuration is NULL: (<OS specific error>). | Out of resources. Check disk space and available memory.
7028 | E | L/N3 | D | Unable to construct new mapped allocator: (<API error>). | Contact technical support.
7029 | E | L/N3 | D | Unable to construct new transaction data. | Contact technical support.
7030 | E | L/N3 | D | Unable to construct new record data. | Contact technical support.
7031 | E | L/N3 | D | Unable to flush the configuration to disk: (<OS specific error>). | Verify installation directory is writable and user ID has appropriate permissions. See OS error message and correct as appropriate.
7032 | E | L | N | Unable to connect to status queue. | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7033 | E | L | N | Unable to open status queue. | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7034 | E | L | N | Unable to enqueue status message. | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7035 | E | L | N | Unable to delete cache map (<queue name>): (<queue subsystem error>). | Ensure that the message queue has been started and initialized correctly, the port number in the Replication Administrator matches the port number in the Registry, and the message queue directory is writable to the current process. See the User Guide for more information.
7036 | E | LN/3 | U | Unable to load cached configuration. Deployment required. | Ensure that the install directory is writable to the Event Producer user/process and re-deploy.
7037 | E | L | S | Unable to reset the Event Producer. Forcing internal replication processes to shutdown. | Contact technical support.
7038 | E | L/N3 | D | Duplicate transaction requested. | Contact technical support.
7039 | E | L/N3 | D | Unable to retrieve pointer to mapped memory: (<API error>). | Contact technical support.
7040 | E | L/N3 | D | Unable to free pointer to mapped memory: (<API error>). | Contact technical support.
7041 | E | L/N3 | D | Unable to cache record. Invalid transaction ID. | Contact technical support.
7042 | E | L/N1 | D | Unable to retrieve transaction data alloc info. | Contact technical support.
7043 | E | L/N1 | D | Unable to retrieve record data alloc info. | Contact technical support.
7044 | E | L | N | Initial state request received when no configuration exists. | Non-fatal error. No action necessary.
7045 | E | L | N | Delete config request received when no configuration exists. | Non-fatal error. No action necessary.
7046 | E | L/N2 | N | EP configuration error: Duplicate source. | Contact technical support.
7047 | E | L/N3 | S | Unable to initialize the Event Producer. Forcing internal replication processes to shutdown. | Contact technical support.
7048 | E | LN/3 | D | Unable to cache configuration. | Ensure that the install directory is writable to the Event Producer user/process and then re-deploy.
7049 | E | LN/3 | S | Number of cached transactions is non-zero and the configuration is new. | Contact technical support.
7050 | E | LN/3 | S | Number of cached transactions does not match the saved configuration. | Contact technical support.
7051 | E | LN/3 | S | Number of cached transactions does not match the number of restored transactions. | Contact technical support.
7052 | E | LN/3 | S | Unable to reconstitute record data: (<API error>) | Contact technical support.
7053 | E | LN/3 | S | Number of cached transactions is zero and the number of cached records is non-zero. | Contact technical support.
7071 | E | LN/3 | N | Adabas to Adabas Deploy Failed. | Check previous error messages in the EP log. Check Nucleus log.
7072 | E | LN/3 | N | Call to Adabas nucleus to change replication status failed. | Check previous messages in the EP log for more detail. Check Nucleus log. Possible causes of this error are adding a file to the replication list that has a referential integrity dependency on another file that was not added or attempting to do an initial state on a file that has a referential integrity dependency on another file that was not part of the initial state process - most likely because it was not added to the replication list.
7200 | E | L/N3 | D | Internal API call failed. Nucleus Response: (<nucleus response code>). | Contact technical support.
7201 | E | L/N3 | D | Unable to retrieve Primary Key data. | Contact technical support.
7202 | E | L/N3 | D | Internal call failed. Nucleus Response: (<nucleus response code>). | Contact technical support.
7203 | E | L/N | D | Unable to resolve sub tables: (<API error>). | Contact technical support.
7204 | E | L/N3 |  | Event handler termination called with non-zero reference count. | Adabas has terminated abnormally. Contact technical support.
7205 | E | L/N3 |  | FATAL ERROR: Unable to initialize producer. | Contact technical support.
7206 | E | L |  | FATAL ERROR: Unable to initialize producer global status framework. | Contact technical support.
7207 | E | L/N3 |  | FATAL ERROR: Unable to initialize ep_config. | Contact technical support.
7208 | E | L/N3 |  | FATAL ERROR: Unable to create handler. | Contact technical support.
7210 | E | L |  | Unable to send message to ep_config: (<socket error>). | System will try to restart CNXEPCFG automatically. If it doesn't, contact technical support.
7211 | E | L/N3 |  | Unable to send message to ep_config: (<socket error>). | System will try to restart CNXEPCFG automatically. If it doesn't, contact technical support.
7212 | E | L/N3 |  | Failed to retrieve reply message to ep_config: (<socket error>). | System will try to restart CNXEPCFG automatically. If it doesn't, contact technical support.
7213 | E | L/N3 |  | Unable to spawn ep_config: (<OS specific error>). | See OS error message and correct as appropriate.
7215 | E | L/N3 |  | Unable to open connection to ep_config: PORT:(<port number>) ERR:(<socket error>). | Contact technical support.
7250 | E | L |  | Unable to initialize socket acceptor on port (<port number>) (<socket error>). | See OS error message and correct as appropriate.
7251 | E | L |  | Unable to accept incoming socket: (<socket error>). Will attempt to re-initialize acceptor. | Non-fatal error.
7252 | E | L |  | Unable to re-initialize socket acceptor on port (<port number>) (<socket error>). | See OS error message and correct as appropriate.
7254 | E | L |  | Receive failed for incoming request: (<host>)(<port number>): (<socket error>). | Ensure that the Adabas nucleus has been started and has been correctly configured for replication.
7255 | E | L |  | Invalid message type received: (<host>)(<port number>): (<socket error>). | Contact technical support.
7256 | E | L |  | Timeout sending response to client: (<host>)(<port number>). | Ensure that the Adabas nucleus has been started and has been correctly configured for replication.
7257 | E | L |  | Unable to send response to client: (<host>)(<port number>): (<socket error>). | Ensure that the Adabas nucleus has been started and has been correctly configured for replication.

Debug
WARNINGS

Message ID | Explanation | Resolution
99801 | W | L | U | EXEC: { {string} }. | Internal use only. For debug level 2.
99802 | W | L | U | ADM: { {string} }. | Internal use only. For debug level 2.
99803 | W | L | U | CTRL: { {string} }. | Internal use only. For debug level 2.
99804 | W | L | U | EC: { {string} }. | Internal use only. For debug level 2.
99805 | W | L | U | RL: { {string} }. | Internal use only. For debug level 2.
99806 | W | L | U | RL Pool: { {string} }. | Internal use only. For debug level 2.
99807 | W | L | U | TX: { {string} }. | Internal use only. For debug level 2.
99808 | W | L | U | EP: { {string} }. | Internal use only. For debug level 2.
99809 | W | L | U | CTRL (ADABAS): { {string} }. | Internal use only. For debug level 2.
99810 | W | L | U | EP (ADABAS): { {string} }. | Internal use only. For debug level 2.