Verifying IEEE 802.2 DLC Configuration
To verify the IEEE 802.2 DLC Confguration:
1. Use the WRKLIND command to open the Work with Line Description window.
The Display Line Description window appears.
2. Verify the Local Adapter Address of the OS/400 and the Exchange Identifier.
The important parameters are the local adapter address and the exchange identifier.
Make a note of these; they are used in the configuration of three-tier server products such as IBM Communications Server, Microsoft SNA Server, and Novell NetWare for SAA; and in two-tier products such as Attachmate Extra! PC or NetManage RUMBA.