Setting up APPC/LU 6.2 Communications on Target Systems

  Setting up MPTN Configuration
  Verifying MPTN APPC Controller Configuration
  Verifying IEEE 802.2 DLC Configuration
  Verifying IBMRDB Mode Description

Setting up MPTN Configuration
This section assumes that your AS/400 is already configured to support TCP/IP.
1. Enter the Display Network Attributes (DSPNETA) command on the main command line in the AS/400 main menu.
This command displays the network attributes configured for your host system.
2. Page down and verify that the Allow AnyNet Support parameter is set to *YES.