Communications Setup and Scenarios for Novell NetWare for SAA 4.0

  Setting up the Novell NetWare in an IEEE 802.2 DLC scenario
  Configuring the Node in APPN/APPC for Novell NetWare
  Configuring Data Link Adapters
  Defining a Peer Link
  Defining a Partner LU 6.2
  Defining a Transaction Program Name
  Defining a Mode

Setting up the Novell NetWare in an IEEE 802.2 DLC scenario
Note:
To use this link via CONNX for DB2, you must have the NetWare for SAA 4.0 client software installed on the same client machine.
This example is based on a Novell NetWare for SAA 4.0 configuration installed on a Novell NetWare 5.0 server. The following scenario defines an IEEE 802.2 DLC (Data Link Control) connection to an AS/400 V4R2 machine.
1. From a Microsoft Windows client machine on which the Novell NetWare client software is installed, start the NetWare for SAA Server configuration application by selecting NetWare for SAA Management + NWSAA Server Configuration from the Start menu.
2. Log in to the NetWare server.
3. In the Select Configuration File dialog box, select New or Existing Configuration File and click the Next button.
4. In the Select a Configuration Scenario dialog box, select APPN/APPC from the list box.
5. Click the Finish button.