Installing Adabas SQL Gateway Components

  Introduction
  Verifying the Installation and Starting the CONNX Listener
  Enabling RACF Security
  Testing User ID and Password Verification
  Stopping the Batch Job/Started Task TCP/IP Listener
  SAS/C Network Administration
  Determining the TCP/IP Stack

Introduction
Once the ftp successfully completes, you are ready to install the selected CONNX components. To begin this process, log on to TSO on the target system. Given the CONNX Server Data set prefix above = CONNX.Adabas, the ftp process creates a JCL/control record partitioned data set with the name and members listed in the following table:

Member | Purpose
INST | The Adabas SQL Gateway installation job built by the CONNX installation program.
REMOVE | Adabas SQL Gateway uninstallation job + delete steps for sample files.
REMOV01 | Adabas SQL Gateway uninstallation job - delete steps for sample files.
CNXLINKA | JCL procedure to execute the IBM linkage editor against CONNX prelinked SAS/C 7.00 object code and create the Adabas SQL Gateway load modules.
CNXPARMS | Sample control records which define SAS/C environment variables for the Adabas SQL Gateway TCP/IP Listener and Server programs (CNXRUNA and CNXAD'X'0B) where 'X' is the version number (10=A, 11=B, 12=C, 13=D, etc).
CNXADA | JCL procedure to invoke the Adabas SQL Gateway TCP/IP Listener/Server programs to access the Adabas SQL Gateway sample files.
CNXADAJ | Execution JCL for procedure CNXADA.
LNKRUNA | Linkage editor control records for load module CNXRUNA.
LNKADAB | Linkage editor control records for load module CNXAD'X'0B, where 'X' is the version number (10=A, 11=B, 12=C, 13=D, etc).

You can edit the INST member and change the job card to match your site standards. Then, submit this job to the batch execution queue. All job steps must end with condition codes less than or equal to 4.