Starting the CONNX CICS/VSAM TCP/IP Listener
The listener process waits for and verifies connections with client machines. To start the CONNX CICS/VSAM TCP/IP Listener:
1. After logging on to the CICS region, enter nx01 start and press <Enter>.
The CONNX TCP/IP Listener starts.
2. Verify that the CONNX CICS/VSAM TCP/IP Listener transaction NX00 started by typing CEMT INQ TA. Press <Enter>. The screen displays a list of transactions currently running. Verify that Tas(0000 xxx) Tra(NX00) is listed as one of the transactions.