Verifying the Installation of CONNX CICS Components
Option 1 - RDO
If you request to install the CONNX CICS components, the installation job executes the IBM DFHCSDUP utility to define the CONNX programs, transactions, and VSAM configuration and sample files to the target CICS partition RDO VSAM file. You can verify the installation of the CONNX CICS components by logging on to the target CICS partition and issuing the following command:
CEDA EXPAND GR(CNXVVRR)
As needed, you can ask your CICS Administrator to add the CNXLIST list to the target CICS partition startup list. CNXLIST contains the CNXVVRR and SASC700 RDO groups.
Option 2 - Non-RDO
If the target CICS partition does not use RDO, you can define the CONNX CICS files and programs to the target FCT and PPT. The CONNX FCT entries are copied to member CNXFCT0 of the installation JCL partitioned data set; the PPT entries to member CNXPPT0. These entries must be manually copied to the master source for the CICS FCT and PPT and reassembled.