Testing CONNX for VSAM Query/Import Functionality against SCT VSAM Master Files
1. Browse CONNX.STASK.CNTL and find members CNXVSCT, CNXVSCT1, CNXVSCTJ, and CNXVSJ02. Members CNXVSCT and CNXVSCT1 define JCL procedures which invoke the CONNX Started Task TCP/IP Listener/Server programs. Procedure CNXVSCT includes parameters and DDNAMEs for the SCT Master VSAM and CONNX sample VSAM / QSAM / PDS files. Procedure CNXVSCT1 defines parameters and DDNAMES for the SCT Master VSAM files and omits the DDNAMES for the CONNX sample files. The batch job execution JCL for these procedures is in members CNXVSCTJ and CNXVSJ02, respectively. See Verifying the CONNX Started Task Components Installation for the recommended settings for the CONNX sample JCL procedure parameters and environment variables.
2. Change the CONNX environment variables in member CNXPARMS from DEBUG=0 to DEBUG=1 and from CNXNOPREAUTHORIZE=0 to CNXNOPREAUTHORIZE=1.
3. Review the following SCT-specific procedure parameters:

ADSHLQ | SCT Alumni Development System VSAM master file high-level qualifier Default:SCT.ADSBASE
FRSHLQ | SCT Financial Records System VSAM master file high-level qualifier Default: SCT.FRSBASE
HRSHLQ | SCT Human Resources System VSAM master file high-level qualifier Default: SCT.HRSBASE
LMSHLQ | SCT Loan Management System VSAM master file High-Level Qualifier Default: SCT.LMSBASE
SISHLQ | SCT Student Information Systems VSAM master file High-Level Qualifier Default: SCT.SISBASE
ZSSHLQ | SCT Z Support Software VSAM master file High-Level Qualifier Default: SCT.ZSSBASE

Note:
For testing purposes, it is not necessary to define all SCT subsystem VSAM master files in the CNXVSCT/CNSVSCT1 procedure. You can make a backup copy of CNXVSCT or CNXVSCT1 and remove or comment out the SCT symbolic parameters and DDNAMES which are not installed at your site.
4. Edit member CNXVSCTJ or CNXVSJ02, change the job card parameters to match your installation standards, and submit the job to a batch execution queue. The CONNX TCP/IP Listener program (CNXRUNB) starts execution and attempts to listen on the TCP/IP port defined by the CNXRUNPORT environment variable. The CONNX debug tracing messages are written by default to the CNXVSCT job output queue.
5. After these messages are written to the job log, the CNXVSCT job waits for a connect request from an ODBC / JDBC / OLE DB / .NET application. An SDSF display of an idle CNXVSCT batch server job follows: