Verifying Server APPC/LU 6.2 Settings via Control Center
The DB2 UDB 5.x and 6.x products can detect selected SNA vendor stacks, including IBM eNetwork Communications Server, automatically. For other SNA vendors, the configurations can be updated using the vendor configuration utility.
CAUTION:
The detected configuration is for an IBM Communications Server Version 6.0.2 installed on the same Windows Server with DB2 UDB 6.1. The IBM Communications Server is configured to support APPC / LU 6.2 connectivity via Anynet/MPTN (Multi-Protocol Transport Networking). To connect to this DB2 UDB server via the IBM Communications server software, you need to have the IBM Communications Server client installed on your machine, or an SNA vendor client which supports AnyNet/MPTN.
1. Start the DB2 Control Center. Right-click on a DB2 instance and select Setup communications.
If APPC is pre-configured, the APPC check box is selected.
2. Click the Properties button to the right of the APPC check box in the Setup Communications dialog box.
The Configure APPC-DB2 dialog box appears.