Return Codes and Reason Codes of the Roll Server Requests

#### Search Results

Search

# Return Codes and Reason Codes of the Roll Server Requests

This section contains the return codes and reason codes of the roll server requests. Unlike Natural system messages, the explanatory long texts to these messages and codes are only available in this document, not online.

The TP monitor interfaces issuing roll server request interpret some reason codes returned by a failed roll server request and issue specific error messages. Other reason codes, however, are not interpreted. These are reported with a more general error message text.

For information on the Roll Server, see:

- Natural Roll Server Functionality

- Natural Roll Server Operation

In addition, refer to the relevant IBM documents mentioned below.

#### Return Codes:

Decimal | Explanation
--- | ---
`0` | Normal completion.
`4` | Wait for disk I/O completion.
`8` | Wait and resume this call.
`12` | Error, see reason code.
`16` | Abnormal end.
`20` | Recursive abend.
`28` | Roll server not active.
`32` | GETMAIN failed for work area.
`36` | Request block is write protected.
`40` | IXLLIST error.

#### Reason Codes Returned with Return Code 12:

Hex | Dec | Function Type | Explanation | Action
--- | --- | --- | --- | ---
`04` | `04` | `ALLOC` | The roll file is full. | Increase and reformat the roll file. Anmerkung Carefully read the constraints regarding reformatting the roll file described in the roll server documentation.
`08` | `08` | All except `STATS` | An abend was intercepted and a SNAP dump was taken. | Contact Software AG Support.
`0C` | `12` | `ALLOC` | The roll file number returned by the user exit `NATRSU14` is invalid. | Correct the user exit.
`10` | `16` | `FREE` `READ` `WRITE` | The roll file number passed by the requestor in the request block is invalid. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`14` | `20` | `FREE` `READ` `WRITE` | The number of the roll file slot passed by the requestor in the request block is invalid. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`18` | `24` | `FREE` `READ` `WRITE` | There is no allocated roll file slot for the user with the identification passed by the requestor in the request block. Possible reasons: The request block has been overwritten since the last successfully executed roll server function, or the respective roll file slot has been deleted from the roll file either by using the Roll Server’s `TIMEOUT` command, or by using the `SYSTP` utility. | Contact Software AG Support.
`1C` | `28` | `READ` `WRITE` | The size of the compressed Natural thread presented (`WRITE`) or requested (`READ`) is zero. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`20` | `32` | `READ` `WRITE` | The size of the compressed Natural thread is greater than the maximum roll file slot. Possible reasons: `READ`: The request block has been overwritten since the last successfully executed roll server function. `WRITE`: The compressed Natural thread does not fit into its roll file slot, and there is not enough free space in the roll file to allocate the necessary overflow slots. | Increase the roll file.
`24` | `36` | `READ` `WRITE` | An internal control block used for inter-task communication could not be allocated. | Increase the amount of available space for the roll server address space. If the problem persists, contact Software AG Support.
`28` | `40` | `READ` `WRITE` | An intermediate buffer for an asynchronous `READ`/`WRITE` request could not be allocated. | Increase the amount of available space for the roll server address space. If the problem persists, contact Software AG Support.
`2C` | `44` | `READ` | The size of the compressed Natural thread requested is not equal to the size used on the preceding `WRITE` request. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`30` | `48` | `READ` `WRITE` | An abend was intercepted and a SNAP dump issued in the roll server's address space. | Contact Software AG Support.
`34` | `52` | `READ` | The `READ`-task could not allocate the intermediate buffer. | Increase the amount of available space for the roll server address space. If the problem persists, contact Software AG Support.
`38` | `56` | `READ` `WRITE` `STATS` | The address of the Natural thread is not specified in the request block. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`3C` | `60` | `FREE` `READ` `WRITE` | The pointer to the directory entry in the request block is invalid. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`40` | `64` | `READ` | The roll server init timestamp specified in the request block is zero. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`44` | `68` | All | Sysplex Services for Data Sharing (XES) returned an unexpected reason code. The XES reason code is returned by the roll server in the request answer area (label `RSPAXRNC`). | Please refer to the IBM document Sysplex Services Reference for the detailed reason and proposed actions. If the reason does not depend on system definitions, contact Software AG Support.
`48` | `72` | All | The connection to the Coupling Facility was lost. Possible reason: Hardware or system software problem. | Contact the z/OS system administration.
`4C` | `76` | All | The Coupling Facility structure failed. Possible Reasons: Hardware or system software problem (Contact IBM Support) | Stop the roll server, deallocate the coupling facility structure and reformat the roll file.
`51-53` | `81-83` | `READ` | The previous `WRITE` request executed on a different z/OS image was not successfully completed due to a Coupling Facility problem or a roll server problem. | Look at the message logs of the roll servers participating in the Sysplex for messages indicating this situation.
`54` | `84` | `FREE` | The entry for the specific user could not be located in the Coupling Facility structure. Possible reason: The request block has been overwritten since the last successfully executed roll server function. | Contact Software AG Support.
`58` | `88` | `READ` | A wait-queue element could not be allocated. | Increase the amount of available space for the roll server address space. If the problem persists, contact Software AG Support.
`5C` | `92` | `READ` | The information contained in the specific entry of the Coupling Facility structure indicates that there was no previous `WRITE` request. | Contact Software AG Support.
`60` | `96` | `DEALLOC` | The length of the generic user ID is smaller than 1 or greater than 16. | Contact Software AG Support.
`64` | `100` | `DZAP` `READ` `WRITE` | The receiving storage area provided by the caller is write-protected. | Contact Software AG Support.
`68` | `104` | `FREE` `READ` `WRITE` | The ECB referenced in the request block is not aligned or is write-protected. | Contact Software AG Support.
`70` | `112` | All `OC` | A session requested a roll file slot with an invalid user ID. | Contact Software AG Support.
`74` | `116` | `FREE` `WRITE` `READ` | A session presented a Roll Server request with an invalid timestamp. | Contact Software AG Support.
`78` | `120` | `READ` | After a `READ` operation, the roll server indicates that the requestor of the slot is no longer active or another user has already taken the place of the requestor. | Contact Software AG Support.
`7C` | `124` | `READ` | After receiving a return code 8, the Natural CICS Interface resumed the call, but the Roll Server did not deliver the requested roll file slot within 30 seconds. | Contact Software AG Support.
`80` | `128` | All | Try to assign overflow slot. | Contact Software AG Support.
`84` | `132` | All | Invalid stack pointer. | Contact Software AG Support.
`88` | `136` | `ALLOC` | Overflow slot could not be allocated (1). | Similar to 12/4: there is no free slot any more to allocate to an overflow slot in location 1.
`8C` | `8C` | `ALLOC` | Overflow slot could not be allocated (2). | Similar to 12/4: there is no free slot any more to allocate to an overflow slot in location 2.
`CC` | `204` | `WRITE` | This error is reported only when Roll Server is invoked from Natural Under CICS Interface (NCI) NCI retries after a certain wait for disk I/O completion. But the retry failed. | Contact Software AG Support.
`D0` | `208` | `READ` | This error is reported only when Roll Server is invoked from Natural Under CICS Interface (NCI) NCI resumes Roll operation after a certain wait. But the retry failed | Contact Software AG Support.
`104` - `13C` | `260` - `316` | All | Internal error. | Contact Software AG Support.