Installing Natural IMS TM Interface on z/OS

#### Search Results

Search

# Installing Natural IMS TM Interface on z/OS

This document describes the steps for installing the Natural IMS TM Interface (product code NII) on z/OS.

- Prerequisites

- Installation Medium

- Installation Procedure

- Prepare, Convert, Assemble and Link the License File for Natural for IMS for zIIP

- Common Installation Steps

- Installing the Batch Message Processing BMP Environment

- Installing the Message-Oriented NTRD Environment

- Installing the Dialog-Oriented MPP Environment

- Installing the Natural Development/Natural Web I/O Interface Server

- Installing the Server Environment

- Customizing the IMS TM Environment

- Installation Verification

#### Related Topic:

For information on how to operate Natural in an IMS TM environment, see Using Natural with TP Monitors and Natural under IMS TM in the TP Monitor Interfaces documentation.

#### Notation vrs or vr:

When used in this document, the notation `vrs` or `vr` represents the relevant product version (see also Version in the Glossary).

## Prerequisites

The following software must be installed before you can install the Natural IMS TM Interface:

- Natural global buffer pool if you are using the MPP environment (strongly recommended).

- Natural Roll Server if the `ROLLSRV` parameter of the Natural IMS TM Interface is set to `YES`.

- Natural Authorized Services Manager with the SIP server function if the Non-Conversational MPP Interface, the monitoring or the broadcasting function of the Natural IMS TM Interface is used.

- Natural Authorized Services Manager if the Accounting to SMF function of the Natural IMS TM Interface is used.

- Adabas IMS/TM Interface (product code AII), version as specified under Software AG Product Versions Supported by Natural in the current Natural Release Notes for Mainframes.

For further information on the functions mentioned above, see the relevant sections in the TP Monitor Interfaces and Operations documentation.

See also General Prerequisites and System Support in the section Overview of the Installation Process.

## Installation Medium

The installation medium contains the following data sets required for product installation:

Data Set Name | Contents
--- | ---
`NIIvrs.LOAD` | Load modules
`NIIvrs.SRCE` | Source modules and macros

Copy the data sets into your environment as described in Copying Data Sets to a z/OS Disk in the section Installing Natural.

#### Sample Jobs

Sample installation jobs are contained in the `NATvrs.JOBS` data set and are prefixed with the product code. The data set is provided on the installation medium supplied for base Natural.

## Installation Procedure

Be sure to read Installation Process and Major Natural Features before you start the installation procedure.

The installation procedure comprises the following:

- Prepare, Convert, Assemble and Link the License File for Natural for IMS for zIIP

- Common Installation Steps

- Installing the Batch Message Processing BMP Environment

- Installing the Message-Oriented NTRD Environment

- Installing the Dialog-Oriented MPP Environment

- Installing the Natural Development/Natural Web I/O Interface

- Installing the Server Environment

- Customizing the IMS TM Environment

## Prepare, Convert, Assemble and Link the License File for Natural for IMS for zIIP

(Job I007, Steps 2501, 2502, 2504)

Anmerkung
This step is optional. It is only required if you want to install Natural for IMS for zIIP, and if Natural IMS TM Interface Version 8.3.4 is installed in your environment.

You must install a valid Natural license file. An additional license file is required if you want to install Natural for IMS for zIIP to enable support of the IBM z/IIP (IBM System z Integrated Information Processor).

For detailed information on the license file and product licensing, see Software AG Mainframe Product Licensing.

1. Copy the license file from the supplied installation medium to disk or transfer it from the PC as described in Transferring a License File from PC to a z/OS Host Using FTP in Software AG Mainframe Product Licensing.

2. Check, convert, assemble and link the license file supplied for Natural for IMS for zIIP:

   Step 2501 | Check license file `NIIvrs.LICS`. This job runs the CHECK function of the LICUTIL license utility (see below).
   Step 2502 | Convert license file into an assembler source. This job runs the MAKE function of the LICUTIL license utility (see below).
   Step 2504 | Assemble and link the assembler source to generate load module `NIILIC`. This module is then linked to all relevant front-ends in the Jobs I070 and I080.

   The functions and option settings provided by LICUTIL are described in Using the License Utility: LICUTIL in Software AG Mainframe Product Licensing.

## Common Installation Steps

> Note for LE Options:

>   If you want Natural to run in the IBM Language Environment (LE), set the System Maintenance Aid (SMA) parameter `NAT-LE` to `Y` (Yes). The default setting is `N` (No). Additionally, if you want to modify the LE options in the `NATLEOPT` source module or if you use non-Natural programs running in 24-bit mode, set the appropriate SMA parameter as described in Build the Natural-Specific IBM Language Environment Options in Installing Natural.

The following is an overview of the installation jobs/steps required to install the Natural IMS TM Interface in a BMP, an NTRD an MPP and/or a server environment:

### Step: Link the Natural IMS TM Interface Module

(Job I055, Step 2582)

- Link the Natural IMS TM Interface module.

  The same interface module can be used in a BMP, an NTRD, an MPP and/or a server environment.

  The name of the interface module must be specified with the `NIINAME` keyword subparameter of the `NTIMSP` macro contained in the Natural parameter module. For details, see the Parameter Reference documentation.

## Installing the Batch Message Processing BMP Environment

The following is an overview of the installation jobs/steps required to install the Natural IMS TM Interface for the BMP environment:

### Step: Link the BMP Front-End

(Job I070, Step 2510)

The front-end consists of the load module `NIIBMP` contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Build the Natural Parameter Module (see Installing Natural) and additional optional modules (see the list of module names supplied with Step 2510).

- Link the front-end for the BMP environment.

  Wichtig
  The name of the linked BMP front-end must also be specified in your BMP region job as the application program name (parameter `MBR` of the `IMSBATCH` procedure invocation).

You can specify the parameter settings for your BMP environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

## Installing the Message-Oriented NTRD Environment

The following is an overview of the installation jobs/steps required to install the Natural IMS TM Interface for the NTRD environment:

- Step 1: Build the NIIBOOT Bootstrap Module

- Step 2: Link the NTRD Front-End

### Step 1: Build the NIIBOOT Bootstrap Module

(Job I056, Steps 2520, 2521)

This step is only required if you want to invoke the NTRD front-end by a bootstrap module and not directly by a transaction code.

1. Create the `NIIBOOT` source module which contains a call to the `NIMBOOT` macro. For the `DRIVERN` parameter, specify the name of the front-end module to be linked in Step 2.

2. Assemble and link the bootstrap module.

### Step 2: Link the NTRD Front-End

(Job I070, Step 2530)

The front-end consists of the `NIINTRD` load module contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Build the Natural Parameter Module (see Installing Natural) and additional optional modules (see the list of module names supplied with Step 2530).

- Link the front-end for the NTRD environment.

  If you invoke the NTRD front-end by a bootstrap module, you must additionally specify the name of the linked NTRD front-end as the driver name (`DRIVERN` parameter) in the `NIMBOOT` macro. The `NIMBOOT` macro is described in the TP Monitor Interfaces documentation.

  If you invoke the NTRD front-end directly by a transaction code, you must additionally specify the name of the linked NTRD front-end as the application program name (parameter `PSB`) in the `APPLCNT` macro.

You can specify the parameter settings for your NTRD environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

## Installing the Dialog-Oriented MPP Environment

The following is an overview of the installation jobs/steps required to install the Natural IMS TM Interface for the MPP environment:

- Step 1: Allocate and Format the Roll Files

- Step 2: Build the Natural Parameter Module

- Step 3: Link the Conversational MPP Front-End

- Step 4: Link the Non-Conversational MPP Front-End

### Step 1: Allocate and Format the Roll Files

(Job I070, Step 2590)

This step is only required if you do not use the Natural Roll Server.

If you do not want to use the Natural Roll Server, you have to allocate and format the roll files to be used by the Natural IMS TM Interface.

You can allocate up to 5 sequential data sets with a fixed-record format for use as roll files.

1. Allocate the roll files.

2. Format the roll files by using the module `NATRSRFI` described in Formatting the Roll File in the Operations documentation.

The roll file initialization program produces a WTO message indicating the number of concurrent users which can be serviced by the roll file. For information on the roll file facility, see Natural Roll Server Functionality in the Operations documentation.

### Step 2: Build the Natural Parameter Module

(Job I080, Steps 2500, 2510)

1. Set the profile parameters `FNAT` and `FUSER` (see the Parameter Reference documentation) in the Natural parameter module:

       FNAT=(database-id,file-number)
       FUSER=(database-id,file-number)

   where `database-id` and `file-number` are the values you specified when loading the system files during the Installation Procedure for base Natural.

2. If you want to use a Natural global buffer pool, specify the macro `NTBPI` in the Natural parameter module with the name of the global Natural buffer pool and set the profile parameter `SUBSID` in the parameter module.

   If you want to use any other buffer pool, specify the macro `NTBPI` in the parameter module for each required buffer pool type.

   We strongly recommend that you use a global buffer pool for each buffer pool type.

   If an editor buffer pool is required, you must use a global editor buffer pool.

3. Modify any other parameters in the parameter module whose default values do not meet your requirements. For further information on the parameters contained in the parameter module, see Building a Natural Parameter Module in the Operations documentation.

4. Assemble and link the Natural parameter module for the dialog-oriented environments.

### Step 3: Link the Conversational MPP Front-End

(Job I080, Step 2570)

The front-end consists of the `NIICONV` load module contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Step 2: Build the Natural Parameter Module and additional optional modules (see the list of module names supplied with Step 2570).

- Link the front-end for the conversational MPP environment.

  Wichtig
  The name of the linked MPP front-end must also be specified in the `APPLCNT` macro as the application program name (parameter `PSB`).

You can specify the parameter settings for your conversational MPP environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

### Step 4: Link the Non-Conversational MPP Front-End

(Job I080, Step 2572)

The front-end consists of the `NIINONC` load module contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Step 2: Build the Natural Parameter Module and additional optional modules (see the list of module names supplied with Step 2572).

- Link the front-end for the non-conversational MPP environment.

  Wichtig
  The name of the Non-Conversational MPP front-end must also be specified in the `APPLCNT` macro as the application program name (parameter `PSB`).

You can specify the parameter settings for your non-conversational MPP environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

## Installing the Natural Development/Natural Web I/O Interface Server

The following steps are required to implement the Natural Development Server (NDV) and the Natural Web I/O Interface (NWO) server in your IMS TM environment.

Anmerkung
You are recommended to also read the information contained in the sections Installing the Natural Development Server IMS Adapter of the Natural Development Server for z/OS (Batch) documentation and Installing the Natural Web I/O Interface Server IMS Adapter under z/OS in the Natural Web I/O Interface documentation.

### Step: Link the Natural Development/Natural Web I/O Interface Server Front-End

(Job I080, Step 2586)

The front-end consists of the `NIISFE` load module contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Step 2: Build the Natural Parameter Module and additional optional modules (see the list of module names supplied with Step 2586).

- Link the front-end for the Natural Development Server/Natural Web I/O Interface server.

  Wichtig
  The name of the linked Natural Development Server/Natural Web I/O Interface server front-end must also be specified in the `APPLCNT` macro as the application program name (parameter `PSB`).

You can specify the parameter settings for your Natural Development Server/Natural Web I/O Interface server environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

## Installing the Server Environment

The following is an overview of the installation jobs/steps required to install the Natural IMS TM Interface for the sever environment:

- Step 1: Build the NIIBOOTS Bootstrap Module

- Step 2: Link the Server Front-End

### Step 1: Build the NIIBOOTS Bootstrap Module

(Job I056, Steps 2540, 2541)

1. Create the `NIIBOOTS` source module which contains a call to the `NIMBOOT` macro with the `SERVER` parameter set to `YES`. For the `DRIVERN` parameter, specify the name of the front-end module to be linked in Step 2.

2. Assemble and link the bootstrap module.

### Step 2: Link the Server Front-End

(Job I070, Step 2550)

The front-end consists of the `NIISRVD` load module contained in the `NIIvrs.LOAD` data set, the Natural parameter module created in Build the Natural Parameter Module (see Installing Natural) and additional optional modules (see the list of module names supplied with Step 2550).

- Link the front-end for the server environment.

  Wichtig
  The name of the server front-end must also be specified in the `NIMBOOT` macro as the driver name (parameter `DRIVERN`) described in the TP Monitor Interfaces documentation.

You can specify the parameter settings for your server environment by using the parameter macros `NTIMSP` and `NTIMSPE` of the Natural parameter module (see the Parameter Reference documentation).

## Customizing the IMS TM Environment

The following steps require system modifications to your IMS TM environment.

- Step 1: Create the APPLCTN Table Definitions for MPP, BMP, NTRD and SFE

- Step 2: Create the PSB/ACB for both the MPP and BMP

- Step 3: Create the BMP and MPP Regions

- Step 4: Create the PRELOAD List

### Step 1: Create the APPLCTN Table Definitions for MPP, BMP, NTRD and SFE

Create the `APPLCTN` table definitions for MPP, BMP and NTRD according to the following examples:

- Example for MPP:

      APPLCTN PSB=NIIvrsFR,PGMTYPE=TP
            TRANSACT CODE=NATvrs,MODE=SNGL,SPA=512,                          *
                MSGTYPE=(SNLGSEG,RESPONSE,4)

  Wichtig
  The size of the SPA must be set to at least 157 bytes plus the `NRAST` value specified in the `NTIMSPT` macro of the Natural parameter module.

- Example for BMP (message-driven or specific for Natural Advanced Facilities):

      APPLCTN PSB=NIIvrsBM,PGMTYPE=BATCH
            TRANSACT CODE=NATvrsBM,MODE=SNGL,                                *
                MSGTYPE=(SNLGSEG,RESPONSE,4)

  This `APPLCTN` definition is required if you use the `CMGETMSG` feature.

- Example for BMP (without message queue processing):

      APPLCTN PSB=NIIvrsBM,PGMTYPE=BATCH

- Example for NTRD:

      APPLCTN PSP=NIIvrsOB,PGMTYPE=TP
              TRANSACT CODE=NATvrsOB,MODE=SNGL,                              *
                MSGTYPE=(MULTSEG,NONRESPONSE,4)

- Example for SFE:

      APPLCTN PSB=NIIvrsAD,PGMTYPE=TP,SCHDTYP=PARALLEL
            TRANSACT CODE=NATvrsAD,MODE=SNGL,                                *
               MSGTYPE=(SNGLSEG,NONRESPONSE,4)

### Step 2: Create the PSB/ACB for both the MPP and BMP

1. Create the PSB for MPP according to the following example for conversational Natural:

       PCB TYPE=TP,MODIFY=YES
       PCB TYPE=TP,MODIFY=YES
       PCB TYPE=TP,MODIFY=YES
       SENSEG NAME=COURSE
       SENSEG NAME=PREREQ,PARENT=COURSE
       SENSEG NAME=OFFERING,PARENT=COURSE
       SENSEG NAME=TEACHER,PARENT=OFFERING
       SENSEG NAME=STUDENT,PARENT=OFFERING

       PSBGEN PSBNAME=NIIvrsFR,LANG=ASSEM,MAXQ=3,IOASIZE=132

   At least one modifiable TP-PCB must be defined for default use of hardcopy, sending messages and transaction switching. The value of the `WRKPCBS` keyword subparameter (`NTIMSPT` macro in the Natural parameter module) in the current environment table must be less than or equal to the number of PCBs minus 1 to avoid a Natural initialization error.

2. Create the PSB for BMP according to the following example:

       PCB TYPE=TP,MODIFY=YES
       PCB TYPE=TP,MODIFY=YES
       SENSEG NAME=COURSE
       SENSEG NAME=PREREQ,PARENT=COURSE
       SENSEG NAME=OFFERING,PARENT=COURSE
       SENSEG NAME=TEACHER,PARENT=OFFERING
       SENSEG NAME=STUDENT,PARENT=OFFERING

       PSBGEN PSBNAME=NIIvrsBM,LANG=ASSEM,MAXQ=3,IOASIZE=132

   At least one modifiable TP-PCB must be defined for default use of hardcopy and sending messages. The value of the `WRKPCBS` keyword subparameter in the current environment table must be less than or equal to the number of PCBs minus 1 to avoid a Natural initialization error.

3. After creating the required `APPLCTN`s for the BMP and MPP environments, generate the PSB, DBD and ACB.

4. After generating the ACB, activate the new definitions by issuing the following commands :

       /MODIFY PREP ACBLIB
       /MODIFY COMMIT

### Step 3: Create the BMP and MPP Regions

(Job I200, Steps 2500, 2504)

- Create the BMP region (Step 2500) according to the `BMPJOB` sample member.

- Create the MPP region (Step 2504) according to the `MPPJOB` sample member.

### Step 4: Create the PRELOAD List

- Update the `PRELOAD` list by using a `PRELOAD` member `DFSMPL xx` with the names of the following modules:

  the nucleus,
  the interface module,
  the front-end, and
  the Adabas link module.

  #### Example for MPP:

      NATvrsSH,NIIvrsIF,NIIvrsFR,ADALNI

  #### Example for BMP:

      NATvrsSH,NIIvrsIF,NIIvrsBM,ADALNK

- If alias names are used for any members in the `PRELOAD` list, these names should be added to the `PRELOAD` list as well. Failure to do so leads to performance degradation.

#### Special Considerations:

- The region size must be large enough to hold the nucleus, the interface module, the front-end, the Natural thread and about 20 KB of working storage below the line.

- Include the load libraries used by the Natural IMS TM Interface.

- Include the DD statement for the roll file created in Step 1: Allocate and Format the Roll Files:

      //ROLLFn   DD  DSN=....DISP=SHR

  where `n` is a value from 1 - 5.

- Include the DD statement for `NATRJE`:

      //NIIRJEDD   DD  SYSOUT=(X,INTRDR)

- In the JCL of the MPP region, add the `SYSTPCD` DD statement if the Natural Development Server or Natural Web I/O Interface server is used. See IBM's z/OS V1Rx.0 Communications Server IP Configuration Guide, Chapter 1.5.2, Configuring TCPIP.DATA.

## Installation Verification

You can verify the successful installation of the Natural IMS TM Interface by following the instructions in this section.

- Start Batch Natural

- Start and Test Online Natural

### Start Batch Natural

1. From an IMS TM session, start a BMP with the following IMS TM command:

       /STA REG BMPJOB

2. Check the output. The output results from the Natural system command `TECH` described in the System Commands documentation. Verify the output in your environment.

### Start and Test Online Natural

1. From an IMS TM session, issue the following IMS TM commands:

       /STA REG MPPJOB
       /STA TRAN NATvrs
       /STA PROG NIIvrsFR

   The Natural IMS TM Interface is available.

2. From an IMS TM session, type in the following transaction name:

       NATvrs

   A Natural session is started.

3. Proceed with the steps described in the section Test Online Natural.

### On this page

- Prerequisites
- Installation Medium
- Installation Procedure
- Prepare, Convert, Assemble and Link the License File for Natural for IMS for zIIP
- Common Installation Steps
- Installing the Batch Message Processing BMP Environment
- Installing the Message-Oriented NTRD Environment
- Installing the Dialog-Oriented MPP Environment
- Installing the Natural Development/Natural Web I/O Interface Server
- Installing the Server Environment
- Customizing the IMS TM Environment
- Installation Verification