Authorized Services Manager Messages

#### Search Results

Search

# Authorized Services Manager Messages

This section lists the messages that may be issued by the Natural Authorized Services Manager (ASM).

Unlike Natural system messages, the explanatory long texts to these messages and codes are only available in this document, not online.

For information on the Authorized Services Manager, see Authorized Services Manager under z/OS in the Operations documentation.

## ASM0001 - Subsystem id invalid

Explanation | A subsystem ID was specified that is longer than 4 characters.
Action | Specify a subsystem ID of 1 to 4 characters.

## ASM0002 - No group name: Sysplex purge propagation disabled

Explanation | The second parameter was not specified. The ASM will not communicate with other ASMs in a Parallel Sysplex.
Action | None.

## ASM0003 - Unexpected return code from IEANTRT: rc

Explanation | The Name/Token Service returned return code rc.
Action | See the current IBM MVS Programming: Authorized Assembler Services Reference manual for information about the return code from the `IEANTRT` request.

## ASM0004 - LX table could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with reasoncode.
Action | Increase virtual storage available to the ASM. (`REGION` option of the JCL `EXEC` statement.)

## ASM0005 - Authorized Services Manager Version vrs is active

Where vrs represents the relevant product version (see also Version in the Glossary).

Explanation | The ASM initialized successfully and is ready for work.
Action | None.

## ASM0006 - Other than MODIFY or STOP command received

Explanation | The ASM received a `CIBVERB` other than `MODIFY` or `STOP`.
Action | Contact Software AG.

## ASM0007 - Unrecognized parameter in parm file:

Explanation | The parameter file contained an unknown parameter. This message is followed by a message displaying the line from the parameter file.
Action | Correct typing error.

## ASM0008 - Invalid value in parm file:

Explanation | An invalid value was specified in the parameter file. This message is followed by a message displaying the line from the parameter file.
Action | Correct typing error.

## ASM0009 - Invalid command: command

Explanation | An invalid operator command was issued to the ASM.
Action | Check for typing error and correct.

## ASM0010 - Bad return code from SNAP routine: rc

Explanation | A SNAP dump could not be taken. The return codes are as follows:
20 | A `STORAGE OBTAIN` request failed.
24 | `SYSUDUMP` could not be opened.
Action | For return code 20: | Increase virtual storage available to the ASM. (`REGION` option of the JCL `EXEC` statement.)
For return code 24: | Ensure that the ASM job or started task includes a DD statement for `SYSUDUMP`.

## ASM0011 - Subtask terminated: taskname rc

Explanation | The subtask indicated by taskname has terminated. If the subtask has terminated abnormally, a return code (rc) is issued with the message.
Action | Contact Software AG support.

## ASM0012 - Subtask termination in progress

Explanation | In response to the `TERM` operator command, the ASM has started to terminate its subtasks.
Action | None.

## ASM0013 - Coupling Facility will not be used for SIP

Explanation | No CF structure name was specified in the third parameter.
Action | None.

## ASM0014 - Invalid SIP CF structure name

Explanation | A structure name of more than 16 characters was specified.
Action | Specify a structure name of 16 characters or less.

## ASM0015 - Invalid number of SIP slots specified

Explanation | The fourth parameter is not a number.
Action | Correct typing error.

## ASM0017 - Connected to SIP CF Structure with nnnn slots

Explanation | The structure was already allocated and contains nnnn slots.
Action | None.

## ASM0018 - SIP CF Structure initialized with nnnn slots

Explanation | The structure was not yet allocated and initialized by the ASM. The number of slots is either the number specified in the fourth parameter or the number of slots the ASM was able to create, whichever is less.
Action | None.

## ASM0019 - Number of SIP slots not specified: SIP service is not available

Explanation | The number of slots was not specified as fourth parameter, and a CF structure was not specified as third parameter. The Session Information Pool Service (SIP) is not available.
Action | None.

## ASM0020 - Invalid SIP slots size specified

Explanation | The fifth parameter is either not numeric, or an invalid number.
Action | Specify 256, 512, 1024, 2048, or 4096.

## ASM0021 - Unexpected return code from IEANTCR: rc

Explanation | The Name/Token Service returned return code rc.
Action | See the current IBM MVS Programming: Authorized Assembler Services Reference manual for information about the return code from the `IEANTCR` request.

## ASM0022 - Wrong ECSAD version: version

Explanation | NATASMvr is started while there is still an ECSA-Directory present for another version of NATASMvr for this subsystem-ID.
Action | Rename the subsystem-ID, IPL the system, or start NATASMvr with option `ECSADUPD`.

## ASM0023 - Old ECSAD with version version no longer in use

Explanation | NATASMvr is started while there is still an ECSA-Directory present for another version of NATASMvr for this subsystem-ID. The current entry is voided, and a new entry is created.
Action | None. However, it is good practice to remove the `ECSADUPD` parameter when all subsystems are migrated.

## ASM0029 - Module NATZPX loaded at address: address

Explanation | Diagnostic message to report where module NATZPX is copied into memory.
Action | None.

## ASM0030 - Module NATFSSM loaded at address: address

Explanation | Diagnostic message to report where module NATFSSM is copied into memory.
Action | None.

## ASM0031 - Module NATNDVX loaded at address: address

Explanation | Diagnostic message to report where module NATNDVX is copied into memory.
Action | None.

## ASM0033 - No space for a PROPBLOK in Message Exit

Explanation | Diagnostic message for Software AG.
Action | Contact Software AG Support.

## ASM0034 - IXCMSGI return code nnnnn reason code nnnnn

Explanation | Diagnostic message for Software AG.
Action | Contact Software AG Support.

## ASM0035 - IXC Message Exit received invalid length: xxxxxxxx

Explanation | Diagnostic message for Software AG.
Action | Contact Software AG Support.

## ASM0036 - IXC Message Exit received invalid message header

Explanation | Diagnostic message for Software AG.
Action | Contact Software AG Support.

## ASM0039 - Module NATZPX removed at address: address

Explanation | Diagnostic message to report where module NATZPX is unloaded from.
Action | None.

## ASM0040 - Module NATFSSM removed at address: address

Explanation | Diagnostic message to report where module NATFSSM is unloaded from.
Action | None.

## ASM0041 - Module NATNDVX removed at address: address

Explanation | Diagnostic message to report where module NATNDVX is unloaded from.
Action | None.

## ASM0045 - Applied Zaps:

Explanation | When Zaps are applied to the ASM, it issues this message, followed by a list of applied zaps.
Action | None.

## ASM0047 - Operator command: command

Explanation | The ASM echoes operator commands to `JESMSGLG`.
Action | None.

## ASM0048 - IARV64 GETSTOR failed. Return code: rc

Explanation | There is not enough memory available above the bar.
Action | Increase the `MEMLIMIT` parameter on the JCL EXEC statement.

## ASM0049 - Too many/few parameters for command

Explanation | An operator `command` was issued that contained an incorrect number of parameters.
Action | Correct the operator command.

## ASM0052 - Not enough storage for IARV64 GETSTOR - Increase MEMLIMIT

Explanation | There is not enough storage available for IARV64, i.e. above the 2GB bar.
Action | Increase the value of MEMLIMIT.

## ASM0058 - ASM already active in subsid: Job jobname ASID asid

Explanation | The ASM determined that in the Natural subsystem specified in the first parameter, `subsid`, another ASM is already active. The other ASM is running in job or started task named `jobname`, with address space identifier `asid`.
Action | Start only one ASM per Natural subsystem per MVS image.

## ASM0066 - REBUILD Start: CF structure temporarily unavailable

Explanation | Operator command `SETXCF START,REBUILD…`was issued for the Coupling Facility Structure that holds the Session Information Pool (SIP) data. SIP operation is quiesced until the Rebuild operation is complete.
Action | None.

## ASM0067 - REBUILD End: CF structure available again

Explanation | Operator command `SETXCF START,REBUILD…`was issued for the Coupling Facility Structure that holds the Session Information Pool (SIP) data. Rebuild is now complete and the SIP service resumes normal operation.
Action | None.

## ASM0068 - Invalid parameter parameter

Explanation | An invalid parameter was supplied in the JCL `EXEC` statement of the ASM job or Started Task.
Action | Correct JCL.

## ASM0069 - Invalid non-activity time

Explanation | The `NONACTIVITY` parameter (or `TIMEOUT NAT` command) is not numeric or greater than 10000000.
Action | Correct parameter file.

## ASM0070 - Invalid timeout check time

Explanation | The `TIMEOUTCHECK` parameter (or `TIMEOUT TOC` command) is not numeric or not a valid time of day.
Action | Specify a valid time in the format `h`, `hh`, `hhm` or `hhmm`.

## ASM0071 - NATFSSM not linked: FSSM parameter ignored

Explanation | The parameter file contains `FSSM` parameters, but the `NATFSSM` module is not linked to the Authorized Services Manager.
Action | Either link the `NATFSSM` module to the Authorized Services Manager or delete the parameters from the parameter file.

## ASM0072 - Installation error: NATBPPRP not linked

Explanation | Module `NATBPPRP` must be included when the Authorized Services Manager is linked into an APF library.
Action | Relink NATASMvr as described in the Installing Natural on z/OS documentation. Anmerkung The notation vr represents the relevant product version (see also Version in the Glossary).

## ASM0073 - module version date time

Explanation | In response to the `VLIST` command, a list of linked modules is displayed with version and assembly date and time.
Action | None.

## ASM0074 - Thread end requested by userid ASID asid

Explanation | The database administrator, Natural Development Server or Natural Web/IO Interface requested that a session thread be cancelled.
Action | None.

## ASM0075 - TIMEOUT ON/NOW rejected: No valid timeout parameters

Explanation | No valid non-activity time and/or no valid timeout-check-time was specified before this command was issued.
Action | Either specify non-activity time and timeout-check-time as startup parameters, or precede the command with the `TIMEOUT NAT` and `TIMEOUT TOC` commands.

## ASM0076 - Timeout check deactivated

Explanation | Timeout processing was disabled by a `TIMEOUT OFF` command.
Action | None.

## ASM0077 - Specify NAT, NOW, ON, OFF,
ASM0077 - REPEAT, TOC, TERSE, VERBOSE, or ?

Explanation | The `TIMEOUT` command was issued with an invalid parameter. This message consists of two lines.
Action | Refer to the description of the `TIMEOUT` command in the section ASM Operator Commands in the Operations documentation.

## ASM0078 - Timeout processing starting

Explanation | The routine to detect and delete non-active sessions is running.
Action | None.

## ASM0079 - Scheduled/Operator timeout processing deleted n sessions

Explanation | Timeout check has detected and deleted `n` sessions that had been inactive longer than the non-activity time specified as the startup parameter or with the `TIMEOUT NAT` command.
Action | None.

## ASM0080 - Timeout processing ended with return code rc

Explanation | The routine to detect and delete non-active sessions has ended with return code `rc`.
Action | If `rc` is not zero, contact Software AG support.

## ASM0082 - Send command TIMEOUT ON to activate timeout check

Explanation | This message is issued in response to a `TIMEOUT TOC` or `TIMEOUT NAT` command. It indicates that the required parameters for the timeout check are valid.
Action | You may now activate the timeout check with the `TIMEOUT ON` command.

## ASM0083 - Authorized Server not in active state. TIMEOUT aborted

Explanation | The Authorized Services Manager is ending due to the `TERM` command or a subtask abnormal end. The `TIMEOUT` command cannot execute in this situation.
Action | None.

## ASM0084 - Too many FSSM parameter lines.

Explanation | More than 51 parameter lines have been passed to the File Server Shared Memory (FSSM) service.
Action | Use a maximum of 51 parameter lines.

## ASM0119 - Authorized Services Manager Server settings in effect:

Explanation | This message is issued at start-up of the Authorized Services Manager. It is followed by several ASM0119 messages of varying contents, summarizing parameters in effect for this run. Selected RSM0119 messages may also be issued in response to the `TIMEOUT` command.
Action | None.

## ASM0401 - Various FSSM messages

Explanation | Various messages are issued by the File Server Shared Memory (FSSM) service of Natural for Db2.
Action | Refer to the Natural for Db2 documentation for explanations of FSSM messages.

### On this page

- ASM0001 - Subsystem id invalid
- ASM0002 - No group name: Sysplex purge propagation disabled
- ASM0003 - Unexpected return code from IEANTRT: rc
- ASM0004 - LX table could not be obtained. Reason: reasoncode
- ASM0005 - Authorized Services Manager Version vrs is active
- ASM0006 - Other than MODIFY or STOP command received
- ASM0007 - Unrecognized parameter in parm file:
- ASM0008 - Invalid value in parm file:
- ASM0009 - Invalid command: command
- ASM0010 - Bad return code from SNAP routine: rc
- ASM0011 - Subtask terminated: taskname rc
- ASM0012 - Subtask termination in progress
- ASM0013 - Coupling Facility will not be used for SIP
- ASM0014 - Invalid SIP CF structure name
- ASM0015 - Invalid number of SIP slots specified
- ASM0017 - Connected to SIP CF Structure with nnnn slots
- ASM0018 - SIP CF Structure initialized with nnnn slots
- ASM0019 - Number of SIP slots not specified: SIP service is not available
- ASM0020 - Invalid SIP slots size specified
- ASM0021 - Unexpected return code from IEANTCR: rc
- ASM0022 - Wrong ECSAD version: version
- ASM0023 - Old ECSAD with version version no longer in use
- ASM0029 - Module NATZPX loaded at address: address
- ASM0030 - Module NATFSSM loaded at address: address
- ASM0031 - Module NATNDVX loaded at address: address
- ASM0033 - No space for a PROPBLOK in Message Exit
- ASM0034 - IXCMSGI return code nnnnn reason code nnnnn
- ASM0035 - IXC Message Exit received invalid length: xxxxxxxx
- ASM0036 - IXC Message Exit received invalid message header
- ASM0039 - Module NATZPX removed at address: address
- ASM0040 - Module NATFSSM removed at address: address
- ASM0041 - Module NATNDVX removed at address: address
- ASM0045 - Applied Zaps:
- ASM0047 - Operator command: command
- ASM0048 - IARV64 GETSTOR failed. Return code: rc
- ASM0049 - Too many/few parameters for command
- ASM0052 - Not enough storage for IARV64 GETSTOR - Increase MEMLIMIT
- ASM0058 - ASM already active in subsid: Job jobname ASID asid
- ASM0066 - REBUILD Start: CF structure temporarily unavailable
- ASM0067 - REBUILD End: CF structure available again
- ASM0068 - Invalid parameter parameter
- ASM0069 - Invalid non-activity time
- ASM0070 - Invalid timeout check time
- ASM0071 - NATFSSM not linked: FSSM parameter ignored
- ASM0072 - Installation error: NATBPPRP not linked
- ASM0073 - module version date time
- ASM0074 - Thread end requested by userid ASID asid
- ASM0075 - TIMEOUT ON/NOW rejected: No valid timeout parameters
- ASM0076 - Timeout check deactivated
- ASM0077 - Specify NAT, NOW, ON, OFF,
  ASM0077 - REPEAT, TOC, TERSE, VERBOSE, or ?
- ASM0078 - Timeout processing starting
- ASM0079 - Scheduled/Operator timeout processing deleted n sessions
- ASM0080 - Timeout processing ended with return code rc
- ASM0082 - Send command TIMEOUT ON to activate timeout check
- ASM0083 - Authorized Server not in active state. TIMEOUT aborted
- ASM0084 - Too many FSSM parameter lines.
- ASM0119 - Authorized Services Manager Server settings in effect:
- ASM0401 - Various FSSM messages