SEFM* - ADASAF SAF Interface and SAF Security Kernel Messages

#### Search Results

Search

# SEFM* - ADASAF SAF Interface and SAF Security Kernel Messages

ADASAF displays an eight-byte code containing various return codes from SAF. This information is shown in a number of messages denoted ssssssss.

The ADASAF return code "ssssssss" contains the following structure:

Position | Information Content
Byte: 1 | SAF return code
Byte: 2 |
Function code. ADASAF internal function codes (hex) include:
04 | Authorize Adabas access
44 or 6C | Authenticate user
Byte: 3 | Return code from security system, for example RACF
Byte: 4 | Reason code from security system, for example RACF
Bytes: 5 - 8 | SAF reason code

Refer to the IBM manual External Security Interface (RACROUTE) Macro Reference manual for z/OS for a thorough explanation of all possible return/reason codes. CA-Top Secret and CA-ACF2 can provide different return code values in some circumstances.

The following message groups are described:

- Messages Displayed on the Operator Console and System Message Data Sets (SEFM001 - SEFM255)

- Operator Command Messages (SEFM900+ Series)

## Messages Displayed on the Operator Console and System Message Data Sets (SEFM001 - SEFM255)

The following messages are displayed on the operator console and system message datasets. The messages may be issued by the SAF Security Kernel component (in a daemon, an Adabas nucleus or an Entire Net-Work node) or by another product into which SAF Security is installed, such as Natural or Entire Broker.

### Meldungen im Überblick

`BLS0334 | SEFM001 | SEFM002 | SEFM004 | SEFM006 | SEFM008 | SEFM009 | SEFM013 | SEFM014 | SEFM015 | SEFM016 | SEFM017 | SEFM020 | SEFM021 | SEFM025 | SEFM026 | SEFM028 | SEFM029 | SEFM030 | SEFM031 | SEFM041 | SEFM049 | SEFM050 | SEFM051 | SEFM060 | SEFM061 | SEFM062 | SEFM070 | SEFM071 | SEFM072 | SEFM073 | SEFM074 | SEFM075 | SEFM205 | SEFM210 | SEFM255`

BLS0334 | SYMBOL 'NETSAF' CANNOT BE FOUND. LOADING ABORTED
Erläuterung | This message should be ignored.

SEFM001 | ssssssss : user : resource
Erläuterung | The security system determined that the user identified in the message ( user) does not have authorization for the resource listed in the message (resource). System return and reason codes are given in the hexadecimal string ssssssss. This message is displayed when access has been denied to a particular resource.

SEFM002 | *XX to request FF : user : resource
Erläuterung | An unexpected response code (XX) was received from the SAF Security Kernel for the user identified in the message (user) when requesting function FF to be performed on the resource specified in the message (resource).

SEFM004 | *Natural programs not extracted
Erläuterung | The SAF Security Kernel was not able to extract a list of protected program objects from the security system on behalf of Natural users.
Empfohlene Handlung | Obtain a trace of SAF call RACROUTE EXTRACT from the security system and contact your Software AG technical support representative. ACF2 and Top Secret users should ensure that the protected programs have been extracted from the security system and supplied to the SAF Security Kernel via the SEFEXT DD statement in the daemon started task JCL.

SEFM006 | *ADARSP XX(xx) to request FF : user
Erläuterung | The SAF Security Kernel returned the Adabas response code (XX) and subcode (xx) shown in the message to request FF for the user shown in the message (user).
Empfohlene Handlung | Ensure that the SAF Kernel started task is active. Check its output for error messages. Take the necessary remedial action indicated by the Adabas response code.

SEFM008 | *SAF Gateway (Vv.r) started * SAF Security Kernel (Vx.x.x - BUILD xxxx) started
Erläuterung | Entire Net-Work SAF Security Interface (ADASAF) startup completed or the SAF Security Kernel initialized successfully.
Empfohlene Handlung | No action is required for this informational message.

SEFM009 | Module module-name not loaded
Erläuterung | Entire Net-Work SAF Security Interface could not load the module listed in the message (module-name).
Empfohlene Handlung | Ensure that the module is in the STEPLIB and that the region size is sufficient.

SEFM013 | *Less {memory | storage} acquired than specified
Erläuterung | The SAF Security Kernel or the Entire Net-Work SAF Security Interface (ADASAF) were not able to allocate all the memory or storage required to satisfy the buffer size specified in its parameters. Operation continues.
Empfohlene Handlung | Ensure that the region size is sufficient and the parameters are appropriate.

SEFM014 | *No {memory | storage}could be acquired
Erläuterung | Entire Net-Work SAF Security Kernel or the SAF Security Interface (ADASAF) could obtain no storag or memory at system startup. Operation has terminated. Operation has terminated.
Empfohlene Handlung | Ensure that the region size is sufficient and system parameters are appropriate.

SEFM015 | *Logic error - XXXX for request FF : user
Erläuterung | The SAF Security Kernel suffered an internal error. A general restart is performed and the operation continues.
Empfohlene Handlung | Keep all information written to DDPRINT and contact your Software AG technical support representative.

SEFM016 | *SAF logoff failed ssssssss ACEE AAAA : user
Erläuterung | The SAF Security Kernel was unable to logoff user from the security system. The SAF error code is ssssssss.
Empfohlene Handlung | Contact your Software AG technical support representative.

SEFM017 | *Insufficient space to initialize - make Natural buffer XX
Erläuterung | The Natural SAF interface requires a larger value to be specidied for `NSFSIZE`.
Empfohlene Handlung | Increase the Natural `NSFSIZE` parameter.

SEFM020 | *GETMAIN failed / IDSIZE error
Erläuterung | The Natural SAF interface could not acquire storage from the designated IDMSBUF.
Empfohlene Handlung | Increase Natural region and/or thread size.

SEFM021 | *Illegal storage use / relocation problem
Erläuterung | Internal problem in Natural SAF storage use.
Empfohlene Handlung | Contact your Software AG technical support representative.

SEFM025 | *Natural IDMSBUF parameter is not defined
Erläuterung | The Natural `NSFSIZE` parameter has not been specified.
Empfohlene Handlung | Ensure `NSFSIZE` is set correctly in the Natural parameters.

SEFM026 | *Natural protected programs not extracted code: XX
Erläuterung | The list of protected programs could not be returned from the SAF Security Kernel to Natural.
Empfohlene Handlung | Ensure the same copy of the configuration module SAFCFG is used by all system components. Check that the `GWSTYP` parameter defined in SAFI010 and `STY` parameter in SAFI020 are both correctly set for the installed security system and that all installation requirements have been met.

SEFM028 | *System files not found in environment table
Erläuterung | The current Natural system files were not matched in the table defining all possible system file sets.
Empfohlene Handlung | Ensure that the environment definitions in Natural Security are correct.

SEFM029 | *Error in communications layer - check installation procedure
Erläuterung | Possible reasons for error: Adabas link module installed into this component is not reentrant.

SEFM030 | *SQL table / VIEview could not be identified for file (XX,YY)
Erläuterung | Interface could not identify table name for DBID/FNR of an SQL request.
Empfohlene Handlung | Ensure interface is correctly installed, then contact your Software AG technical support representative.

SEFM031 | *DBID / FNR identified with SQL request not recognized XXXX
Erläuterung | Interface component could not determine the DBID/FNR associated with this SQL request.
Empfohlene Handlung | Contact your Software AG technical support representative.

SEFM041 | *Interface installed for Net-work
Erläuterung | The interface is installed for operation with Entire Net-Work.
Empfohlene Handlung | No action is required for this informational message.

SEFM049 | *User type T not permitted by installed options
Erläuterung | The SAF Kernel will not permit user type T to operate using the currently installed options.

SEFM050 | *Error writing SMF record : XX
Erläuterung | The stated error occurred when an SMF record was being written.

SEFM051 | *SAFPRINT dataset not defined, DDPRINT will be used
Erläuterung | `SAFPRINT=Y` is set in SAFCFG, but no SAFPRINT dataset is defined.

SEFM060 | * RACLIST REQUESTED FOR CLASS cccccccc
Erläuterung | The specified security class cccccccc has been configured to use FASTAUTH in SAFCFG. This message indicates the start of the RACLISTing process for this class.
Empfohlene Handlung | No action is required for this informational message.

SEFM061 | * RACLIST SUCCESSFUL FOR CLASS cccccccc
Erläuterung | This message indicates RACLISTing has been successful for class cccccccc.
Empfohlene Handlung | No action is required for this informational message.

SEFM062 | * RACLIST FAILED FOR CLASS cccccccc ERROR ssssssss
Erläuterung | This message indicates RACLISTing has failed for class cccccccc. The FASTAUTH option for this class cannot be honoured, authorization checks will be performed using RACROUTE REQUEST=AUTH (the default).
Empfohlene Handlung | Refer to Adabas SAF Security > Adabas SAF Security Messages and Codes > SAF Return Codes for information on how to interpret the error code ssssssss.

SEFM070 | * LISTENER ACTIVE FOR SIGNAL ENF-xx
Erläuterung | This message indicates the signal listener has been successfully activated and is listening for ENF signal type xx.
Empfohlene Handlung | No action is required for this informational message.

SEFM071 | * UNABLE TO ACTIVATE LISTENER FOR SIGNAL ENF-xx ERROR eeeeeeee
Erläuterung | This message indicates the signal listener could not be activated for ENF signal type xx. The error code is eeeeeeee.
Empfohlene Handlung | Contact your Software AG technical support representative.

SEFM072 | * LISTENER TERMINATED FOR SIGNAL ENF-xx
Erläuterung | This message indicates the signal listener has been successfully de-activated and is no longer listening for ENF signal type xx.
Empfohlene Handlung | No action is required for this informational message.

SEFM073 | * SIGNAL LISTENERS REQUESTED BUT INCOMPATIBLE RUNTIME
Erläuterung | This message indicates that signal listeners have been requested by configuration but there is an incompatibility between the Adabas SAF Security and the Adabas Limited Library (WAL) runtimes. The job continues to run, but without any active ENF Signal listeners.
Empfohlene Handlung | Ensure Adabas SAF Security is at least version 8.4 SP1, and the Adabas Limited Library (WAL) is at least version 8.5 SP4 Patch level 1.

SEFM074 | * UNABLE TO ALLOCATE REQUIRED MEMORY FOR SIGNAL LISTENERS
Erläuterung | This message indicates a memory shortage when attempting to establish the signal listeners. The job continues to run, but without any active ENF Signal listeners.
Empfohlene Handlung | Review the `REGION` size for the job. Review the `SIGNQSZ` parameter.

SEFM075 | * UNABLE TO TERMINATE SIGNAL LISTENERS. PLEASE TRY LATER
Erläuterung | SAF daemon only. This message indicates that Adabas SAF Security in the daemon has been unable to cleanly terminate the ENF Signal listeners in response to a `SSIGTERM` command. The ENF Signal listeners are asynchronous processes that were likely busy at the time of termination.
Empfohlene Handlung | Retry the `SSIGTERM` command at a later time

SEFM205 | *CPU identity : cpuid
Erläuterung | The interface component linked to Entire Net-Work displays the CPU ID of the host machine.
Empfohlene Handlung | No action is required for this informational message.

SEFM210 | *SAF Gateway is active for Entire Net-Work
Erläuterung | The Entire Net-Work SAF Security Interface is active.
Empfohlene Handlung | No action is required for this informational message.

SEFM255 | *Unauthorized use of request
Erläuterung | Attempted illegal use of security request.
Empfohlene Handlung | Contact your Software AG technical support representative.

## Operator Command Messages (SEFM900+ Series)

The following messages are displayed in response to operator commands:

### Meldungen im Überblick

`SEFM900 | SEFM901 | SEFM902 - 905 | SEFM909 | SEFM910 | SEFM911 | SEFM913 | SEFM914 | SEFM915 | SEFM916 | SEFM918 | SEFM919 | SEFM920 | SEFM921 | SEFM922 | SEFM923 | SEFM924 | SEFM928 | SEFM929 | SEFM930 | SEFM931`

SEFM900 | * Operator issued command: command
Erläuterung | Entire Net-Work SAF Security Interface (ADASAF) or the SAF Security Kernel received the operator command identified in the message.
Empfohlene Handlung | No action is required for this informational message.

SEFM901 | * SAF server - General statistics (at hhhhhhhh) * SAF Security Kernel - General statistics (at hhhhhhhh)
Erläuterung | The operator command for general statistics was issued. Here is an example of the statistics messages produced for the SAF server:
    SEFM901 * SAF SERVER - GENERAL STATISTICS (AT hhhhhhhh)
    SEFM902 * RESOURCE    CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES LEN
    SEFM903 * APPLICATION         1          0          0           0    8
    SEFM903 * ADABAS              0          0          0           0   32
    SEFM903 * SYSMAIN             0          0          0           0   13
    SEFM903 * SYSTEM FILE         2          0          0           0   24
    SEFM903 * PROGRAM             0          0          0           0   17
    SEFM903 * BROKER              0          0          0           0   32
    SEFM903 * NET-WORK            0          0          0           0    0
    SEFM903 * SQL SERVER          0          0          0           0    0
    SEFM904 * USERS - ACTIVE: 1 FREE: 55 OVEWRITES: 0
Here is an example of the statistics messages produced for the SAF Security Kernel:. The address in the first line is the address of the SAF Kernel's storage cache.
    SEFM901 * SAF SECURITY KERNEL - SERVER STATISTICS (AT 12C47000)
    SEFM902 * RESOURCE    CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES LEN
    SEFM903 * APPLICATION        10          0          0           0    8
    SEFM903 * DBMS CHECK          0          0          0           0   17
    SEFM903 * SYSMAIN             0          0          0           0   21
    SEFM903 * SYSTEM FILE         2          0          0           0   40
    SEFM903 * PROGRAM             0          0          0           0   17
    SEFM903 * BROKER              0          0          0           0   68
    SEFM903 * NET-WORK            0          0          0           0   17
    SEFM903 * SQL SERVER          0          0          0           0   32
    SEFM904 * CACHED USERS:       1 HIGH WATERMARK:     1 MAX USERS:  5545
    SEFM905 * OVERWRITES:         0 AUTHENTICATED:      0 DENIED:        0
Empfohlene Handlung | No action is required for this informational message.

SEFM902 - 905 | statistics
Erläuterung | Various statistics for the SAF server and the SAF Security Kernel are displayed. See message SEFM901.
Empfohlene Handlung | No action is required for this informational message.

SEFM909 | * {SAF Gateway | SAF Security Kernel} - shutdown initiated
Erläuterung | The operator issued a command to shut down Entire Net-Work SAF Security Interface or the daemon started task (SAF Security Kernel). This message is also issued when a secure Adabas nucleus, Net-Work node or Adabas SQL server terminates.
Empfohlene Handlung | No action is required for this informational message.

SEFM910 | *{SAF Server | SAF Security Kernel} - list all active users
Erläuterung | The operator issued a command to display a list of currently active users. The following is a sample of the output produced for the SAF server:
    SEFM910 * SAF SERVER - LIST ALL ACTIVE USERS
    SEFM911 * USERID      CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES BUFF
    SEFM912 * K11079              3          0          0           0   0
The following is a sample of the output produced for the SAF Security Kernel:
    SEFM910 * SAF GATEWAY - LIST ALL ACTIVE USERS
    SEFM911 * USERID CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES BUFF
    SEFM912 * K11079         3          0          0           0   0
Empfohlene Handlung | No action is required for this informational message.

SEFM911 | *userid . . .
Erläuterung | The operator issued a command to display statistics specific to a currently active user. The following is a sample of the output produced for the SAF server:
    SEFM911 * NXB         CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES  BUFF
    SEFM912 * APPLICATION         1          0          0           0    0
    SEFM912 * DBMS CHECK          0          0          0           0    0
    SEFM912 * SYSMAIN             0          0          0           0    0
    SEFM912 * SYSTEM FILE         2          0          0           0    0
    SEFM912 * PROGRAM             0          0          0           0    0
    SEFM912 * BROKER              0          0          0           0    0
    SEFM912 * NET-WORK            0          0          0           0    0
    SEFM912 * SQL SERVER          0          0          0           0    0
The following is a sample of the output produced for the SAF Security Kernel:
    SEFM911 * SJU         CHECK(+VE) CHECH(-VE) CHECK SAVED OVERWRITES  BUFF
    SEFM912 * APPLICATION        10          0            0           0   10
    SEFM912 * DBMS CHECK          0          0            0           0    0
    SEFM912 * SYSMAIN             0          0            0           0    0
    SEFM912 * SYSTEM FILE         2          0            0           0    2
    SEFM912 * PROGRAM             0          0            0           0    0
    SEFM912 * BROKER              0          0            0           0    0
    SEFM912 * NET-WORK            0          0            0           0    0
    SEFM912 * SQL SERVER          0          0            0           0    0
Empfohlene Handlung | No action is required for this informational message.

SEFM913 | * No active users found in SAF {Server | Gateway | Security Kernel}
Erläuterung | No active users were found in Entire Net-Work SAF Security Interface (ADASAF) or in the SAF Security Kernel.
Empfohlene Handlung | No action is required for this informational message.

SEFM914 | * Requested user userid not found in SAF {Server | Gateway | Security Kernel}
Erläuterung | The requested user was not found in the Entire Net-Work SAF Security Interface (ADASAF) or in the SAF Security Kernel.
Empfohlene Handlung | No action is required for this informational message.

SEFM915 | SEFM915 * SAF Security Kernel - snap of server memory
Erläuterung | This message is issued in response to an `SSNAP` operator command and is followed by a sequence of SEFM916 messages.
Empfohlene Handlung | No action is required for this informational message.

SEFM916 | * hhhhhhhh hhhhhhhh hhhhhhh hhhhhhhh hhhhhhhh.x..X.Y/
Erläuterung | This message contains the results of an `SSNAP` command. Each SSNAP snaps up to 256 bytes and shows the address, the hexadecimal storage contents, and the interpretation.
Empfohlene Handlung | No action is required for this informational message.

SEFM918 | * Supplied address is outside of legal range
Erläuterung | An attempt was made to snap storage outside the bounds of the SAF Kernel's cache.

SEFM919 | *Operator command did not contain required arguments
Erläuterung | A required parameter was omitted from an operator command. For example, `SUSTAT` with no userid specified.
Empfohlene Handlung | Correct the operator command and try again.

SEFM920 | command1, command2, command3, and so on
Erläuterung | This message is issued in response to an `SHELP` operator command and lists the available SAF Kernel operator commands.
Empfohlene Handlung | No action is required. This message is informational.

SEFM921 | * Memory allocation failure - users cannot be logged off
Erläuterung | The SAF Kernel was unable to obtain temporary storage (approximately 16Kb) to log users off in response to an `SREST, SNEWCOPY` or `SLOGOFF` operator command.
Empfohlene Handlung | Increase the region size.

SEFM922 | * User userid logged off
Erläuterung | This message is issued in response to an `SLOGOFF` operator command. The indicated user has been logged off from the security system.
Empfohlene Handlung | No action is required for this informational message.

SEFM923 | * User userid not logged off - user not found
Erläuterung | This message is issued in response to an `SLOGOFF` operator command. The requested user could not be found in the SAF Kernel’s cache.
Empfohlene Handlung | Verify the correct user ID was specified.

SEFM924 | * User userid not logged off - return code ZZ
Erläuterung | This message is issued in response to an `SLOGOFF` operator command. An internal error (indicated by ZZ) occurred while attempting to log the requested user off.
Empfohlene Handlung | Evaluate the return code to determine the cause of the error.

SEFM928 | * Invalid trace setting - must be 0, 1, 2 or 3
Erläuterung | The `STRACE` operator command was issued with an invalid trace setting.
Empfohlene Handlung | Correct the trace setting and try again.

SEFM929 | * Invalid SAF Security Kernel operator command
Erläuterung | An invalid SAF Security Kernel operator command was entered.
Empfohlene Handlung | Specify a valid SAF Security Kernel operator command.

SEFM930 | * SIGNAL SREST INTERVAL COUNTS:
Erläuterung | When the ENF Signal Listener is active, this message is appended to the general statistics displayed by message SEFM901 as a result of an `SSTAT` or `SREST` command. Together with SEFM931, counts are displayed relating to the number of ENF Signal conditions which have resulted in an SREST operation being requested, since the time of the last completed SREST operation.
Empfohlene Handlung | No action is required for this informational message.

SEFM931 | * QUEUE FULL: nnnnnnnn ENF-62: nnnnnnnn * ENF-71: nnnnnnnn ENF-79: nnnnnnnn
Erläuterung | When the ENF Signal Listener is active, this message is appended to the general statistics displayed by message SEFM901 as a result of an `SSTAT` or `SREST` command. Counts are displayed relating to the number of ENF Signal conditions which have resulted in an SREST operation being requested, since the time of the last completed SREST operation. #### QUEUE FULL The number of times a free entry in the ENF Signal Listener Queue could not be found. #### ENF-nn The number of times the ENF Signal Listener was unable to identify the signal type nn as belonging to a specific user.
Empfohlene Handlung | No action is required for this informational message.

### On this page

- Messages Displayed on the Operator Console and System Message Data Sets (SEFM001 - SEFM255)
- Operator Command Messages (SEFM900+ Series)