Installation for REQUEST DOCUMENT and PARSE XML Statements on z/OS

#### Search Results

Search

# Installation for REQUEST DOCUMENT and PARSE XML Statements on z/OS

This document describes the installation steps for enabling the use of the Natural statements `REQUEST DOCUMENT` and `PARSE XML` on z/OS.

- Prerequisites

- Installation Procedure

- Support for Architecture Levels

- Installation Verification

#### Related Topics:

For information on the functions provided by `REQUEST DOCUMENT` and `PARSE XML`, see the following documents:

- Statements for Internet and XML Access in the Programming Guide

- `REQUEST DOCUMENT` in the Statements documentation

- `PARSE XML` in the Statements documentation

## Prerequisites

The following requirements must be met to execute the `REQUEST DOCUMENT` and `PARSE XML` statements:

- The ICU library must be installed to convert data from one encoding to another (at least internally). For details, see the relevant section in the Unicode and Code Page Support documentation.

- A TCP/IP stack must be available and enabled for the execution environment.

- A DNS (Domain Name System) server or DNS services must be available in the execution environment to resolve internet addresses (`gethostbyname` function).

For Internet Protocol Version 6 (IPv6) support, the following additional prerequisites apply:

- An activated IPv6 stack must be available on the local host.

- The local network must support IPv6.

- An accessible and IPv6-capable DNS server must be available.

- For IPv6 internet communication, an IPv6 connection from the service provider must be available.

- If both IPv4 and IPv6 are used, a dual stack must be supported.

- IPv6 support must be configured with the appropriate keyword subparameters of the Natural profile parameter `XML` described in the Parameter Reference documentation.

See also General Prerequisites and System Support in the section Overview of the Installation Process.

## Installation Procedure

Be sure to read Installation Process and Major Natural Features before you start the installation procedure.

The installation procedure comprises the following:

- Step 1: Link the Module NATXML or NATXMLA9 to the Nucleus

- Step 2: Enable the Environment-Dependent Nucleus for LE Execution

- Step 3: Link the Required Modules to the Nucleus

### Step 1: Link the Module NATXML or NATXMLA9 to the Nucleus

The module `NATXML` is required to execute the statements `REQUEST DOCUMENT` and `PARSE XML`. If you want the `PARSE XML` statement to support IBM architecture level 9, alternatively, you can use the module `NATXMLA9`. See also Support for Architecture Levels.

1. Set the System Maintenance Aid (SMA) parameter `NATXML` to `Y` (default is `N`).

2. The `NATXML` module is then linked to the environment-independent nucleus by using the following `INCLUDE` statement:

        INCLUDE NATLIB(NATXML)

Or:

For support of IBM architecture level 9:

1. Set the SMA parameters `NATXML` and `NAT-ARCHLEVEL9` to `Y` (default is `N`).

2. The alternative `NATXMLA9` module is then linked to the environment-independent nucleus by using the following `INCLUDE` statement:

       INCLUDE NATLIB(NATXMLA9)

### Step 2: Enable the Environment-Dependent Nucleus for LE Execution

The `REQUEST DOCUMENT` and `PARSE XML` statements require the IBM Language Environment (LE) for execution.If you want Natural to run in the IBM Language Environment (LE), perform the following steps:

1. Set the System Maintenance Aid (SMA) parameter `NAT-LE` to `Y` (Yes). The default setting is `N` (No).

2. Additionally, if you want to modify the LE options in the `NATLEOPT` source module or if you use non-Natural programs running in 24-bit mode, set the appropriate SMA parameter as described in Build the Natural-Specific IBM Language Environment Options in Installing Natural.

3. Link the environment-dependent nucleus to support LE.

This applies to all batch and TP monitor system environments except Com-plete and CICS.

### Step 3: Link the Required Modules to the Nucleus

Link the modules indicated in this section to the nucleus depending on the environment to be used.

In the following instructions, `hilev` denotes a valid high-level qualifier.

- Batch and TSO
- CICS
- Com-plete
- IMS TM

#### Batch and TSO

- Add the LE library (usually `hilev.SCEELKED`) to the `SYSLIB` definition of the link step to resolve the references to LE functions.

- Link the LE and TCP/IP access modules to the environment-dependent nucleus by using the appropriate `INCLUDE` statements:

       INCLUDE NATLIB(NAT2LE)
       INCLUDE NATOLIB(NAT2TCP)

- Do not specify the `NCAL` parameter for the link step.

#### CICS

- Add the LE library (usually `hilev.SCEELKED`) to the `SYSLIB` definition of the link step to resolve the references to LE functions.

- Add the CICS socket library (usually `hilev.SEZARNT1`, `hilev.SEZATCP` or `hilev.SEZACMTX`) to the `SYSLIB` definition of the link step to resolve the reference to the CICS socket module.

- Link the CICS socket module to the environment-dependent nucleus by using the appropriate `INCLUDE` statement:

       INCLUDE NATLIB(NAT2LE)
       INCLUDE NCIOLIB(NCI2TCP)
       INCLUDE CICSSOCK(EZACIC17)

- Do not specify the `NCAL` parameter for the link step.

- Configure the CICS TCP/IP environment as described in the IP CICS Socket Guide by IBM.

#### Com-plete

- Link the LE access module to the environment-dependent nucleus by using the appropriate `INCLUDE` statement:

       INCLUDE NATLIB(NAT2LE)

- Copy the `NCFTCPvr` module from the Natural Com-plete Interface load library to the Com-plete load library.

- For support of the IBM TCP/IP stack, define the CDI (Communication Driver Interface) as described in Standard CDI Definitions in the Com-plete documentation.

- Add the `POSIX SERVER` statement to the Com-plete parameter module `SYSPARM`.

#### IMS TM

- Add the LE library (usually `hilev.SCEELKED`) to the `SYSLIB` definition of the link job to resolve the references to LE functions.

- Link the LE and TCP/IP access modules to the environment-dependent nucleus by using the appropriate `INCLUDE` statements:

       INCLUDE NATLIB(NAT2LE)
       INCLUDE NATOLIB(NAT2TCP)

- Do not specify the `NCAL` parameter for the link step.

## Support for Architecture Levels

If your Natural system runs on z/OS with an IBM processor with architecture level 9 or higher, you can replace the module `NATXML` by `NATXMLA9`. `NATXMLA9` is built to use advanced machine instructions introduced with IBM’s ESA/390 and z/Architecture. You can use the system command `TECH`(see the System Commands documentation) to find out the architecture level supported on your current machine.

`NATXMLA9` improves execution performance, especially for the statements `REQUEST DOCUMENT` and `PARSE XML` that use Unicode variables or perform code-page encoding operations. For more information on architecture levels, refer to the related documentation from IBM (z/Architecture, Principles of Operation).

| Warnung: An operation exception error (abend code S0C1) can occur if the `NATXMLA9` module is used, but the underlying machine architecture level is lower than 9.

## Installation Verification

After the last step of the installation procedure has been completed, proceed as follows:

1. Activate the statements in the runtime environment; see Activation/Deactivation in the section Statements for Internet and XML Access in the Programming Guide.

   For information on the profile settings that enable the support of the `REQUEST DOCUMENT` and/or `PARSE XML` statement, see the following documents:

   - Profile Settings in the section Statements for Internet and XML Access in the Programming Guide

   - Profile parameter `XML` in the Parameter Reference documentation

2. Try the example programs contained in the Natural system library `SYSEXV`.

### On this page

- Prerequisites
- Installation Procedure
- Support for Architecture Levels
- Installation Verification