Natural Profile Parameters for NATSPOOL

#### Search Results

Search

# Natural Profile Parameters for NATSPOOL

This documentdescribes the profile parameters which must be defined in the Natural parameter module.

- NTPRINT Macro or PRINT Parameter

- FSPOOL Parameter

- NAFUPF Parameter

- NAFSIZE Parameter

For further information on Natural profile parameters and parameter macros, see the Natural Parameter Reference and the Natural Operations documentation.

## NTPRINT Macro or PRINT Parameter

To define the logical printers for which reports can be generated, the `NTPRINT` macro in the Natural parameter module has to be used.

Example:

    NTPRINT (1,3,6-11,15),AM=NAF

The corresponding profile parameter `PRINT` can also be used to specify the same options dynamically when starting a session.

## FSPOOL Parameter

The `FSPOOL` parameter setting determines the database identification (DBID), file number (FNR), password, and cipher key of the spool file for the Natural session.

The `FSPOOL` parameter has the following syntax:

    FSPOOL=(nnnnn,fffff,password,cipher-key)

Operand | Description
--- | ---
`nnnnn` | The database ID of the spool file.
`fffff` | The file number of the spool file.
`password` | The password required if the spool file has been password-protected using the Adabas security feature.
`cipher-key` | The cipher key required if the spool file has been ciphered using the Adabas security feature.

## NAFUPF Parameter

The `NAFUPF` parameter is used to specify the name of the user profile (1 to 8 characters) to be used when creating reports. The user profile can only be defined by using Function 31.1.

Example:

    NAFUPF=SAG00001

## NAFSIZE Parameter

The `NAFSIZE` parameter setting determines the size of work buffer used by Natural Advanced Facilities.

`NAFSIZE=0` is the default and prevents the initialization of Natural Advanced Facilities.

`NAFSIZE=1` is sufficient for operation. Greater values do not improve operation.

Set `NAFSIZE` to `1` in all environments in which Natural Advanced Facilities can be used.

### On this page

- NTPRINT Macro or PRINT Parameter
- FSPOOL Parameter
- NAFUPF Parameter
- NAFSIZE Parameter