Installing International Components for Unicode for Software AG on z/OS

#### Search Results

Search

# Installing International Components for Unicode for Software AG on z/OS

This document describes the steps for installing International Components for Unicode for Software AG (ICS) on z/OS which allows Natural to convert code pages and support Unicode.

International Components for Unicode for Software AG (ICS) requires the use of an ICS module and an ICU data library. In addition, you can use ICU data items to load ICU components that are not contained in the ICU data library. The ICS module does not have to be linked to the Natural nucleus if neither code page conversion nor Unicode support are required.

The use of ICU functionality increases the required Natural thread size.

Note
For increased flexibility, it is also possible to load the ICS module during initialization of the Natural session. A dynamically loaded ICS module overrides the statically linked ICS module. You can also load an ICU data library during initialization of the Natural session. A dynamically loaded ICU data library overrides any statically linked ICU data library.

The ICS module, the ICU data libraries and the ICU data items are explained in Enabling Unicode and Code Page Support in the Unicode and Code Page Support documentation.

#### Notation vrs or vr:

When used in this document, the notation `vrs` or `vr` represents the relevant product version (see also Version in the Glossary).

- Prerequisites

- Installation Medium

- Installation Procedure

- Installation Verification

- Using ICS32 in Natural subtask (needs APF-authorized ICS load library)

## Prerequisites

See General Prerequisites and System Support in the section Overview of the Installation Process.

## Installation Medium

The ICS module, the ICU data libraries and the ICU data items are contained on the `ICSvrs.LOAD` and `ICSvrs.SRCE` data sets supplied on the installation medium for base Natural.

## Installation Procedure

Be sure to read Installation Process and Major Natural Features before you start the installation procedure.

- Step 1: Link the ICS Module

- Step 2: Link an ICU Data Library

- Step 3: Load the ICS Module at Session Start

- Step 4: Load an ICU Data Library at Session Start

- Step 5: Load ICU Data Items on Request in a Session

### Step 1: Link the ICS Module

1. Add the following `INCLUDE` statement to the link instructions for the environment-independent nucleus:

        INCLUDE ICSLIB(SAGICU)

   For support of IBM architecture level 9, instead of `SAGICU`, you can use the alternative ICS module `SAGICUA9`:

   - Set the System Maintenance Aid (SMA) parameter `NAT-ARCHLEVEL9` to `Y` (default is `N`).

     Or:

   - Add the following `INCLUDE` statement to the link instructions for the environment-independent nucleus:

          INCLUDE ICSLIB(SAGICUA9)

   - See also alternative ICS modules in the Unicode and Code Page Support documentation.

   Note
   The ICU data library `ICSDT58J` is contained in the ICS module `SAGICU` (or `SAGICUA9` respectively) and available by default.

2. Link the ICS module to the environment-independent nucleus as described in Link the Nucleus in Installing Natural.

### Step 2: Link an ICU Data Library

Data libraries provided by Software AG are not supported with ICS 321. They will still be supported as part of the ICS Transition Version 222 .

ICS 321 uses the entirety of ICU localization data as described in Step. 5.

This step is only required if you want to use another data library in addition to `ICSDT58J`.

1. Add one of the following `INCLUDE` statements to the link instructions for the environment-independent nucleus depending on the ICU data library to be used:

        INCLUDE ICSLIB(ICSDT58E)

   Or:

        INCLUDE ICSLIB(ICSDT58X)

2. Link the ICU data library to the environment-independent nucleus as described in Link the Nucleus in Installing Natural.

   If you link the `ICSDT58X` data library, link the environment-independent nucleus into a PDSE instead of a PDS to avoid IBM error IEW2641S.

### Step 3: Load the ICS Module at Session Start

1. Make sure that the ICS load library from the `ICSvrs.LOAD` data set is available to the execution JCL of your Natural or TP monitor interface. Depending on your environment, perform one of the following options:

   - In batch mode, under TSO and in all IMS TM environments:

     Add `ICSvrs.LOAD` to the `STEPLIB` concatenation of your execution JCL.

   - Under CICS:

     Add `ICSvrs.LOAD` to the `DFHRPL` concatenation of your CICS execution JCL.

   - Under Com-plete:

     Add `ICSvrs.LOAD` to the `COMPLIB` concatenation of your Com-plete execution JCL.

2. At the start of a Natural session, set the Natural profile parameter `RCA` as follows:

       RCA=SAGICU

   `RCA` is described in the Parameter Reference documentation.

   The ICS module `SAGICU` is described in the Unicode and Code Page Support documentation.

   Instead of the ICS module `SAGICU`, you can also load the ICS module `SAGICUA9`. In addition to `SAGICU`, this module supports IBM architecture level 9: see alternative ICS modules in the Unicode and Code Page Support documentation.

   If you want to load `SAGICUA9`, use the following parameter setting:

       RCA=SAGICU RCALIAS=(SAGICU,SAGICUA9)

   The Natural profile parameter `RCALIAS` is described in the Parameter Reference documentation.

### Step 4: Load an ICU Data Library at Session Start

Data libraries provided by Software AG are not supported with ICS 321. They will still be supported as part of the ICS Transition Version 222 .

ICS 321 uses the entirety of ICU localization data as described in Step. 5.

1. Make sure that the ICS load library from the `ICSvrs.LOAD` data set is available to the execution JCL of your Natural or TP monitor interface. Depending on your environment, perform one of the following options:

   - In batch mode, under TSO and in all IMS TM environments:

     Add `ICSvrs.LOAD` to the `STEPLIB` concatenation of your execution JCL.

   - Under CICS:

     Add `ICSvrs.LOAD` to the `DFHRPL` concatenation of your CICS execution JCL.

   - Under Com-plete:

     Add `ICSvrs.LOAD` to the `COMPLIB` concatenation of your Com-plete execution JCL.

2. At the start of a Natural session, set the Natural profile parameters `RCA` and `CFICU` for the ICU data library to be used:

   For `ICSDT58E`:

       RCA=ICSDT58E  CFICU=(DATFILE=ICSDT58E)

   For `ICSDT58X`:

       RCA=ICSDT58X  CFICU=(DATFILE=ICSDT58X)

   `RCA` and `CFICU` are described in the Parameter Reference documentation.

### Step 5: Load ICU Data Items on Request in a Session

This step depends on the ICS version.

- For ICS Transition Version 222
- For ICS 321

#### For ICS Transition Version 222

This step is optional and only required if you want to dynamically load an ICU data item on request during a Natural session instead of an entire ICU data library. For more information, see the Unicode and Code Page Support documentation.

1. Make sure that the ICS load library from the `ICSvrs.LOAD` data set is available to the execution JCL of your Natural or TP monitor interface. Depending on your environment, perform one of the following options:

   - In batch mode, under TSO and in all IMS TM environments:

     Add >`ICSvrs.LOAD` to the `STEPLIB` concatenation of your execution JCL.

   - Under CICS:

     Add `ICSvrs.LOAD` to the `DFHRPL` concatenation of your CICS execution JCL.

   - Under Com-plete:

     Add `ICSvrs.LOAD` to the `COMPLIB` concatenation of your Com-plete execution JCL.

2. Depending on your TP environment and the setting of the Natural `CFICU` profile parameter, perform one of the following options:

   - Under CICS, with `CFICU=(DATITEM=NONE)` set:

     Add one PPT entry for each ICU data item.

     See also the corresponding step in Installing Natural CICS Interface.

   - Under Com-plete, with `CFICU=(DATITEM=NONE)` set:

     Add `THREAD-ESQA-SIZE=15K` as a keyword parameter to the startup options for your Com-plete.

#### For ICS 321

1. You can specify the name of the dataset containing the ICU data items from ICSvrs.LOAD dynamically at the start of the session using the CFICU STEPLIB parameter .

   - See section Data Scope and Data Handling in Unicode and Code Page Support

   - Add the load library containing the data items to the execution JCL of your Natural or TP monitor interface as described in Step 2.

2. You can also statically add the load library containing the data items from the `ICSvrs.LOAD` data set to the execution JCL of your Natural or TP monitor interface.

   - In batch mode, under TSO and in all IMS TM environments:

     Add `ICSvrs.LOAD` to the STEPLIB concatenation of your execution JCL.

   - Under CICS:

     Add `ICSvrs.LOAD` to the DFHRPL concatenation of your CICS execution JCL.

   - Under Com-plete:

     Add `ICSvrs.LOAD` to the COMPLIB concatenation of your Com-plete execution JCL.

   ICS uses both allocation methods to search for data items, starting (if given) from the CFICU STEPLIB dataset and the statically specified Natural Steplibs in the JCL.

## Installation Verification

After the last step of the installation procedure has been completed, proceed as follows:

1. Configure and activate your Unicode and code page environment by following the instructions in Configuration and Administration of the Unicode/Code Page Environment and Profile Parameters and Macros in the Unicode and Code Page Support documentation.

   For information on the code pages and ICU data files available in your current Natural environment, you can use the SYSCP utility (described in the Utilities documentation).

2. After successful activation, you can execute the example programs described in the Unicode and Code Page Support documentation.

## Using ICS32 in Natural subtask (needs APF-authorized ICS load library)

Under the current implementation of NPR, the `PRD.ICSnnn.MVSLOAD` must always be APF-authorized. This is independent of whether it is part of the STEPLIB concatenation or specified with the STEPLIB parameter of CFICU.

The scenarios for using ICS32 in a Natural subtask are:

- When running multiple Natural sessions / subtasks from an Entire System Server (NPR) node.

- When NOP, NOM, EOR are automated to be run by an ESS/NPR node.

- When running an NDV server.

### On this page

- Prerequisites
- Installation Medium
- Installation Procedure
- Installation Verification
- Using ICS32 in Natural subtask (needs APF-authorized ICS load library)