NAFSIZE - Size of Buffer for Natural Advanced Facilities

#### Search Results

Search

# NAFSIZE - Size of Buffer for Natural Advanced Facilities

This Natural profile parameter specifies the size of the work buffer used by Natural Advanced Facilities.

Possible settings | `1 - 64` | Buffer size in KB.
`0` | `NAFSIZE=0` disables Natural Advanced Facilities.
Default setting | `0` |
Dynamic specification | yes |
Specification within session | no |

Notes:

1. This Natural profile parameter only applies if Natural Advanced Facilities is installed.
2. Alternatively, you can use the equivalent Natural profile parameter `DS` or macro `NTDS` to specify the size of the buffer.
3. If Natural Advanced Facilities is to be used, a setting has to be specified for this parameter; see NATSPOOL Initialization and further information on the `NAFSIZE` parameter in Natural Profile Parameters for NATSPOOL in the Natural Advanced Facilities documentation.
4. If the requested space is not available, Natural Advanced Facilities cannot be used.