Message Buffer Pool Messages

#### Search Results

Search

# Message Buffer Pool Messages

This section contains the messages that may be issued by the message buffer pool.

For information on this buffer pool, see Message Buffer Pool in the section Operationsof the documentation of Natural .

## MTBP001 - Work buffer could not be obtained

Explanation | Work buffer could not be obtained.
Action | Check if there is memory saturation on your system.

## MTBP002 - Bad return code from IEANTRT: xxxx

Explanation | Bad return code from IEANTRT: xxxx.
Action | Contact Software AG Support.

## MTBP003 - Bad return code from IEANTCR: xxxx

Explanation | Bad return code from IEANTCR: xxxx.
Action | Contact Software AG Support.

## MTBP004 - Allocation of an ECSA directory segment failed: xxxx

Explanation | Allocation of an ECSA directory segment failed: xxxx.
Action | Contact Software AG Support.

## MTBP005 - A recursive abend occurred. Now waiting for CANCEL cmd.

Explanation | A recursive abend occurred. Now waiting for CANCEL command.
Action | Contact Software AG Support.

## MTBP006 - Message BP handler is active

Explanation | A Message Buffer Pool handler can only be started once for the same subsystem ID.
Action | None.

## MTBP007 - Other than MODIFY or STOP command received

Explanation | The received command is different from MODIFY or STOP.
Action | Use only MODIFY or STOP TSO commands. No other TSO commands are allowed.

## MTBP008 - Received command: xxxx

Explanation | This is the command that has been issued.
Action | None.

## MTBP009 - Invalid command, nothing specified

Explanation | Invalid command, nothing specified.
Action | Specify a valid command.

## MTBP010 - Negative command/keyword length encountered

Explanation | Negative command/keyword length encountered.
Action | Contact Software AG Support.

## MTBP011 - Invalid command: xxxx

Explanation | The issued command is unkown or not allowed.
Action | Specify a valid command.

## MTBP012 - More than one command: xxxx

Explanation | More than one command: xxxx.
Action | Contact Software AG Support.

## MTBP013 - Invalid parameter keyword: xxxx

Explanation | Invalid parameter keyword: xxxx.
Action | Specify valid parameter keyword(s).

## MTBP014 - Invalid BPNAME specified

Explanation | The syntax of the buffer pool name is not correct.
Action | Check the syntax of the buffer pool name.

## MTBP015 - Invalid SUBSID specified

Explanation | The syntax of the subsystem-ID is not correct.
Action | Check the syntax of the subsystem-ID.

## MTBP016 - Invalid SIZE specified

Explanation | Invalid SIZE specified.
Action | Specify the size of the message buffer pool as an integer value in the correct range.

## MTBP017 - Buffer pool is already allocated: xxxx

Explanation | The specified buffer pool name is already active. You cannot have more than one job for a given buffer pool.
Action | None.

## MTBP018 - Allocation of IDT segment failed: xxxx

Explanation | Allocation of IDT segment failed: xxxx.
Action | Contact Software AG Support.

## MTBP019 - DSPSERV CREATE failed with reason: xxxx

Explanation | DSPSERV CREATE failed with reason: xxxx.
Action | Contact Software AG Support.

## MTBP020 - ALESERV ADD failed with return code: xxxx

Explanation | ALESERV ADD failed with return code: xxxx.
Action | Contact Software AG Support.

## MTBP021 - Subsystem not active: xxxx

Explanation | Message Buffer pool must be started after NATASMvr and/or NATRSMvr.
Action | Start NATASMvr and/or NATRSMvr before starting NATMBPvr.

## MTBP022 - Buffer pool not active: xxxx

Explanation | Buffer pool not active: xxxx.
Action | Contact Software AG Support.

## MTBP023 - ALESERV DELETE failed with return code: xxxx

Explanation | ALESERV DELETE failed with return code: xxxx.
Action | Contact Software AG Support.

## MTBP024 - DSPSERV DELETE failed with reason code: xxxx

Explanation | DSPSERV DELETE failed with reason code: xxxx.
Action | Contact Software AG Support.

## MTBP025 - Message BP is deactivated now: xxxx

Explanation | This is an information message.
Action | None.

## MTBP026 - Message BP is active now: xxxx

Explanation | This is an information message.
Action | None.

## MTBP027 - Buffer pool table is full.

Explanation | Buffer pool table is full.
Action | Contact Software AG Support.

## MTBP028 - Other than MODIFY or STOP command received

Explanation | The received command is different from MODIFY or STOP.
Action | Use only MODIFY or STOP TSO commands. No other TSO commands are allowed.

## MTBP029 - Allocation of LX memory failed: xxxx

Explanation | Allocation of LX memory failed: xxxx.
Action | Contact Software AG Support.

## MTBP030 - DDNAME missing for input file: xxxx

Explanation | DDNAME missing for input file: xxxx.
Action | Make sure a dataset with the given DDNAME is specified in the JCL.

## MTBP031 - DDNAME not specified or invalid

Explanation | The syntax of the DDNAME is invalid, or no DDNAME is specified at all.
Action | Check the syntax of DDNAME.

## MTBP032 - OPEN for command input file failed: xxxx

Explanation | OPEN for command input file failed: xxxx.
Action | Check the access level of the specified dataset.

## MTBP033 - No Zaps are applied

Explanation | No Zaps are applied.
Action | Contact Software AG Support.

## MTBP034 - DD statement for SNAP missing: xxxx

Explanation | DD statement for SNAP missing: xxxx.
Action | Make sure that there is a DDNAME for a SNAP dump.

## MTBP035 - OPEN for SNAP failed: xxxx

Explanation | OPEN for SNAP failed: xxxx.
Action | Conact Software AG Support.

## MTBP036 - DDNAME too long.

Explanation | A DDNAME must have a length between 1 and 8 characters.
Action | Check the length of the DDNAME.

## MTBP037 - Invalid value specified for AREA

Explanation | Invalid value specified for AREA.
Action | Specify a valid value for AREA (ALL|HT|TEXT|CB|COMM).

## MTBP038 - Invalid BPLIST specified

Explanation | Invalid BPLIST specified.
Action | Specify a name with a length between 1 and 8 characters.

## MTBP039 - Buffer pool poolname owned by other task

Explanation | There is a sharing conflict with the buffer pool.
Action | Check if another active configuration is using the same pool name.

## MTBP040 - Startup parameter: parameter

Explanation | The startup parameters are echoed to JESMSGLG.
Action | None.

## MTBP041 - Operator command: command

Explanation | The Message Buffer Pool Server echoes operator commands to JESMSGLG.
Action | None.

## MTBP042 - OPEN command file: filename

Explanation | The name of the command file is echoed to JESMSGLG.
Action | None.

## MTBP043 - CLOSE command file: filename

Explanation | The name of the command file is echoed to JESMSGLG.
Action | None.

## MTBP044 - Wrong ECSAD version: version

Explanation | The Message Buffer Pool Server is started while there is still an ECSA-Directory present for another version of the Message Buffer Pool Server for this subsystem-ID.
Action | Rename the subsystem-ID, IPL the system, or start NATASMvr with option `ECSADUPD`.

## MTBP045 - Dataspace created: dataspace name, token, ALET, TaskId

Explanation | Diagnostic message for Software AG Support.
Action | Report the `SYSOUT` containing this message to Software AG Support when requested.

### On this page

- MTBP001 - Work buffer could not be obtained
- MTBP002 - Bad return code from IEANTRT: xxxx
- MTBP003 - Bad return code from IEANTCR: xxxx
- MTBP004 - Allocation of an ECSA directory segment failed: xxxx
- MTBP005 - A recursive abend occurred. Now waiting for CANCEL cmd.
- MTBP006 - Message BP handler is active
- MTBP007 - Other than MODIFY or STOP command received
- MTBP008 - Received command: xxxx
- MTBP009 - Invalid command, nothing specified
- MTBP010 - Negative command/keyword length encountered
- MTBP011 - Invalid command: xxxx
- MTBP012 - More than one command: xxxx
- MTBP013 - Invalid parameter keyword: xxxx
- MTBP014 - Invalid BPNAME specified
- MTBP015 - Invalid SUBSID specified
- MTBP016 - Invalid SIZE specified
- MTBP017 - Buffer pool is already allocated: xxxx
- MTBP018 - Allocation of IDT segment failed: xxxx
- MTBP019 - DSPSERV CREATE failed with reason: xxxx
- MTBP020 - ALESERV ADD failed with return code: xxxx
- MTBP021 - Subsystem not active: xxxx
- MTBP022 - Buffer pool not active: xxxx
- MTBP023 - ALESERV DELETE failed with return code: xxxx
- MTBP024 - DSPSERV DELETE failed with reason code: xxxx
- MTBP025 - Message BP is deactivated now: xxxx
- MTBP026 - Message BP is active now: xxxx
- MTBP027 - Buffer pool table is full.
- MTBP028 - Other than MODIFY or STOP command received
- MTBP029 - Allocation of LX memory failed: xxxx
- MTBP030 - DDNAME missing for input file: xxxx
- MTBP031 - DDNAME not specified or invalid
- MTBP032 - OPEN for command input file failed: xxxx
- MTBP033 - No Zaps are applied
- MTBP034 - DD statement for SNAP missing: xxxx
- MTBP035 - OPEN for SNAP failed: xxxx
- MTBP036 - DDNAME too long.
- MTBP037 - Invalid value specified for AREA
- MTBP038 - Invalid BPLIST specified
- MTBP039 - Buffer pool poolname owned by other task
- MTBP040 - Startup parameter: parameter
- MTBP041 - Operator command: command
- MTBP042 - OPEN command file: filename
- MTBP043 - CLOSE command file: filename
- MTBP044 - Wrong ECSAD version: version
- MTBP045 - Dataspace created: dataspace name, token, ALET, TaskId